Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0155	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	08/04/97	Elevation:	1289 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6049535 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	606297  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Sgg	Substrate Material:	Granodiorite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	No Data
	Slope:	2 % 	Aspect:	45 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Brown Dermosol Thin Non-gravelly Silty 	Principal Profile Form:	Um6.32
	Clayey Very deep
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	O1	0 - 0.02 m	Organic Layer; ; 
	A1	0.02 - 0.11 m	 (7.5YR2.5/2-Moist); ; Silty clay loam; Moderate grade of structure, 5-10 mm, Polyhedral; 2-5 mm,
	 Polyhedral; Smooth-ped fabric; Dry; Weak consistence; Few cutans, <10% of ped faces or 
	walls coated, distinct; Field pH 4.5 (Raupach); Common, very fine (0-1mm) roots; Common, fine 
	(1-2mm) roots; Clear change to - 
	B21	0.11 - 0.3 m	Dark brown (7.5YR3/4-Moist); ; Silty clay loam; Moderate grade of structure, 5-10 mm, 
	Polyhedral; 2-5 mm, Polyhedral; Smooth-ped fabric; Dry; Firm consistence; Common cutans, 
	10-50% of ped faces or walls coated, distinct; Field pH 4 (Raupach); Common, very fine (0-
	1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) roots; Gradual change to - 
	B22	0.3 - 0.48 m	Strong brown (7.5YR4/6-Moist); ; Silty clay; Moderate grade of structure, 5-10 mm, Subangular 
	blocky; 2-5 mm, Polyhedral; Smooth-ped fabric; Dry; Firm consistence; Common cutans, 10-
	50% of ped faces or walls coated, distinct; Field pH 4 (Raupach); Few, very fine (0-1mm) roots; 
	Gradual change to - 
	B3	0.48 - 0.95 m	Yellowish brown (10YR5/6-Moist); ; Silty clay loam; Weak grade of structure, 10-20 mm, Angular
	 blocky; Earthy fabric; Moderately moist; Firm consistence; 2-10%, fine gravelly, 2-6mm, 
	subangular, Quartz, coarse fragments; Field pH 4 (Raupach); Few, very fine (0-1mm) roots; Clear
	 change to - 
	C1	0.95 - 1.47 m	Light brownish grey (2.5Y6/3-Moist); ; Coarse sandy loam; Massive grade of structure; Sandy 
	(grains prominent) fabric; Weak consistence; Field pH 4 (Raupach); Gradual change to - 
	C2	1.47 - 2.52 m	Pale yellow (2.5Y7/3-Moist); Substrate influence, 2.5Y76, 10-20% , Faint; Substrate influence, 
	2.5Y2.51, 2-10% , Distinct; Loamy coarse sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Weak consistence; 2-10%, coarse gravelly, 20-60mm, subrounded platy, 
	Granodiorite, coarse fragments; Field pH 5 (Raupach); 
	Morphological Notes
	C1	Clear change to  weathering granodiorite - pale.                                                                  
	                                                                                      
	C2	Weathering granodiorite, feldspar and  Fe-Mn minerals. Banding of Ferro-Manganesium 
	minerals.
	Observation Notes

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0155	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site is 50m north of Bulongra rd, 1km east of BM154.
	Site Notes
	BULONGA RD, 1KM EAST OF BM154         

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0155	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02
	0.02 - 0.11	4.15C	0.58H	0.56	0.58	0	6.51J	8.23E
	0K
	0.11 - 0.3	4.06C	0.46H	0.51	0.44	0	6.16J	7.58E
	0K
	0.3 - 0.48	3.99C	0.47H	0.58	0.38	0	5.93J	7.36E
	0K
	0.48 - 0.95	3.94C	0.05H	0.34	0.16	0	4.88J	5.43E
	0K
	0.95 - 1.47	4.08C	0.07H	0.1	0.12	0.02	1.16J	1.46E
	0K
	1.47 - 2.52	4.16C	0.06H	0.1	0.05	0	0.77J	0.98E
	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02
	0.02 - 0.11	4.79B	1009.4B	0.27A	0.91	8.44
	0.11 - 0.3	1.84B	724B	0.12A	1.07	6.21
	0.3 - 0.48	0.77B	463.4B	0.07A	1.01	4.26
	0.48 - 0.95	0.19B	333.1B	0.02A	1.47	6.17
	0.95 - 1.47	0.07B	396.2B	0.01A	7.81
	1.47 - 2.52	0.04B	257.3B	0A	12.69
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02
	0.02 - 0.11
	0.11 - 0.3
	0.3 - 0.48
	0.48 - 0.95
	0.95 - 1.47
	1.47 - 2.52

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0155	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3