Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0164	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	05/05/97	Elevation:	1279 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6034044 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	617052  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Od	Substrate Material:	Schist 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	27 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Red Kandosol Medium Slightly gravelly 	Principal Profile Form:	Gn2.11
	Clay-loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	O1	0 - 0.03 m	Organic Layer; ; 
	A1	0.03 - 0.13 m	Dark reddish brown (5YR2.5/2-Moist); Biological mixing, 7.5YR33, 10-20% , Faint; Clay loam; 
	Strong grade of structure, 2-5 mm, Polyhedral; 5-10 mm, Polyhedral; Rough-ped fabric; 
	Moderately moist; Firm consistence; 2-10%, fine gravelly, 2-6mm, subangular tabular, coarse 
	fragments; Field pH 5.5 (Raupach); Many, very fine (0-1mm) roots; Common, fine (1-2mm) roots; 
	Few, medium (2-5mm) roots; Clear, Wavy change to - 
	A3	0.13 - 0.21 m	 (7.5YR2.5/3-Moist); Biological mixing, 5YR2.52, 20-50% , Faint; Clay loam; Strong grade of 
	structure, 5-10 mm, Polyhedral; 2-5 mm, Polyhedral; Rough-ped fabric; Dry; Firm consistence; 2-
	10%, fine gravelly, 2-6mm, subangular tabular, coarse fragments; Field pH 6 (Raupach); 
	Common, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) roots; Few, 
	coarse (>5mm) roots; Clear, Irregular change to - 
	B1	0.21 - 0.43 m	Dark reddish brown (5YR3/4-Moist); Biological mixing, 5YR2.52, 10-20% , Faint; Silty clay loam; 
	Strong grade of structure, 5-10 mm, Polyhedral; 2-5 mm, Polyhedral; Smooth-ped fabric; Dry; 
	Firm consistence; 2-10%, fine gravelly, 2-6mm, angular tabular, Coal, coarse fragments; Few 
	cutans, <10% of ped faces or walls coated, faint; Field pH 5.5 (Raupach); Few, very fine (0-
	1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) roots; Gradual, Irregular change to - 
	B21	0.43 - 0.98 m	Red (2.5YR4/6-Moist); Mottles, 10YR66, 2-10% , Faint; Silty clay; Moderate grade of structure, 
	10-20 mm, Subangular blocky; 5-10 mm, Polyhedral; Smooth-ped fabric; Moderately moist; Firm 
	consistence; 0-2%, fine gravelly, 2-6mm, angular tabular, Coal, coarse fragments; 2-10%, 
	coarse gravelly, 20-60mm, subangular, coarse fragments; Few cutans, <10% of ped faces or 
	walls coated, faint; Field pH 5.5 (Raupach); Few, very fine (0-1mm) roots; Diffuse change to - 
	B22	0.98 - 1.53 m	Red (2.5YR4/6-Moist); Mottles, 7.5YR68, 2-10% , Distinct; Silty clay; Massive grade of structure; 
	Earthy fabric; Moderately moist; Weak consistence; 0-2%, coarse gravelly, 20-60mm, 
	subangular, coarse fragments; Field pH 5 (Raupach); Diffuse change to - 
	B23	1.53 - 2.73 m	Dark red (2.5YR3/6-Moist); ; Silty clay; Massive grade of structure; Earthy fabric; Moderately 
	moist; Weak consistence; 10-20%, fine gravelly, 2-6mm, subangular tabular, coarse fragments; 
	Field pH 5 (Raupach); Diffuse change to - 

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0164	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	B3	2.73 - 3.03 m	Red (2.5YR4/6-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Moderately moist; 
	Weak consistence; 10-20%, fine gravelly, 2-6mm, subangular tabular, coarse fragments; Field 
	pH 4.5 (Raupach); 
	Morphological Notes
	A1	Numerous fungal mats.                                                                                                        
	                                                                           
	A3	Numerous fungal mats.                                                                                                        
	                                                                           
	B21	Several infilled root channels produce  variable bulk density. Yellow patches are 
	possibly highly weathered colluvial gravel.
	B22	Yellow patches are possibly highly weathered colluvial gravel.
	B23	Recurring bands of fine sedimentary gravel.
	B3	Colour and texture would indicate this layer still a B2 horizon
	Observation Notes
	First of 2 growth plots in the older age class along Stan's Trail.                                                                                                       
	                               
	Site Notes
	STAN'S TRAIL OLD AGE CLASS PLOT 1     

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0164	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03
	0.03 - 0.13	4.19C	2.43H	1.38	1.37	0	6.63J	11.81E
	0K
	0.13 - 0.21	4.19C	1.36H	1.1	1.01	0.01	6.4J	9.87E
	0K
	0.21 - 0.43	4.37C	1.38H	1.98	0.95	0.03	3.44J	7.77E
	0K
	0.43 - 0.98	4.38C	0.06H	0.65	0.71	0.01	4.61J	6.03E
	0K
	0.98 - 1.53	4.09C	0.05H	0.4	0.72	0	5.84J	7.02E
	0K
	1.53 - 2.73	4.02C	0.03H	0.15	0.4	0	4.87J	5.46E
	0K
	2.73 - 3.03	3.96C	0.09H	0.08	0.25	0.03	4.23J	4.68E
	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03
	0.03 - 0.13	8.41B	437.9B	0.31A	0.64	6.29
	0.13 - 0.21	5.44B	383.9B	0.23A	0.95	7.42
	0.21 - 0.43	2.63B	322B	0.13A	1.09	4.5
	0.43 - 0.98	0.78B	268B	0.05A	1.11	0.51
	0.98 - 1.53	0.67B	266.6B	0.04A	3.14
	1.53 - 2.73	0.23B	269.6B	0.03A	2.66
	2.73 - 3.03	0.14B	278.9B	0.02A	2.67
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.13
	0.13 - 0.21
	0.21 - 0.43
	0.43 - 0.98
	0.98 - 1.53
	1.53 - 2.73
	2.73 - 3.03

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0164	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P10_S_0.48	0.48 micron (cumulative %) - Sedigraph
	P10_S_1	1 micron (cumulative %) - Sedigraph
	P10_S_1000	1000 micron (cumulative %) - Sedigraph
	P10_S_125	125 micron (cumulative %) - Sedigraph
	P10_S_15.6	15.6 micron (cumulative %) - Sedigraph
	P10_S_2	2 micron (cumulative %) - Sedigraph
	P10_S_20	20 micron (cumulative %) - Sedigraph
	P10_S_2000	2000 micron (cumulative %) - Sedigraph
	P10_S_250	250 micron (cumlative %) - Sedigraph
	P10_S_3.9	3.9 micron (cumulative %) - Sedigraph
	P10_S_31.2	31.2 micron (cumulative %) - Sedigraph
	P10_S_500	500 micron (cumulative %) - Sedigraph
	P10_S_53	53 micron (cumulative %) - Sedigraph
	P10_S_63	63 micron (cumulative %) - Sedigraph
	P10_S_7.8	7.8 micron (cumulative %) - Sedigraph
	P3A1	Bulk density - g/cm3