Project Name:	CAN
	Project Code:	CAN	Site ID:	C615	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	J.R. Sleeman	Locality:	Csiro Farm Ginninderra
	Date Desc.:	05/07/66	Elevation:	 650 metres
	Map Ref.:	Sheet No. : 8727   1:100000	Rainfall:	580
	Northing/Long.:	149.066666666667	Runoff:	Moderately rapid
	Easting/Lat.:	-35.2	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Non-porous, dense, Quartz porphyry 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Moderately inclined
	Slope:	5 % 	Aspect:	165 degrees
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Mesotrophic Brown Chromosol     	Principal Profile Form:	Dr3.21
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	All necessary analytical data are available.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:	Low Strata - Sod grass, , Mid-dense. *Species includes - None recorded
	Tall Strata - Tree, , Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	0 - 0.02 m	Brown (10YR4/3-Moist); Brown (10YR5/3-Dry); ; Loamy sand; Massive grade of structure; Weak 
	consistence; Field pH 6 (pH meter); ManyAbrupt change to - 
	0.02 - 0.1 m	Brown (7.5YR4/3-Moist); Pale brown (10YR6/3-Dry); ; Loamy sand; Massive grade of structure; 
	Weak consistence; Field pH 5.5 (pH meter); ManyAbrupt change to - 
	0.1 - 0.2 m	Brown (7.5YR5/4-Moist); Pink (7.5YR7/4-Dry); ; Loamy sand; Massive grade of structure; Weak 
	consistence; 0-2%, fine gravelly, 2-6mm, dispersed, Gravel, coarse fragments; Field pH 5.9 (pH 
	meter); CommonClear change to - 
	0.2 - 0.25 m	Reddish yellow (7.5YR6/5-Moist); Pinkish grey (7.5YR7/3-Dry); ; Loamy sand; Massive grade of 
	structure; Weak consistence; 0-2%, fine gravelly, 2-6mm, dispersed, Gravel, coarse fragments; 
	Field pH 6.1 (pH meter); FewClear change to - 
	0.25 - 0.3 m	Reddish yellow (7.5YR6/5-Moist); , 5YR56; , 7.5YR74; Sand; Massive grade of structure; Weak 
	consistence; 0-2%, fine gravelly, 2-6mm, dispersed, Gravel, coarse fragments; Very few (0 - 2 
	%), Ferruginous, Medium (2 -6 mm), Nodules; Field pH 6.2 (pH meter); 
	0.3 - 0.35 m	Reddish yellow (7.5YR6/5-Moist); , 5YR56; , 7.5YR74; Sand; Massive grade of structure; Weak 
	consistence; 0-2%, fine gravelly, 2-6mm, dispersed, Gravel, coarse fragments; Very few (0 - 2 
	%), Ferruginous, Medium (2 -6 mm), Nodules; Field pH 6.3 (pH meter); Abrupt change to - 
	0.35 - 0.41 m	Reddish yellow (7.5YR6/5-Moist); , 5YR56, 2-10% ; , 7.5YR74, 2-10% ; Sandy light clay; Massive
	 grade of structure; Firm consistence; 2-10%, fine gravelly, 2-6mm, dispersed, Gravel, coarse 
	fragments; Field pH 6.2 (pH meter); Clear change to - 
	0.41 - 0.5 m	Red (2.5YR4/6-Moist); Brown (7.5YR5/4-Dry); , 2.5YR56, 2-10% ; , 2-10% ; Medium heavy clay; 
	Weak grade of structure, 2-5 mm, Subangular blocky; Firm consistence; 10-20%, fine gravelly, 2-
	6mm, dispersed, Gravel, coarse fragments; Field pH 6.3 (pH meter); Clear change to - 
	0.5 - 0.6 m	Red (2.5YR4/6-Moist); Red (2.5YR4/6-Dry); , 10R36, 2-10% ; , 2-10% ; Medium heavy clay; 
	Moderate grade of structure, 10-20 mm, Angular blocky; Very firm consistence; Field pH 6.3 (pH 
	meter); Clear change to - 

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C615	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	0.6 - 0.72 m	Red (2.5YR4/6-Moist); Red (2.5YR4/6-Dry); , 10R36, 2-10% ; , 2.5Y63, 2-10% ; Medium heavy 
	clay; Moderate grade of structure, 10-20 mm, Angular blocky; Very firm consistence; Field pH 
	6.2 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	GINNINDERRA

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C615	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02	6A	 0.15A	 4.6K	 0.78	 1.1	 0	 12.2J	0.00
	0.02 - 0.1	5.5A	 0.03A	 1.1K	 1	 0.49	 0	 5.4J	0.00
	0.1 - 0.2	5.9A	 0.03A	 1K	 0.86	 0.26	 0	 5.7J	0.00
	0.2 - 0.25	6.1A	 0.03A	 1.4K	 0	 0.21	 0	 5.6J	0.00
	0.25 - 0.3	6.2A	 0.03A	 1.2K	 0.18	 0.18	 0.02	 6.4J	0.31
	0.3 - 0.35	6.3A	 0.03A	 1.4K	 0.21	 0.18	 0	 6.3J	0.00
	0.35 - 0.41	6.2A	 0.03A	 2.2K	 0.56	 0.26	 0	 7.5J	0.00
	0.41 - 0.5	6.3A	 0.06A	 4K	 1.4	 0.36	 0	 10.3J	0.00
	0.5 - 0.6	6.3A	 0.03A	 7K	 3.1	 0.5	 0.04	 14.7J	0.27
	0.6 - 0.72	6.2A	 0.03A	 9.5K	 4.6	 0.58	 0.08	 20.7J	0.39
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02	 3.4F	 38A	 0.25B	1.50	 0	 28D	 48	 12	 11
	0.02 - 0.1	 0.81F	 5A	 0.073B	 8	 23D	 57	 11	 8
	0.1 - 0.2	 0.33F	 2A	 0.031B	 18	 25D	 58	 12	 7
	0.2 - 0.25	 0.22F	 2A	 0.023B	1.60	 21	 26D	 56	 12	 7
	0.25 - 0.3	 0.2F	 1A	 0.02B	 26	 24D	 56	 13	 9
	0.3 - 0.35	 0.17F	 1A	 0.016B	 29	 25D	 54	 13	 10
	0.35 - 0.41	 0.17F	 1A	 0.02B	1.50	 28	 27D	 46	 11	 16
	0.41 - 0.5	 0.19F	 1A	 0.02B	 20	 25D	 38	 11	 26
	0.5 - 0.6	 0.28F	 1A	 0.029B	1.50	 12	 16D	 27	 10	 47
	0.6 - 0.72	 0.27F	 1A	 0.03B	 11	 13D	 18	 8	 60
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02	 0.2C	 0.05C
	0.02 - 0.1
	0.1 - 0.2
	0.2 - 0.25	 0.18C	 0.04C
	0.25 - 0.3
	0.3 - 0.35
	0.35 - 0.41	 0.17C	 0.03C
	0.41 - 0.5
	0.5 - 0.6	 0.35C	 0.24C
	0.6 - 0.72

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C615	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6_DC	Organic carbon (%) - Dry combustion
	7_NR	Total nitrogen (%) - Not recorded
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P3A_NR	Bulk density - Not recorded
	P3B_VL_01	0.1 BAR Moisture m3/m3 - Volumetric using suction plate
	P3B_VL_15	15 BAR Moisture m3/m3 - Volumetric using pressure plate