Project Name:	CAN
	Project Code:	CAN	Site ID:	C625	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	J.R. Sleeman	Locality:	Ginninderra farm extension tank 1 paddock
	Date Desc.:	01/03/70	Elevation:	 705 metres
	Map Ref.:	Sheet No. : 8727   1:100000	Rainfall:	640
	Northing/Long.:	149.083333333333	Runoff:	Moderately rapid
	Easting/Lat.:	-35.2	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Slightly porous, Quartz porphyry 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Kandosol     	Principal Profile Form:	Gn2.24
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Tall Strata - Tree, , Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.12 m	Brown (7.5YR4/4-Moist); ; Fine sandy loam; Massive grade of structure; Field pH 5.4 (pH meter); 
	A2	0.12 - 0.25 m	Reddish yellow (7.5YR6/6-Moist); ; Sandy clay loam; Massive grade of structure; Field pH 5.3 
	(pH meter); 
	A3	0.25 - 0.37 m	Reddish yellow (7.5YR6/6-Moist); ; Sandy clay loam (Heavy); Massive grade of structure; Field 
	pH 5.5 (pH meter); 
	B2	0.37 - 0.48 m	Yellowish red (5YR5/6-Moist); , 2-10% ; , 2-10% ; Sandy medium clay; Massive grade of 
	structure; Field pH 6 (pH meter); 
	C	0.48 - 0.6 m	Yellow (2.5Y7/6-Moist); , 5YR56, 2-10% ; , 2.5Y52, 2-10% ; Field pH 6.2 (pH meter); 
	C	0.6 - 0.6 m	; 
	Morphological Notes
	C	>60 weathered QP
	Observation Notes
	Site Notes
	GINNINDERRA

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C625	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	5.4A	 0.06A	 2.4K	 1.4	 1.1	 0.13	 5.7E	 10.7J	1.21
	0.12 - 0.25	5.3A	 0.03A	 1.8K	 1.3	 0.83	 0.06	 5.9E	 9.9J	0.61
	0.25 - 0.37	5.5A	 0.03A	 2.4K	 3.1	 0.67	 0.43	 4.5E	 11.1J	3.87
	0.37 - 0.48	6A	 0.03A	 2.4K	 9	 0.51	 0.14	 1.8E	 13.8J	1.01
	0.48 - 0.6	6.2A	<0.03A	 1.3K	 13.6	 0.29	 0.37	 12.8J	2.89
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12	 1.7F	 27A	 0.144B	 8	 34D	 35	 16	 10
	0.12 - 0.25	 0.54F	 10A	 0.048B	 7	 29D	 37	 18	 16
	0.25 - 0.37	 0.38F	 6A	 0.03B	 12	 30D	 33	 21	 16
	0.37 - 0.48	 0.28F	 5A	 0.022B	 14	 35D	 18	 20	 24
	0.48 - 0.6	 0.15F	 13A	 0.008B	 20	 39D	 17	 9	 23
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.12
	0.12 - 0.25
	0.25 - 0.37
	0.37 - 0.48
	0.48 - 0.6

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C625	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6_DC	Organic carbon (%) - Dry combustion
	7_NR	Total nitrogen (%) - Not recorded
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance