Project Name:	CAN
	Project Code:	CAN	Site ID:	CP247	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Hook, Rosemary	Locality:	Hall
	Date Desc.:	04/09/86	Elevation:	586 metres
	Map Ref.:	Sheet No. : 050569   1:50000	Rainfall:	No Data
	Northing/Long.:	149.0430555	Runoff:	No Data
	Easting/Lat.:	-35.1636111  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Quartz porphyry 
	Landform
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	12 metres
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition 
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn4.1
	ASC Confidence:	Great Soil Group:	Red earth
	Confidence level not specified
	Site Disturbance
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	A12	0.05 - 0.1 m	Dark yellowish brown (10YR4/4-Moist); Strong brown (7.5YR4/6-Moist); ; Fine sandy loam; Weak grade 
	of structure, 5-10 mm, Granular; Firm consistence; 0-2%, fine gravelly, 2-6mm, Quartz, coarse 
	fragments; Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; 
	AB	0.1 - 0.2 m	Strong brown (7.5YR4/6-Moist); ; Fine sandy clay loam; Weak grade of structure, 2-5 mm, Granular; 
	Firm consistence; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; Very few (0 - 2 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules; Gradual change to - 
	B	0.25 - 0.3 m	Red (2.5YR4/6-Moist); ; Light clay; Moderate grade of structure, 5-10 mm, Subangular blocky; Firm 
	consistence; 2-10%, fine gravelly, 2-6mm, Quartz, coarse fragments; Few (2 - 10 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules; Gradual change to - 
	B	0.32 - 0.48 m	Red (2.5YR4/6-Moist); ; Light clay; Massive grade of structure; Firm consistence; 2-10%, medium 
	gravelly, 6-20mm, Quartz, coarse fragments; Common (10 - 20 %), Ferromanganiferous, Coarse (6 - 20 
	mm), Nodules; 
	B	0.48 - 0.62 m	Yellowish red (5YR4/6-Moist); ; Light clay; Massive grade of structure; Firm consistence; 20-50%, 
	medium gravelly, 6-20mm, Quartz, coarse fragments; Many (20 - 50 %), Ferromanganiferous, Coarse (6
	 - 20 mm), Nodules; Clear change to - 
	B	0.62 - 0.7 m	Pale brown (10YR6/3-Moist); ; Clayey sand; Massive grade of structure; Very weak consistence; 50-90%,
	 medium gravelly, 6-20mm, Quartz, coarse fragments; Very many (50 - 100 %), Ferromanganiferous, 
	Coarse (6 - 20 mm), Nodules; Clear change to - 
	B	0.7 - 0.85 m	Pale red (2.5YR7/2-Moist); ; Heavy clay; Massive grade of structure; Firm consistence; Few (2 - 10 %), 
	Ferromanganiferous, Coarse (6 - 20 mm), Nodules; 
	B	0.85 - 0.95 m	Pale red (2.5YR7/2-Moist); ; Heavy clay; Massive grade of structure; Firm consistence; Very few (0 - 2 
	%), Ferromanganiferous, Coarse (6 - 20 mm), Nodules; 
	Morphological Notes
	B	gravelly
	B	gravelly
	B	very gravelly
	B	clayey
	B	with gravel
	B	with gravel; a few fine roots to 0.85 m.
	Observation Notes
	Site Notes
	Ginninderra experimental station toposequence for Rosemary Hook's MSc program. CP247 is 20 m NE of CP246 (on hillcrest), 
	approximately 250 m west of Bond/Willett sludge sites. Improved pasture land.

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP247	Observation 	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.05 - 0.1	5A	0.04A	0.75F	0.21	0.58	0.05
	0.1 - 0.2	5A	0.02A	0.46F	0.13	0.17	0
	0.25 - 0.3	5.5A	0.02A	1.6F	0.73	0.44	0.05
	0.32 - 0.48	5.9A	0.02A	2.7F	1.3	0.65	0.05
	0.48 - 0.62	6.5A	0.02A	3.2F	2.2	0.56	0.03
	0.62 - 0.7	6.5A	0.02A	1.7F	1.5	0.15	0.05
	0.7 - 0.85	6.2A	0.02A	5.6F	7.8	0.69	0.29
	0.85 - 0.95	6A	0.02A	5.7F	8.8	0.75	0.3
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.05 - 0.1	1.22A
	0.1 - 0.2	0.44A
	0.25 - 0.3	0.29A
	0.32 - 0.48	0.24A
	0.48 - 0.62	0.15A
	0.62 - 0.7	0.14A
	0.7 - 0.85	0.13A
	0.85 - 0.95	0.13A
	Laboratory Analyses Completed for this profile
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15I4	CEC measurement - titration of ammonium and chloride ions
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6A1	Organic carbon - Walkley and Black