Project Name:	CAN
	Project Code:	CAN	Site ID:	CP73	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P.H. Walker	Locality:	901
	Date Desc.:	01/04/77	Elevation:	 600 metres
	Map Ref.:	Sheet No. : 8727   1:100000	Rainfall:	640
	Northing/Long.:	149.205	Runoff:	Slow
	Easting/Lat.:	-35.2852777777778	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Terrace (alluvial)
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	225 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Hypercalcic Brown Kandosol     	Principal Profile Form:	Gn
	ASC Confidence:	Great Soil Group:	Yellow earth
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Irrigated, past or present
	Vegetation:	Low Strata - Forb, , . *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Brown (7.5YR4/4-Moist); ; Fine sandy loam; Massive grade of structure; Dry; Firm consistence; 
	Field pH 5 (pH meter); Gradual change to - 
	A1	0.1 - 0.2 m	Yellowish red (5YR4/6-Moist); ; Fine sandy loam; Massive grade of structure; Dry; Firm 
	consistence; 2-10%, fine gravelly, 2-6mm, dispersed, Gravel, coarse fragments; Very few (0 - 2 
	%), Ferromanganiferous, Fine (0 - 2 mm), ; Field pH 5.1 (pH meter); Diffuse change to - 
	A2	0.2 - 0.3 m	Yellowish red (5YR4/8-Moist); Strong brown (7.5YR5/6-Dry); ; Fine sandy loam; Massive grade of
	 structure; Dry; Very firm consistence; 2-10%, fine gravelly, 2-6mm, dispersed, Gravel, coarse 
	fragments; Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), ; Field pH 6.3 (pH meter); 
	Diffuse change to - 
	A3	0.3 - 0.4 m	Yellowish red (5YR4/8-Moist); ; Clay loam, fine sandy; Massive grade of structure; Dry; Very firm 
	consistence; 2-10%, fine gravelly, 2-6mm, dispersed, Gravel, coarse fragments; Very few (0 - 2 
	%), Ferromanganiferous, Medium (2 -6 mm), ; Field pH 6.8 (pH meter); Clear change to - 
	B1	0.4 - 0.5 m	Yellowish red (5YR5/6-Moist); ; Fine sandy medium clay; Massive grade of structure; Earthy 
	fabric; Dry; Very strong consistence; 10-20%, fine gravelly, 2-6mm, dispersed, Gravel, coarse 
	fragments; Few (2 - 10 %), Ferromanganiferous, Medium (2 -6 mm), ; Field pH 6.7 (pH meter); 
	Clear change to - 
	B1	0.5 - 0.6 m	Strong brown (7.5YR5/6-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Dry; Very 
	strong consistence; 20-50%, fine gravelly, 2-6mm, dispersed, Gravel, coarse fragments; 
	Common (10 - 20 %), Ferromanganiferous, Medium (2 -6 mm), ; Field pH 6.9 (pH meter); Gradual 
	change to - 
	B1	0.6 - 0.7 m	Reddish brown (2.5YR5/4-Moist); , 2.5YR36, 2-10% ; , 2-10% ; Light clay; Massive grade of 
	structure; Earthy fabric; Dry; Very firm consistence; 20-50%, fine gravelly, 2-6mm, dispersed, 
	Gravel, coarse fragments; Common (10 - 20 %), Ferromanganiferous, Medium (2 -6 mm), ; Field 
	pH 7 (pH meter); Clear change to - 
	B2	0.7 - 0.8 m	Yellowish red (5YR4/6-Moist); , 2.5Y56, 20-50% ; , 20-50% ; Heavy clay; Massive grade of 
	structure; Smooth-ped fabric; Dry; Very strong consistence; Field pH 7 (pH meter); Clear change
	 to - 

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP73	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	B2	0.8 - 0.9 m	Light olive brown (2.5Y5/4-Moist); , 2.5Y42; Heavy clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Smooth-ped fabric; Dry; Very strong consistence; Field pH 7.2 (pH meter); 
	Gradual change to - 
	B2	0.9 - 1 m	Light olive brown (2.5Y5/4-Moist); , 2.5Y42, 0-2% ; , 0-2% ; Heavy clay; Moderate grade of 
	structure, 20-50 mm, Angular blocky; Smooth-ped fabric; Dry; Very strong consistence; Field pH 
	7.9 (pH meter); Gradual change to - 
	B2	1.1 - 1.3 m	Greyish brown (2.5Y5/3-Moist); , 2.5Y42, 0-2% ; , 0-2% ; Heavy clay; Weak grade of structure, 20-
	50 mm, Angular blocky; Smooth-ped fabric; Dry; Very strong consistence; Field pH 8.6 (pH 
	meter); Gradual change to - 
	Bk	1.3 - 1.5 m	Light olive brown (2.5Y5/4-Moist); , 5YR46, 2-10% ; , 2-10% ; Medium clay; Massive grade of 
	structure; Smooth-ped fabric; Dry; Very strong consistence; Very few (0 - 2 %), 
	Ferromanganiferous, , ; Very few (0 - 2 %), Calcareous, , Concretions; Field pH 8.9 (pH meter); 
	Clear change to - 
	BCk	1.5 - 1.7 m	Light olive brown (2.5Y5/4-Moist); , 5YR58, 20-50% ; , 2.5YR44, 20-50% ; Light clay; Massive 
	grade of structure; Smooth-ped fabric; Dry; Very strong consistence; Few (2 - 10 %), Calcareous,
	 , Concretions; Field pH 8.9 (pH meter); Gradual change to - 
	Ck	1.7 - 1.9 m	Light brownish grey (2.5Y6/2-Moist); , 2.5Y58, 0-2% ; , 2.5YR44, 0-2% ; Light clay; Massive 
	grade of structure; Earthy fabric; Dry; Very strong consistence; Very few (0 - 2 %), Calcareous, , 
	Concretions; Field pH 8.9 (pH meter); Gradual change to - 
	Ck	1.9 - 2 m	Light brownish grey (2.5Y6/2-Moist); , 2.5Y58, 0-2% ; , 2.5YR44, 0-2% ; Light clay; Massive 
	grade of structure; Earthy fabric; Dry; Very strong consistence; Very few (0 - 2 %), Calcareous, , 
	Concretions; Field pH 8.9 (pH meter); 
	Morphological Notes
	Observation Notes
	ALLUVIUM BIOTIC ACTIVITY 0-60CM                                                                                         
	Site Notes
	KARARA

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP73	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5A	 0.07A	 1.8K	 0.2	 0.23	 0	 10.4B	 12.7J	0.00
	0.1 - 0.2	5.1A	<0.04A
	0.2 - 0.3	6.3A	<0.04A	 3K	 0.55	 0.11	 0	 4.9B	 8.6J	0.00
	0.3 - 0.4	6.8A	<0.04A
	0.4 - 0.5	6.7A	<0.04A	 2.8K	 0.94	 0.15	 0	 5.8B	 9.7J	0.00
	0.5 - 0.6	6.9A	<0.04A
	0.6 - 0.7	7A	<0.04A	 2.8K	 1.8	 0.15	 0.35	 5.6B	 10.8J	3.24
	0.7 - 0.8	7A	 0.04A
	0.8 - 0.9	7.2A	 0.08A	 8.1K	 9.9	 0.38	 2.5	 11.4B	 32.3J	7.74
	0.9 - 1	7.9A	 0.12A
	1.1 - 1.3	8.6A	 0.12A	 8.7K	 11.7	 0.33	 3.3	 3.3B	 27.3J	12.09
	1.3 - 1.5	8.9A	 0.12A
	1.5 - 1.7	8.9A	 0.08A
	1.7 - 1.9	8.9A	 0.08A
	1.9 - 2	8.9A	 0.13A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.55D	 0.137B	 6D	 53	 23	 14
	0.1 - 0.2	 0.51D	 0.055B	 6D	 51	 21	 19
	0.2 - 0.3	 0.33D	 0.044B	 6D	 49	 25	 20
	0.3 - 0.4	 0.33D	 0.043B	 6D	 46	 22	 22
	0.4 - 0.5	 0.23D	 0.033B	 8D	 42	 27	 23
	0.5 - 0.6	 0.18D	 0.023B	 6D	 39	 28	 26
	0.6 - 0.7	 0.16D	 0.028B	 5D	 37	 28	 28
	0.7 - 0.8	 0.43D	 0.067B	 1D	 14	 16	 72
	0.8 - 0.9	 0.41D	 0.064B	 1D	 8	 15	 75
	0.9 - 1	 0.26D	 0.048B
	1.1 - 1.3	 0.07A	 0.14D	 1D	 13	 20	 66
	1.3 - 1.5	 0.07A	 0.09D	 0D	 18	 28	 52
	1.5 - 1.7	 0.07A	 0.06D
	1.7 - 1.9	 0.08A	 0.05D	 0D	 43	 23	 30
	1.9 - 2	 0.17A	 0.06D
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1
	1.1 - 1.3

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP73	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	1.3 - 1.5
	1.5 - 1.7
	1.7 - 1.9
	1.9 - 2

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP73	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G_C_AL1	Exchangeable aluminium - meq per 100g of soil - Aluminium By difference of C and A or B
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance