Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	16	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Locality:	Temora, NSW.  Owner Ag Res Stn W2
	Date Desc.:	01/01/78	Elevation:	No Data
	Map Ref.:	1:100000	Rainfall:	No Data
	Northing/Long.:	147.51666666	Runoff:	No Data
	Easting/Lat.:	-34.4	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dr2.43
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	Confidence level not specified
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Reddish brown (5YR4/4-Moist); ; Loamy fine sand; Massive grade of structure; Weak 
	consistence; Field pH 5.5 (Raupach); 
	A2	0.1 - 0.27 m	Brown (7.5YR4/4-Moist); ; Loamy fine sand; Massive grade of structure; Weak consistence; 
	B11	0.27 - 0.38 m	Reddish brown (5YR4/4-Moist); ; Medium clay; , Subangular blocky; Firm consistence; 
	B12	0.38 - 0.56 m	Yellowish red (5YR4/6-Moist); ; Medium clay; , Subangular blocky; Firm consistence; 
	0.56 - 1.5 m	Brown (7.5YR5/4-Moist); ; Medium clay; , Subangular blocky; Firm consistence; Field pH 8.5 
	(Raupach); 
	1.5 - 2 m	Yellowish brown (10YR5/4-Moist); ; Medium clay; , Subangular blocky; Firm consistence; Field 
	pH 9 (Raupach); 
	Morphological Notes
	Observation Notes
	Met stn:  Ag Res Stn.  Rain zone Wm
	Site Notes

	Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	16	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.6A	0.18A
	0.05 - 0.1
	0.1 - 0.2	5.3A	0.18A
	0.2 - 0.3	5.5A	0.1A
	0.3 - 0.4	6.1A	0.09A
	0.32 - 0.37
	0.4 - 0.6	6.9A	0.1A
	0.6 - 0.8	7.8A	0.07A
	0.8 - 1	8.5A	0.11A
	1 - 1.2	8.5A	0.08A
	1.2 - 1.6	8.7A	0.06A
	1.6 - 2	8.6A	0.07A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0C	1.23A	3A	57	22	15
	0.05 - 0.1	1.44
	0.1 - 0.2	0C	0.57A	2A	45	34	19
	0.2 - 0.3	0C	0.23A	1A	39	36	22
	0.3 - 0.4	0C	0.22A	1A	24	31	45
	0.32 - 0.37	1.69
	0.4 - 0.6	0C	1A	18	24	56
	0.6 - 0.8
	0.8 - 1
	1 - 1.2
	1.2 - 1.6
	1.6 - 2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.05 - 0.1	0.39D	0.31D	0.29D	0.21D	0.12E	65C
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.32 - 0.37	0.28D	0.26D	0.25D	0.23D	0.16E	1.25C
	0.4 - 0.6
	0.6 - 0.8
	0.8 - 1
	1 - 1.2
	1.2 - 1.6
	1.6 - 2

	Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	16	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6A1	Organic carbon - Walkley and Black
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P3A1	Bulk density - g/cm3
	P3B1VL_1	1 BAR Moisture m3/m3 - Volumetric using <2mm sample on pressure plate
	P3B1VL_15	15 BAR Moisture m3/m3 - Volumetric using <2mm sample on pressure plate
	P3B3VLa005	0.05 BAR Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P3B3VLa01	0.1 BAR Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P3B3VLaSAT	Saturated Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P4_sat_For	Saturated Hydraulic Conductivity (Forrest et al, 1985)