Project Name:	Hardsetting Soils
	Project Code:	HS	Site ID:	CP297	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	C.J. Chartres	Locality:	East-southeast of 'Yerong Creek'
	Date Desc.:	01/01/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8327   1:100000	Rainfall:	No Data
	Northing/Long.:	6082317 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	509267  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	 % 	Aspect:	5 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.11 m	Dark brown (7.5YR3/4-Moist); ; Silty loam; Moderate grade of structure, <2 mm, Granular; Weak 
	consistence; Many
	A12	0.11 - 0.2 m	Brown (7.5YR4/4-Moist); , 7.5YR34; Silty loam; Massive grade of structure; Weak grade of 
	structure, 5-10 mm, Subangular blocky; Weak consistence; Common
	A2	0.2 - 0.32 m	Yellowish brown (10YR5/4-Moist); ; Silty loam; Weak grade of structure, 5-10 mm, Subangular 
	blocky; Massive grade of structure; Firm consistence; Common
	B21t	0.32 - 0.47 m	Strong brown (7.5YR5/6-Moist); , 10YR54, 10-20% , 5-15mm, Faint; Silty clay loam; Moderate 
	grade of structure, 5-10 mm, Subangular blocky; Firm consistence; Few
	B22t	0.47 - 0.7 m	Yellowish red (5YR5/6-Moist); ; Silty clay; Moderate grade of structure, 5-10 mm, Subangular 
	blocky; Firm consistence; Few
	B23t	0.7 - 1.1 m	Yellowish brown (10YR5/6-Moist); , 5YR56, 20-50% , 5-15mm, Distinct; Silty clay; Weak grade 
	of structure, 5-10 mm, Subangular blocky; Weak consistence; 
	BC1	1.1 - 1.3 m	Yellowish brown (10YR5/6-Moist); , 5YR58, 10-20% , 5-15mm, Distinct; Silty clay loam; Massive
	 grade of structure; Weak consistence; 
	BC2	1.3 - 1.5 m	Yellowish brown (10YR5/6-Moist); , 5YR58, 10-20% , 5-15mm, Faint; Silty clay loam; Massive 
	grade of structure; Weak consistence; 
	1.5 - 2 m	Yellowish brown (10YR5/6-Moist); , 2.5YR58, 10-20% , 5-15mm, Distinct; Silty clay; Massive 
	grade of structure; Weak consistence; 
	2 - 2.55 m	Yellowish brown (10YR5/6-Moist); , 2.5YR58, 10-20% , 5-15mm, Distinct; Silty clay; Massive 
	grade of structure; Weak consistence; 
	Morphological Notes
	A11	American system, horizon is A.
	A12	American system, horizon is E+A.
	A2	American system, horizon is E.
	B21t	American system, horizon is Bt1.
	B22t	American system, horizon is Bt2.
	B23t	American system, horizon is Bt3.

	Project Name:	Hardsetting Soils
	Project Code:	HS	Site ID:	CP297	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	No horizon given, sample 9.
	No horizon given, sample 10.
	Observation Notes
	Soil Taxonomy, Typic Natrixeralf fine.
	Site Notes

	Project Name:	Hardsetting Soils
	Project Code:	HS	Site ID:	CP297	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.11	5.19A	0.06A	1.2E	0.31	0.55	0.01
	0.11 - 0.2	5.92A	0.04A	1.4E	0.61	0.39	0.14
	0.2 - 0.32	7.36A	0.09A	2.1E	2.4	0.35	0.91
	0.32 - 0.47	7.62A	0.3A	2.5E	4.5	0.35	2.5
	0.47 - 0.7	8.36A	0.57A	3.4E	9.2	0.83	5
	0.7 - 1.1	8.69A	0.46A	2.9E	9.8	0.96	5.6
	1.1 - 1.3	8.91A	0.38A	2.9E	10.2	0.99	5.3
	1.3 - 1.5	9.17A	0.42A	2.6E	8.1	0.75	4.7
	1.5 - 2	8.94A	0.36A
	2 - 2.55	9.09A	0.52A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.11	1.05C	7D	52	19	21
	0.11 - 0.2	0.3C	8D	57	20	14
	0.2 - 0.32	0.16C	8D	52	20	20
	0.32 - 0.47	7D	40	15	38
	0.47 - 0.7	5D	31	11	48
	0.7 - 1.1	4D	31	11	53
	1.1 - 1.3	3D	32	11	52
	1.3 - 1.5	5D	31	11	50
	1.5 - 2
	2 - 2.55
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.11
	0.11 - 0.2
	0.2 - 0.32
	0.32 - 0.47
	0.47 - 0.7
	0.7 - 1.1
	1.1 - 1.3
	1.3 - 1.5
	1.5 - 2
	2 - 2.55

	Project Name:	Hardsetting Soils
	Project Code:	HS	Site ID:	CP297	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	13A1_AL	Oxalate-extractable aluminium
	13A1_FE	Oxalate-extractable iron
	13A1_MN	Oxalate-extractable manganese
	13A1_SI	Oxalate-extractable silicon
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_SI	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment 
	for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15I4	CEC measurement - titration of ammonium and chloride ions
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance