Project Name:	LSG
	Project Code:	LSG	Site ID:	CP70	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P.H. Walker	Locality:	Sand sheet on river terrace
	Date Desc.:	//	Elevation:	 600 metres
	Map Ref.:	Sheet No. : 8729   1:100000	Rainfall:	640
	Northing/Long.:	149.186111111111	Runoff:	No runoff
	Easting/Lat.:	-35.3194444444445	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Terrace (alluvial)
	3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	125 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Kandosol     	Principal Profile Form:	Uc
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.15 m	Red (2.5YR5/8-Moist); ; Loamy coarse sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Field pH 6.8 (pH meter); Abrupt change to - 
	A	0.15 - 0.25 m	Dark reddish brown (5YR3/3-Moist); ; Loamy sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; Very firm consistence; Field pH 6.2 (pH meter); Clear change to - 
	AB	0.25 - 0.35 m	Yellowish red (5YR4/6-Moist); ; Sandy loam; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; Very firm consistence; Field pH 6.5 (pH meter); Gradual change to - 
	B	0.35 - 0.45 m	Yellowish red (5YR5/6-Moist); ; Loamy sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; Very firm consistence; Field pH 7 (pH meter); Gradual change to - 
	B	0.45 - 0.55 m	Yellowish red (5YR5/8-Moist); ; Loamy sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; Firm consistence; Field pH 7.2 (pH meter); Clear change to - 
	B	0.55 - 0.65 m	Red (2.5YR4/6-Moist); ; Sandy loam; Massive grade of structure; Sandy (grains prominent) 
	fabric; Dry; Firm consistence; Field pH 7.2 (pH meter); Diffuse change to - 
	B	0.65 - 0.72 m	Red (2.5YR4/6-Moist); ; Sandy loam; Massive grade of structure; Sandy (grains prominent) 
	fabric; Dry; Firm consistence; Field pH 7.2 (pH meter); Gradual change to - 
	BC	0.72 - 0.8 m	Red (2.5YR4/6-Moist); , 7.5YR58; Loamy sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; Firm consistence; Field pH 7.1 (pH meter); Diffuse change to - 
	BC	0.8 - 0.9 m	Red (2.5YR4/6-Moist); , 7.5YR58; Loamy sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; Firm consistence; Field pH 7.1 (pH meter); Gradual change to - 
	C	0.9 - 1 m	Reddish yellow (7.5YR6/6-Moist); , 7.5YR44, 2-10% ; , 2.5YR46, 2-10% ; Loamy sand; Massive
	 grade of structure; Sandy (grains prominent) fabric; Dry; Firm consistence; Field pH 7.1 (pH 
	meter); Gradual change to - 
	C	1.1 - 1.2 m	Reddish yellow (7.5YR6/6-Moist); , 2.5YR46, 20-50% ; , 7.5YR44, 20-50% ; Sand; Massive 
	grade of structure; Sandy (grains prominent) fabric; Dry; Very weak consistence; Field pH 7 
	(pH meter); Gradual change to - 

	Project Name:	LSG
	Project Code:	LSG	Site ID:	CP70	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	C	1.2 - 1.2 m	Yellowish brown (10YR5/8-Moist); , 7.5YR44, 20-50% ; , 2.5YR48, 20-50% ; Sand; Massive 
	grade of structure; Sandy (grains prominent) fabric; Dry; Very weak consistence; 0-2%, fine 
	gravelly, 2-6mm, coarse fragments; Field pH 6.8 (pH meter); Clear change to - 
	D	1.32 - 1.4 m	Light brownish grey (2.5Y6/2-Moist); , 5YR58, 20-50% ; , 10YR22, 20-50% ; Light clay; 
	Massive grade of structure; Earthy fabric; Dry; Very firm consistence; 2-10%, fine gravelly, 2-
	6mm, coarse fragments; Field pH 7.3 (pH meter); Clear change to - 
	D	1.4 - 1.55 m	Yellowish red (5YR4/8-Moist); , 2.5YR52, 20-50% ; , 10YR22, 20-50% ; Medium clay; Massive 
	grade of structure; Earthy fabric; Dry; Very firm consistence; Field pH 7.6 (pH meter); Clear 
	change to - 
	D	1.55 - 1.65 m	Weak red (2.5YR5/2-Moist); , 2.5Y68, 20-50% ; , 10YR58, 20-50% ; Clay loam; Massive grade 
	of structure; Earthy fabric; Dry; Firm consistence; Field pH 7.8 (pH meter); Clear change to - 
	D	1.65 - 1.8 m	Yellowish red (5YR4/8-Moist); , 5Y62, 20-50% ; , 20-50% ; Medium clay; Massive grade of 
	structure; Earthy fabric; Dry; Very firm consistence; Field pH 7.9 (pH meter); Clear change to - 
	D	1.85 - 2 m	Pinkish grey (5YR6/2-Moist); , 7.5YR58, 20-50% ; , 20-50% ; Clay loam; Massive grade of 
	structure; Earthy fabric; Dry; Firm consistence; 20-50%, coarse fragments; Field pH 7.9 (pH 
	meter); 
	Morphological Notes
	Observation Notes
	AEOLIAN SAND:15-25CM SAND UNIMODAL <0.5MM:25-120CM BIMODOL:LUSTROUS S 132-200CM:SLICKENSIDES 165-180CM:
	                 
	Site Notes
	PIALLIGO

	Project Name:	LSG
	Project Code:	LSG	Site ID:	CP70	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	6.8A	<0.04A
	0.15 - 0.25	6.2A	<0.04A	 2.6K	 0.78	 0.14	 0.25	 2.2B	 6.1J	4.10
	0.25 - 0.35	6.5A	<0.04A	 2.5K	 0.45	 0.14	 0.21	 1.7B	 5.1J	4.12
	0.35 - 0.45	7A	<0.04A	 3K	 0.48	 0.07	 0.13	 3.3B	 7.1J	1.83
	0.45 - 0.55	7.2A	<0.04A
	0.55 - 0.65	7.2A	<0.04A	 4.6K	 1.1	 0.21	 0.22	 2.6B	 8.7J	2.53
	0.65 - 0.72	7.2A	<0.04A
	0.72 - 0.8	7.1A	<0.04A	 3.9K	 1	 0.06	 0.08	 1.1B	 6.1J	1.31
	0.8 - 0.9	7.1A	<0.04A
	0.9 - 1	7.1A	<0.04A	 3.5K	 0.95	 0.15	 0.11	 0.8B	 5.6J	1.96
	1.1 - 1.2	7A	<0.04A
	1.2 - 1.3	6.8A	<0.04A	 3.2K	 1.1	 0.15	 0.13	 1B	 5.6J	2.32
	1.32 - 1.4	7.3A	<0.04A
	1.4 - 1.55	7.6A	<0.04A
	1.55 - 1.65	7.8A	<0.04A
	1.65 - 1.8	7.9A	<0.04A
	1.85 - 2	7.9A	<0.04A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15
	0.15 - 0.25	 0.4D	 0.051B	 0	 39D	 35	 13	 11
	0.25 - 0.35	 0.24D	 0.034B	 0	 40D	 36	 12	 11
	0.35 - 0.45	 0.2D	 0.025B	 0	 38D	 39	 11	 12
	0.45 - 0.55	 0.15D	 0.021B	 0	 36D	 42	 11	 11
	0.55 - 0.65	 0.23D	 0.035B	 0	 31D	 41	 9	 19
	0.65 - 0.72	 0.24D	 0.028B	 0	 33D	 43	 8	 16
	0.72 - 0.8	 0.19D	 0.02B	 0	 37D	 43	 7	 13
	0.8 - 0.9	 0.18D	 0.018B	 0	 42D	 37	 10	 13
	0.9 - 1	 0.11D	 0.012B	 0	 52D	 28	 8	 12
	1.1 - 1.2	 0.08D	 0.007B	 0	 60D	 24	 8	 9
	1.2 - 1.3	 0.08D	 0.01B	 0	 61D	 21	 7	 11
	1.32 - 1.4	 0.05D	 0.007B	 3	 22D	 39	 16	 21
	1.4 - 1.55	 0.07D	 0.016B	 2	 15D	 38	 14	 32
	1.55 - 1.65	 0.03D
	1.65 - 1.8	 0.05D
	1.85 - 2	 0.03D
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.25
	0.25 - 0.35
	0.35 - 0.45
	0.45 - 0.55
	0.55 - 0.65
	0.65 - 0.72

	Project Name:	LSG
	Project Code:	LSG	Site ID:	CP70	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	0.72 - 0.8
	0.8 - 0.9
	0.9 - 1
	1.1 - 1.2
	1.2 - 1.3
	1.32 - 1.4
	1.4 - 1.55
	1.55 - 1.65
	1.65 - 1.8
	1.85 - 2

	Project Name:	LSG
	Project Code:	LSG	Site ID:	CP70	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G_C_AL1	Exchangeable aluminium - meq per 100g of soil - Aluminium By difference of C and A or B
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance