Project Name:	LSG
	Project Code:	LSG	Site ID:	CP79	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	J.R. Sleeman	Locality:	Northcott Dve. site 1
	Date Desc.:	01/04/77	Elevation:	 650 metres
	Map Ref.:	Sheet No. : S155-16   1:250000	Rainfall:	640
	Northing/Long.:	149.166666666667	Runoff:	Very slow
	Easting/Lat.:	-35.2666666666667	Drainage:	Poorly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Hills
	1-3%
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	1 % 	Aspect:	210 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melanic Eutrophic Yellow Chromosol     	Principal Profile Form:	Dy2.82
	ASC Confidence:	Great Soil Group:	Yellow podzolic 
	All necessary analytical data are available.	soil
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	AC	0 - 0.2 m	Dark brown (7.5YR3/2-Moist); ; Fine sandy loam; Massive grade of structure; Sandy (grains 
	prominent) fabric; Few (<1 per 100mm2)  macropores, Very firm consistence; Field pH 6.3 (pH 
	meter); Clear change to - 
	2A1	0.2 - 0.34 m	Very dark greyish brown (10YR3/2-Moist); Brown (10YR5/3-Dry); , 10YR71, 20-50% ; , 20-
	50% ; Silty loam; Massive grade of structure; Sandy (grains prominent) fabric; Few (<1 per 
	100mm2)  macropores, Very firm consistence; Very few (0 - 2 %), Ferruginous, Fine (0 - 2 
	mm), Nodules; Field pH 6.4 (pH meter); Clear change to - 
	2A1	0.34 - 0.41 m	Very dark greyish brown (10YR3/2-Moist); Brown (10YR5/3-Dry); , 10YR71, 20-50% ; , 20-
	50% ; Silty loam; Massive grade of structure; Sandy (grains prominent) fabric; Few (<1 per 
	100mm2)  macropores, Very firm consistence; Very few (0 - 2 %), Ferruginous, Fine (0 - 2 
	mm), Nodules; Field pH 6.4 (pH meter); Clear change to - 
	2A3	0.41 - 0.48 m	Brown (10YR4/3-Moist); Pale brown (10YR6/3-Dry); ; Clay loam; Massive grade of structure; 
	Sandy (grains prominent) fabric; Very strong consistence; Few (2 - 10 %), Ferruginous, 
	Medium (2 -6 mm), Nodules; Field pH 6.4 (pH meter); Abrupt change to - 
	2B21	0.48 - 0.6 m	Reddish yellow (7.5YR6/8-Moist); Dark yellowish brown (10YR3/4-Dry); ; Medium clay; Massive
	 grade of structure; Very strong consistence; Very few (0 - 2 %), Ferromanganiferous, Medium
	 (2 -6 mm), Nodules; Field pH 6.7 (pH meter); Gradual change to - 
	2B22	0.6 - 0.85 m	Greyish brown (10YR5/2-Moist); Brownish yellow (10YR6/6-Dry); ; Medium clay; Massive 
	grade of structure; Earthy fabric; Very strong consistence; Very few (0 - 2 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules; Field pH 6.9 (pH meter); 
	2B23	0.85 - 1 m	Greyish brown (10YR5/2-Moist); Brownish yellow (10YR6/6-Dry); ; Medium clay; Massive 
	grade of structure; Very strong consistence; 
	Morphological Notes
	Observation Notes
	48-60CM LUSTOUS FACES:COLLUVIUM:                                                                                        
	Site Notes

	Project Name:	LSG
	Project Code:	LSG	Site ID:	CP79	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)

	Project Name:	LSG
	Project Code:	LSG	Site ID:	CP79	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.2	6.3A	 0.05A	 5.2K	 6.2	 0.21	 0.21	 12.2B	 24J	0.88
	0.2 - 0.34	6.4A	 0.03A	 3.8K	 5.7	 0.08	 0.17	 8.9B	 18.7J	0.91
	0.34 - 0.41	6.4A	 0.03A	 2.3K	 4.8	 0.06	 0.13	 4.9B	 12.2J	1.07
	0.41 - 0.48	6.4A	 0.03A	 2K	 5.4	 0.07	 0.22	 4.7B	 12.4J	1.77
	0.48 - 0.6	6.7A	 0.03A	 2.2K	 8.7	 0.14	 0.38	 9.2B	 20.7J	1.84
	0.6 - 0.85	6.9A	 0.04A	 2.1K	 8.9	 0.17	 0.64	 9.9B	 21.7J	2.95
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.2	 2.74D	 0.18B	 28	 5D	 32	 35	 22
	0.2 - 0.34	 1.51D	 0.116B	 1	 3D	 39	 35	 20
	0.34 - 0.41	 0.8D	 0.06B	 3	 6D	 43	 33	 16
	0.41 - 0.48	 0.64D	 0.052B	 9	 6D	 42	 30	 22
	0.48 - 0.6	 0.65D	 0.06B	 9	 5D	 30	 23	 42
	0.6 - 0.85	 0.31D	 0.018B	 13	 5D	 27	 28	 46
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.2
	0.2 - 0.34
	0.34 - 0.41
	0.41 - 0.48
	0.48 - 0.6
	0.6 - 0.85

	Project Name:	LSG
	Project Code:	LSG	Site ID:	CP79	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G_C_AL1	Exchangeable aluminium - meq per 100g of soil - Aluminium By difference of C and A or B
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance