Project Name:	LSG
	Project Code:	LSG	Site ID:	CP83	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	J.R. Sleeman	Locality:	30M upstream of Fairburn Ave.bridge(west bank)site
	 3:
	Date Desc.:	01/04/77	Elevation:	 610 metres
	Map Ref.:	Sheet No. : S155-16   1:250000	Rainfall:	640
	Northing/Long.:	149.183333333333	Runoff:	Moderately rapid
	Easting/Lat.:	-35.2833333333333	Drainage:	Moderately well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Slightly porous, 
	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Hills
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	210 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mesotrophic Subnatric Red Sodosol     	Principal Profile Form:	Dy2.52
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Sod grass, , . *Species includes - None recorded
	Surface Coarse Fragments:	2-10%, fine gravelly, 2-6mm, , Substrate material
	Profile Morphology
	A11	0 - 0.1 m	Brown (7.5YR4/4-Moist); ; Loam; Massive grade of structure; Sandy (grains prominent) fabric; 
	Few (<1 per 100mm2)  macropores, Dry; Firm consistence; 2-10%, fine gravelly, 2-6mm, 
	Substrate material, coarse fragments; Field pH 5.7 (pH meter); Clear change to - 
	A12	0.1 - 0.3 m	Dark reddish brown (5YR3/4-Moist); ; Loam (Heavy); Massive grade of structure; Sandy 
	(grains prominent) fabric; Many (>5 per 100mm2)  macropores, Dry; Firm consistence; 2-10%, 
	coarse gravelly, 20-60mm, Substrate material, coarse fragments; Field pH 6.2 (pH meter); Clear 
	change to - 
	A2	0.3 - 0.42 m	Pink (7.5YR7/4-Moist); Reddish yellow (7.5YR6/6-Dry); , 5YR56, 20-50% , Distinct; , 20-50% , 
	Distinct; Clay loam; Massive grade of structure; Sandy (grains prominent) fabric; Many (>5 per 
	100mm2)  macropores, Dry; Very firm consistence; Field pH 6.7 (pH meter); Clear change to - 
	B	0.42 - 0.6 m	Yellowish red (5YR5/6-Moist); ; Medium clay; Massive grade of structure; Earthy fabric; Dry; 
	Very strong consistence; Field pH 7.1 (pH meter); Abrupt change to - 
	0.6 - 0.74 m	Yellowish red (5YR5/8-Moist); Brownish yellow (10YR6/8-Dry); ; Medium clay; Massive grade 
	of structure; Earthy fabric; Very strong consistence; 20-50%, coarse gravelly, 20-60mm, 
	angular, Substrate material, coarse fragments; Field pH 8 (pH meter); Clear change to - 
	0.74 - 1 m	Yellowish red (5YR5/6-Moist); , 5YR73, 20-50% , Distinct; , 20-50% , Distinct; Light clay; 
	Massive grade of structure; Earthy fabric; Very strong consistence; , Manganiferous, , Soft 
	segregations; Field pH 8.9 (pH meter); 
	Morphological Notes
	Observation Notes
	42-100CM SOME LUSTROUS CLAY FACES:COLLIUM:                                                                              
	Site Notes
	C'BERRA A'PORT

	Project Name:	LSG
	Project Code:	LSG	Site ID:	CP83	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.7A	 0.05A	 4.1K	 1.5	 0.38	 0.13	 9.2B	 15.3J	0.85
	0.1 - 0.3	6.2A	 0.02A	 3.6K	 1.5	 0.22	 0.15	 5.7B	 11.3J	1.33
	0.3 - 0.42	6.7A	 0.02A	 3.2K	 2.5	 0.11	 0.38	 7.3B	 13.6J	2.79
	0.42 - 0.6	7.1A	 0.02A	 2.9K	 3.2	 0.14	 1	 9.8B	 17.1J	5.85
	0.6 - 0.74	8A	 0.06A	 3.3K	 5.6	 0.17	 2.1	 4.8B	 16.1J	13.04
	0.74 - 1	8.9A	 0.16A	 2.6K	 6	 0.17	 2.6	 3.6B	 14J	18.57
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 2.11D	 0.173B	 6	 14D	 40	 24	 20
	0.1 - 0.3	 0.85D	 0.067B	 13	 17D	 37	 24	 22
	0.3 - 0.42	 0.47D	 0.063B	 4	 9D	 37	 25	 31
	0.42 - 0.6	 0.43D	 0.054B	 4	 7D	 32	 21	 44
	0.6 - 0.74	 0.03A	 0.33D	 26	 9D	 31	 19	 44
	0.74 - 1	 0.05A	 0.12D	 23	 7D	 30	 25	 39
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.3
	0.3 - 0.42
	0.42 - 0.6
	0.6 - 0.74
	0.74 - 1

	Project Name:	LSG
	Project Code:	LSG	Site ID:	CP83	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G_C_AL1	Exchangeable aluminium - meq per 100g of soil - Aluminium By difference of C and A or B
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance