Project Name:	LSG
	Project Code:	LSG	Site ID:	CP85	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	J.R. Sleeman	Locality:	N.side of Pialligs Ave:150M W. of culvert. site 6A:
	Date Desc.:	01/04/77	Elevation:	 650 metres
	Map Ref.:	Sheet No. : S155-16   1:250000	Rainfall:	640
	Northing/Long.:	149.233333333333	Runoff:	Slow
	Easting/Lat.:	-35.3166666666667	Drainage:	Poorly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Porous, Detrital 
	sedimentary rock (unidentified) 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Pediment	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Lithic Bleached Tenosol     	Principal Profile Form:	Uc2.31
	ASC Confidence:	Great Soil Group:	Podzol
	All necessary analytical data are available.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Tall Strata - Tree, , . *Species includes - Pinus species
	Surface Coarse Fragments:
	Profile Morphology
	A/C	0 - 0.01 m	Brown (10YR5/3-Moist); , 5YR48, 2-10% , Distinct; , 2-10% , Distinct; Loam; Massive grade of 
	structure; Sandy (grains prominent) fabric; Firm consistence; Field pH 5.5 (pH meter); Abrupt 
	change to - 
	2A1	0.07 - 0.12 m	Brown (10YR5/3-Moist); ; Sandy loam (Light); Massive grade of structure; Sandy (grains 
	prominent) fabric; Firm consistence; Field pH 5.3 (pH meter); Clear change to - 
	2A21	0.12 - 0.3 m	Very pale brown (10YR7/3-Moist); White (10YR8/1-Dry); ; Loamy sand; Massive grade of 
	structure; Sandy (grains prominent) fabric; Very weak consistence; 0-2%, fine gravelly, 2-
	6mm, rounded, dispersed, Detrital sedimentary rock (unidentified), coarse fragments; Very few 
	(0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; Field pH 5.9 (pH meter); Gradual 
	change to - 
	2A22	0.3 - 0.56 m	Pale brown (10YR6/3-Moist); White (10YR8/1-Dry); ; Loamy sand; Massive grade of structure; 
	Sandy (grains prominent) fabric; Very weak consistence; 2-10%, fine gravelly, 2-6mm, 
	rounded, dispersed, Detrital sedimentary rock (unidentified), coarse fragments; Few (2 - 10 %),
	 Ferromanganiferous, Medium (2 -6 mm), Nodules; Field pH 5.9 (pH meter); Gradual change to - 
	2B	0.56 - 0.73 m	Pale brown (10YR6/3-Moist); , 10YR56, 20-50% , Distinct; , 20-50% , Distinct; Loamy sand; 
	Massive grade of structure; Sandy (grains prominent) fabric; Very weak consistence; 10-20%, 
	medium gravelly, 6-20mm, rounded, dispersed, Detrital sedimentary rock (unidentified), coarse 
	fragments; Common (10 - 20 %), Ferromanganiferous, Coarse (6 - 20 mm), Nodules; Field pH 
	6.5 (pH meter); Gradual change to - 
	B21	0.73 - 0.9 m	Yellowish brown (10YR5/6-Moist); ; Sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Very weak consistence; 2-10%, medium gravelly, 6-20mm, rounded, 
	dispersed, Detrital sedimentary rock (unidentified), coarse fragments; Very few (0 - 2 %), 
	Ferromanganiferous, Coarse (6 - 20 mm), Nodules; Field pH 6.6 (pH meter); 
	Morphological Notes
	Observation Notes
	COLLUVIUM FROM ORDOVICIAN METASED'S:PITMAN FORMATION:                                                                   
	Site Notes
	C'BERRA A'PORT

	Project Name:	LSG
	Project Code:	LSG	Site ID:	CP85	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)

	Project Name:	LSG
	Project Code:	LSG	Site ID:	CP85	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.07	5.5A	 0.08A	 1.9K	 0.74	 0.23	 0.04	 5.2B	 8.1J	0.49
	0.07 - 0.12	5.3A	 0.1A	 2.7K	 0.75	 0.21	 0.06	 10.5B	 14.2J	0.42
	0.12 - 0.3	5.9A	 0.03A	 0.92K	 0.29	 0.05	 0.04	 0.7B	 2J	2.00
	0.3 - 0.56	5.9A	 0.01A	 0.6K	 0.93	 0.05	 0.06	 1.9B	 3.5J	1.71
	0.56 - 0.73	6.5A	 0.01A	 0.36K	 0.34	 0.04	 0.04	 0.2B	 1J	4.00
	0.73 - 0.9	6.6A	 0.01A	 0.83K	 0.48	 0.06	 0.05	 0.1B	 1.5J	3.33
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.07	 2.1D	 0.104B	 4	 62D	 20	 11	 8
	0.07 - 0.12	 2.73D	 0.128B	 1	 56D	 21	 11	 11
	0.12 - 0.3	 0.2D	 0.024B	 1	 46D	 33	 17	 5
	0.3 - 0.56	 0.11D	 0.016B	 3	 46D	 26	 18	 10
	0.56 - 0.73	 0.04D	 0.006B	 7	 65D	 22	 9	 4
	0.73 - 0.9	 0.03D	 0.006B	 1	 61D	 28	 6	 6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.07
	0.07 - 0.12
	0.12 - 0.3
	0.3 - 0.56
	0.56 - 0.73
	0.73 - 0.9

	Project Name:	LSG
	Project Code:	LSG	Site ID:	CP85	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G_C_AL1	Exchangeable aluminium - meq per 100g of soil - Aluminium By difference of C and A or B
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance