Project Name:	Improving Soil Survey Field Measurement and Interpretation. LWRRDC Project No. 90/R16
	Project Code:	Morphology	Site ID:	CP304	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	N.J. McKenzie	Locality:
	Date Desc.:	18/11/91	Elevation:	170 metres
	Map Ref.:	Sheet No. : 5932-3   1:50000	Rainfall:	No Data
	Northing/Long.:	6366700 AMG zone: 53	Runoff:	No Data
	Easting/Lat.:	514200  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Soil pit, 1.5 m deep,Porous, Calcarenite 
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Low hills
	10%
	Morph. Type:	Lower-slope	Relief:	50 metres
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):
	Erosion:	Minor or present (wind); 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Marly Lithocalcic Calcarosol     	Principal Profile Form:	Gc1.22
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.1 m	Dark brown (7.5YR3/2-Moist); , 0-0% ; Sandy loam; Massive grade of structure; Earthy fabric; 
	Dry; Weak consistence; Soil matrix is Moderately calcareous; Field pH 8 (Raupach); Many, very 
	fine (0-1mm) roots; Clear, Smooth change to - 
	A12	0.1 - 0.17 m	Dark brown (7.5YR3/2-Moist); Light brown (7.5YR6/4-Dry); , 0-0% ; Loam; Massive grade of 
	structure; Earthy fabric; Dry; Weak consistence; Soil matrix is Moderately calcareous; Field pH 
	8.5 (Raupach); Many, very fine (0-1mm) roots; Sharp, Smooth change to - 
	B21	0.17 - 0.35 m	Dark reddish brown (5YR3/4-Moist); , 0-0% ; Loam; Weak grade of structure, 100-200 mm, 
	Polyhedral; Rough-ped fabric; Dry; Firm consistence; Soil matrix is Highly calcareous; Field pH 
	8.5 (Raupach); Many, very fine (0-1mm) roots; Clear, Smooth change to - 
	B22k	0.35 - 0.47 m	Yellowish red (5YR4/6-Moist); , 0-0% ; Loam; Massive grade of structure; Rough-ped fabric; 
	Dry; Firm consistence; Very few (0 - 2 %), Calcareous, Medium (2 -6 mm), Nodules; Soil matrix 
	is Very highly calcareous; Field pH 9 (Raupach); Many, very fine (0-1mm) roots; Gradual, 
	Smooth change to - 
	B3k	0.47 - 0.7 m	Reddish yellow (7.5YR6/6-Moist); , 0-0% ; Clay loam; Massive grade of structure; Rough-ped 
	fabric; Dry; Firm consistence; Very many (50 - 100 %), Calcareous, Coarse (6 - 20 mm), 
	Nodules; Soil matrix is Very highly calcareous; Field pH 9 (Raupach); Many, very fine (0-1mm) 
	roots; Gradual, Smooth change to - 
	BC	0.7 - 0.85 m	Reddish yellow (7.5YR6/6-Moist); , 0-0% ; Clay loam; Massive grade of structure; Rough-ped 
	fabric; Dry; Firm consistence; Common (10 - 20 %), Calcareous, Coarse (6 - 20 mm), Nodules; 
	Soil matrix is Very highly calcareous; Field pH 9.5 (Raupach); Few, very fine (0-1mm) roots; 
	Diffuse, Irregular change to - 
	C	0.85 - 1.3 m	Pink (7.5YR8/4-Moist); , 0-0% ; Light clay; Massive grade of structure; Rough-ped fabric; Dry; 
	Firm consistence; Few (2 - 10 %), Calcareous, Medium (2 -6 mm), Soft segregations; Soil matrix
	 is Very highly calcareous; Field pH 9.5 (Raupach); 
	Morphological Notes
	Observation Notes
	Site Notes
	Minnipa, Ag Research Centre (Morph 3)

	Project Name:	Improving Soil Survey Field Measurement and Interpretation. LWRRDC Project No. 90/R16
	Project Code:	Morphology	Site ID:	CP304	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)

	Project Name:	Improving Soil Survey Field Measurement and Interpretation. LWRRDC Project No. 90/R16
	Project Code:	Morphology	Site ID:	CP304	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8.64A	0.24A	7.9B	1.3	2.7	0.3	9.8A	3.06
	0 - 0.17
	0 - 0.17
	0.1 - 0.17	8.66A	0.17A	9.5B	1.6	2.1	0.36	13.1A	2.75
	0.17 - 0.35	8.63A	0.16A	10.9B	2.7	1.8	0.22	13.3A	1.65
	0.17 - 0.35	8.63A	0.16A	10.9B	2.7	1.8	0.22	13.3A	1.65
	0.17 - 0.35	8.63A	0.16A	10.9B	2.7	1.8	0.22	13.3A	1.65
	0.35 - 0.47	8.85A	0.14A	10.6B	3.8	0.92	0.42	12.9A	3.26
	0.47 - 0.7	9.32A	0.32A	6.2B	3.9	0.57	1.9	10.4A	18.27
	0.7 - 0.85	9.35A	0.79A	3.3B	4	0.74	3.1	9.5A	32.63
	0.85 - 1.3	9.72A	1.26A	1.2B	3.4	0.99	5.2	6.7A	77.61
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.16B	0.93B	0
	0 - 0.17	1.54
	1.54
	1.56
	1.58
	0 - 0.17	1.54
	1.54
	1.56
	1.58
	0.1 - 0.17	0.9B	1.1B	1.58	0
	0.17 - 0.35	0.61B	0.42B	1.56	0
	1.43
	1.44
	1.54
	1.51
	0.17 - 0.35	0.61B	0.42B	1.56	0
	1.43
	1.44
	1.54
	1.51
	0.17 - 0.35	0.61B	0.42B	1.56	0
	1.43
	1.44
	1.54
	1.51
	0.35 - 0.47	4.66B	0.29B	0
	0.47 - 0.7	26.5B	0.01B	0
	0.7 - 0.85	27.9B	0.27B	14
	0.85 - 1.3	42.9B	0.01B	16
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1

	Project Name:	Improving Soil Survey Field Measurement and Interpretation. LWRRDC Project No. 90/R16
	Project Code:	Morphology	Site ID:	CP304	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	0 - 0.17	0.37E	0.31E	0.24E	0.18D	0.12F	0.09F	135.6D	33.4A
	0.38E	0.32E	0.23E	0.17D	0.11F	0.08F
	0.36E	0.32E	0.22E	0.21D
	0.37E	0.34E	0.22E	0.21D
	0 - 0.17	0.37E	0.31E	0.24E	0.18D	0.12F	0.09F	135.6D	33.4A
	0.38E	0.32E	0.23E	0.17D	0.11F	0.08F
	0.36E	0.32E	0.22E	0.21D
	0.37E	0.34E	0.22E	0.21D
	0.1 - 0.17	0.008B
	0.17 - 0.35	0.008B	0.41E	0.35E	0.28E	0.27D	0.17F	0.14F	116D	36.9A
	0.41E	0.35E	0.29E	0.28D	0.12F	0.11F
	0.35E	0.3E	0.25E	0.19D
	0.37E	0.32E	0.26E	0.19D
	0.17 - 0.35	0.008B	0.41E	0.35E	0.28E	0.27D	0.17F	0.14F	116D	36.9A
	0.41E	0.35E	0.29E	0.28D	0.12F	0.11F
	0.35E	0.3E	0.25E	0.19D
	0.37E	0.32E	0.26E	0.19D
	0.17 - 0.35	0.008B	0.41E	0.35E	0.28E	0.27D	0.17F	0.14F	116D	36.9A
	0.41E	0.35E	0.29E	0.28D	0.12F	0.11F
	0.35E	0.3E	0.25E	0.19D
	0.37E	0.32E	0.26E	0.19D
	0.35 - 0.47
	0.47 - 0.7
	0.7 - 0.85
	0.85 - 1.3

	Project Name:	Improving Soil Survey Field Measurement and Interpretation. LWRRDC Project No. 90/R16
	Project Code:	Morphology	Site ID:	CP304	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	19B1	Carbonates - manometric
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	P10_GRAV	Gravel (%)
	P10_S_0.20	0.20 micron (cumulative %) - Sedigraph
	P10_S_0.48	0.48 micron (cumulative %) - Sedigraph
	P10_S_1	1 micron (cumulative %) - Sedigraph
	P10_S_1000	1000 micron (cumulative %) - Sedigraph
	P10_S_125	125 micron (cumulative %) - Sedigraph
	P10_S_15.6	15.6 micron (cumulative %) - Sedigraph
	P10_S_2	2 micron (cumulative %) - Sedigraph
	P10_S_20	20 micron (cumulative %) - Sedigraph
	P10_S_2000	2000 micron (cumulative %) - Sedigraph
	P10_S_250	250 micron (cumlative %) - Sedigraph
	P10_S_3.9	3.9 micron (cumulative %) - Sedigraph
	P10_S_31.2	31.2 micron (cumulative %) - Sedigraph
	P10_S_500	500 micron (cumulative %) - Sedigraph
	P10_S_53	53 micron (cumulative %) - Sedigraph
	P10_S_63	63 micron (cumulative %) - Sedigraph
	P10_S_7.8	7.8 micron (cumulative %) - Sedigraph
	P3A1	Bulk density - g/cm3
	P3B2VL_15	15 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B2VL_5	5 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B3VLb001	0.01 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLb003	0.03 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLb005	0.05 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLb01	0.1 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLb05	0.5 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLbSAT	Saturated Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P4_50_McK	Unsaturated Hydraulic Conductivity - 50mm potential (CSIRO Div of Soil, DR 125, McKenzie and 
	Jacquier, 1996)
	P4_sat_McK	Saturated Hydraulic Conductivity (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 1996)
	P5_LS_MOD	Modified linear shrinkage (McKenzie, Jacquier and Ringrose-Voase, AJSR, 1994, 32, 931-8)