Project Name:	Improving Soil Survey Field Measurement and Interpretation. LWRRDC Project No. 90/R16
	Project Code:	Morphology	Site ID:	CP305	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	N.J. McKenzie	Locality:
	Date Desc.:	19/11/91	Elevation:	No Data
	Map Ref.:	1:250000	Rainfall:	No Data
	Northing/Long.:	134.733	Runoff:	No Data
	Easting/Lat.:	-32.667	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	3 % 	Aspect:	315 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:	Minor or present (wind); 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Supravescent Regolithic Hypercalcic Calcarosol Thin Non-	Principal Profile Form:	Uc5.12
	gravelly Loamy Loamy Very deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Brown (10YR4/3-Moist); , 0-0% ; Sandy loam; Massive grade of structure; Earthy fabric; Dry; 
	Very weak consistence; Soil matrix is Highly calcareous; Field pH 9 (Raupach); Many, very fine 
	(0-1mm) roots; Sharp, Smooth change to - 
	B11	0.1 - 0.2 m	Brown (7.5YR5/4-Moist); , 0-0% ; Sandy loam; Massive grade of structure; Earthy fabric; Dry; 
	Weak consistence; Very few (0 - 2 %), Calcareous, Medium (2 -6 mm), Nodules; Soil matrix is 
	Highly calcareous; Field pH 9 (Raupach); Common, very fine (0-1mm) roots; Diffuse, Smooth 
	change to - 
	B12	0.2 - 0.3 m	Brown (7.5YR5/4-Moist); , 0-0% ; Sandy loam; Massive grade of structure; Earthy fabric; Dry; 
	Weak consistence; Very few (0 - 2 %), Calcareous, Coarse (6 - 20 mm), Nodules; Soil matrix is 
	Highly calcareous; Field pH 9 (Raupach); Common, very fine (0-1mm) roots; Diffuse, Smooth 
	change to - 
	B21	0.3 - 0.5 m	Brown (7.5YR5/4-Moist); , 0-0% ; Sandy loam; Massive grade of structure; Earthy fabric; Dry; 
	Weak consistence; Very few (0 - 2 %), Calcareous, Coarse (6 - 20 mm), Nodules; Soil matrix is 
	Highly calcareous; Field pH 9 (Raupach); Few, very fine (0-1mm) roots; Diffuse, Smooth 
	change to - 
	B22	0.5 - 0.8 m	Brown (7.5YR5/4-Moist); , 0-0% ; Sandy loam; Massive grade of structure; Earthy fabric; Dry; 
	Weak consistence; Very few (0 - 2 %), Calcareous, Coarse (6 - 20 mm), Nodules; Soil matrix is 
	Highly calcareous; Field pH 9 (Raupach); Few, very fine (0-1mm) roots; Diffuse, Smooth 
	change to - 
	B23	0.8 - 1.2 m	Reddish yellow (7.5YR6/6-Moist); , 0-0% ; Sandy loam; Massive grade of structure; Earthy 
	fabric; Dry; Weak consistence; Very few (0 - 2 %), Calcareous, Coarse (6 - 20 mm), Nodules; 
	Soil matrix is Highly calcareous; Field pH 9 (Raupach); Abrupt, Smooth change to - 
	B3	1.2 - 1.25 m	Reddish yellow (7.5YR6/6-Moist); , 0-0% ; Sandy loam; Massive grade of structure; Earthy 
	fabric; Dry; Weak consistence; Many (20 - 50 %), Calcareous, Very coarse (20 - 60 mm), 
	Nodules; Soil matrix is Highly calcareous; Field pH 9 (Raupach); Clear, Smooth change to - 
	B4	1.25 - 1.5 m	Reddish yellow (7.5YR6/6-Moist); , 0-0% ; Sandy loam; Massive grade of structure; Earthy 
	fabric; Dry; Weak consistence; Very few (0 - 2 %), Calcareous, Coarse (6 - 20 mm), Nodules; 
	Soil matrix is Highly calcareous; Field pH 9 (Raupach); 
	Morphological Notes
	B3	Calcrete rubble much shallower at Nundroo.

	Project Name:	Improving Soil Survey Field Measurement and Interpretation. LWRRDC Project No. 90/R16
	Project Code:	Morphology	Site ID:	CP305	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Observation Notes
	Cereal crop (barley) cut two months prior.
	Site Notes
	Cungena S.A. !20km east of Ceduna (Morph 4)

	Project Name:	Improving Soil Survey Field Measurement and Interpretation. LWRRDC Project No. 90/R16
	Project Code:	Morphology	Site ID:	CP305	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8.69A	0.2A	7.6B	1.1	1.1	0.15	6A	2.50
	0 - 0.17
	0 - 0.17
	0.1 - 0.2	8.88A	0.16A	8.1B	1.4	1.1	0.2	6.6A	3.03
	0.2 - 0.3	9.04A	0.15A	5B	1.8	0.82	0.21	5.1A	4.12
	0.3 - 0.5	9.18A	0.23A	2.9B	3.1	0.88	0.39	4.2A	9.29
	0.3 - 0.47
	0.3 - 0.47
	0.5 - 0.8	10.03A	0.7A	0.99B	2.2	1.4	2.8	3.8A	73.68
	0.8 - 1.2	9.84A	1.13A	0.67B	1.3	1.1	3.2	3A	106.67
	1.2 - 1.35	9.58A	1.15A	0.76B	1.2	0.81	2.8	1.9A	147.37
	1.35 - 1.5	9.6A	0.97A	0.69B	1	0.72	2.3	1.8A	127.78
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	59.8B	1B	1
	0 - 0.17	1.28
	1.28
	1.25
	1.32
	0 - 0.17	1.28
	1.28
	1.25
	1.32
	0.1 - 0.2	63.4B	0.74B	1.22	0
	0.2 - 0.3	64.8B	0.4B	0
	0.3 - 0.5	66.4B	0.25B	1.25	5
	0.3 - 0.47	1.28
	1.41
	1.30
	1.31
	0.3 - 0.47	1.28
	1.41
	1.30
	1.31
	0.5 - 0.8	70B	0.37B	0
	0.8 - 1.2	73.6B	0.04B	0
	1.2 - 1.35	79.4B	0.01B	32
	1.35 - 1.5	78.7B	0.01B	14
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0 - 0.17	0.51E	0.45E	0.31E	0.23D	0.17F	0.13F	178.6D	74.7A
	0.5E	0.45E	0.3E	0.22D	0.16F	0.14F
	0.52E	0.46E	0.31E	0.21D
	0.49E	0.43E	0.29E	0.19D

	Project Name:	Improving Soil Survey Field Measurement and Interpretation. LWRRDC Project No. 90/R16
	Project Code:	Morphology	Site ID:	CP305	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	0 - 0.17	0.51E	0.45E	0.31E	0.23D	0.17F	0.13F	178.6D	74.7A
	0.5E	0.45E	0.3E	0.22D	0.16F	0.14F
	0.52E	0.46E	0.31E	0.21D
	0.49E	0.43E	0.29E	0.19D
	0.1 - 0.2	0B
	0.2 - 0.3
	0.3 - 0.5	0B
	0.3 - 0.47	0.42E	0.37E	0.29E	0.19D	0.17F	0.13F	194.4D	78.8A
	0.46E	0.41E	0.33E	0.22D	0.16F	0.13F
	0.45E	0.39E	0.31E	0.29D
	0.45E	0.36E	0.29E	0.2D
	0.3 - 0.47	0.42E	0.37E	0.29E	0.19D	0.17F	0.13F	194.4D	78.8A
	0.46E	0.41E	0.33E	0.22D	0.16F	0.13F
	0.45E	0.39E	0.31E	0.29D
	0.45E	0.36E	0.29E	0.2D
	0.5 - 0.8
	0.8 - 1.2
	1.2 - 1.35
	1.35 - 1.5

	Project Name:	Improving Soil Survey Field Measurement and Interpretation. LWRRDC Project No. 90/R16
	Project Code:	Morphology	Site ID:	CP305	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	19B1	Carbonates - manometric
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	P10_GRAV	Gravel (%)
	P10_S_0.20	0.20 micron (cumulative %) - Sedigraph
	P10_S_0.48	0.48 micron (cumulative %) - Sedigraph
	P10_S_1	1 micron (cumulative %) - Sedigraph
	P10_S_1000	1000 micron (cumulative %) - Sedigraph
	P10_S_125	125 micron (cumulative %) - Sedigraph
	P10_S_15.6	15.6 micron (cumulative %) - Sedigraph
	P10_S_2	2 micron (cumulative %) - Sedigraph
	P10_S_20	20 micron (cumulative %) - Sedigraph
	P10_S_2000	2000 micron (cumulative %) - Sedigraph
	P10_S_250	250 micron (cumlative %) - Sedigraph
	P10_S_3.9	3.9 micron (cumulative %) - Sedigraph
	P10_S_31.2	31.2 micron (cumulative %) - Sedigraph
	P10_S_500	500 micron (cumulative %) - Sedigraph
	P10_S_53	53 micron (cumulative %) - Sedigraph
	P10_S_63	63 micron (cumulative %) - Sedigraph
	P10_S_7.8	7.8 micron (cumulative %) - Sedigraph
	P3A1	Bulk density - g/cm3
	P3B2VL_15	15 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B2VL_5	5 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B3VLb001	0.01 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLb003	0.03 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLb005	0.05 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLb01	0.1 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLb05	0.5 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLbSAT	Saturated Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P4_50_McK	Unsaturated Hydraulic Conductivity - 50mm potential (CSIRO Div of Soil, DR 125, McKenzie and 
	Jacquier, 1996)
	P4_sat_McK	Saturated Hydraulic Conductivity (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 1996)
	P5_LS_MOD	Modified linear shrinkage (McKenzie, Jacquier and Ringrose-Voase, AJSR, 1994, 32, 931-8)