Project Name:	Improving Soil Survey Field Measurement and Interpretation. LWRRDC Project No. 90/R16
	Project Code:	Morphology	Site ID:	CP315	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	N.J. McKenzie	Locality:
	Date Desc.:	28/07/92	Elevation:	No Data
	Map Ref.:	1:250000	Rainfall:	1200
	Northing/Long.:	151.217	Runoff:	Very slow
	Easting/Lat.:	-33.183	Drainage:	Rapidly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Brown Kandosol Medium Non-gravelly 	Principal Profile Form:	Gn2.22
	Loamy Clay-loamy Deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - None recorded
	Mid Strata - Tree, 6.01-12m, Sparse. *Species includes - None recorded
	Tall Strata - Tree, 20.01-35m, Sparse. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.04 m	Brown (10YR5/3-Moist); Biological mixing, 10YR32, 20-50% , Faint; Sandy loam; Weak grade of 
	structure, 10-20 mm, Subangular blocky; Earthy fabric; Moderately moist; Very weak 
	consistence; Field pH 5 (Raupach); Abundant, medium (2-5mm) roots; Abrupt, Smooth change 
	A12	0.04 - 0.1 m	Brown (10YR4/3-Moist); Biological mixing, 10YR42, 20-50% , 5-15mm, Faint; Sandy loam; Weak 
	grade of structure, 10-20 mm, Subangular blocky; Earthy fabric; Moderately moist; Weak 
	consistence; Field pH 6.5 (Raupach); Many, medium (2-5mm) roots; Clear, Smooth change to - 
	A3	0.1 - 0.2 m	Brown (10YR4/3-Moist); Biological mixing, 7.5YR68, 20-50% , 5-15mm, Distinct; Sandy loam; 
	Weak grade of structure, 10-20 mm, Subangular blocky; Earthy fabric; Moderately moist; Weak 
	consistence; Field pH 6.5 (Raupach); Common, medium (2-5mm) roots; Gradual, Smooth change
	 to - 
	B1	0.2 - 0.3 m	Strong brown (7.5YR5/8-Moist); Biological mixing, 10YR53, 20-50% , 5-15mm, Distinct; Sandy 
	clay loam; Massive grade of structure; Earthy fabric; Moist; Weak consistence; Field pH 6.5 
	(Raupach); Common, medium (2-5mm) roots; Diffuse, Smooth change to - 
	B21	0.3 - 0.5 m	Strong brown (7.5YR5/8-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 
	Moist; Very weak consistence; Field pH 6.5 (Raupach); Few, fine (1-2mm) roots; 
	B21	0.5 - 0.7 m	Strong brown (7.5YR5/8-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 
	Moist; Very weak consistence; Field pH 6 (Raupach); Few, fine (1-2mm) roots; Diffuse, Smooth
	 change to - 
	B22	0.7 - 1 m	Strong brown (7.5YR5/8-Moist); Mottles, 5YR58, 20-50% , 5-15mm, Faint; Sandy clay loam; 
	Massive grade of structure; Earthy fabric; Moist; Very weak consistence; Field pH 6 (Raupach);
	 Few, fine (1-2mm) roots; Diffuse, Smooth change to - 
	B3	1 - 1.4 m	Reddish yellow (7.5YR6/8-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 
	Moist; Very weak consistence; Very few (0 - 2 %), Ferruginous, Coarse (6 - 20 mm), 
	Concretions; Field pH 6 (Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes

	Project Name:	Improving Soil Survey Field Measurement and Interpretation. LWRRDC Project No. 90/R16
	Project Code:	Morphology	Site ID:	CP315	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Notes
	Kulnura  (Morph 14)
	Regolith depth >3m and is Hawkesbury Sandstone. A few ant mounds at site. Very old surface (miocene) on an undulating 
	part of the somersby plateau.

	Project Name:	Improving Soil Survey Field Measurement and Interpretation. LWRRDC Project No. 90/R16
	Project Code:	Morphology	Site ID:	CP315	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	4.7A	0.06A	1.3B	0.61	0.09	0.03	6.3A	0.48
	0 - 0.2
	0 - 0.2
	0.04 - 0.1	5.09A	0.03A	0.29B	0.29	0.05	0.04	3.2A	1.25
	0.1 - 0.2	5.36A	0.02A	0.37B	0.37	0.05	0.04	2.5A	1.60
	0.2 - 0.3	5.4A	0.02A	0.36B	0.38	0.04	0.04	2.1A	1.90
	0.2 - 0.4
	0.2 - 0.4
	0.3 - 0.5	5.36A	0.01A	0.22B	0.31	0.05	0.05	1.7A	2.94
	0.5 - 0.7	5.25A	0.01A	0.17B	0.36	0.05	0.05	1.4A	3.57
	0.7 - 1	5.45A	0.01A	0.17B	0.61	0.04	1.4A
	0.7 - 0.9
	0.7 - 0.9
	1 - 1.4	5.37A	0.01A	0.11B	0.67	0.06	1.4A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	2.7B	0
	0 - 0.2	1.53
	1.49
	1.36
	1.42
	0 - 0.2	1.53
	1.49
	1.36
	1.42
	0.04 - 0.1	1.3B	1.27	0
	0.1 - 0.2	0.74B	0
	0.2 - 0.3	0.54B	1.51	0
	0.2 - 0.4	1.68
	1.63
	1.54
	1.59
	0.2 - 0.4	1.68
	1.63
	1.54
	1.59
	0.3 - 0.5	0.32B	0
	0.5 - 0.7	0.21B	0
	0.7 - 1	0.16B	1.39	0
	0.7 - 0.9	1.36
	1.45
	1.39
	1.41
	0.7 - 0.9	1.36
	1.45
	1.39
	1.41
	1 - 1.4	0.12B	3
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat

	Project Name:	Improving Soil Survey Field Measurement and Interpretation. LWRRDC Project No. 90/R16
	Project Code:	Morphology	Site ID:	CP315	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0 - 0.2	0.4E	0.33E	0.29E	0.21D	0.1F	0.09F	176D	107.7A
	0.39E	0.3E	0.27E	0.19D	0.09F	0.08F
	0.39E	0.3E	0.27E	0.19D
	0.4E	0.32E	0.28E	0.2D
	0 - 0.2	0.4E	0.33E	0.29E	0.21D	0.1F	0.09F	176D	107.7A
	0.39E	0.3E	0.27E	0.19D	0.09F	0.08F
	0.39E	0.3E	0.27E	0.19D
	0.4E	0.32E	0.28E	0.2D
	0.04 - 0.1	0B
	0.1 - 0.2
	0.2 - 0.3	0.004B
	0.2 - 0.4	0.32E	0.24E	0.21E	0.16D	0.12F	0.1F	69.9D	26.1A
	0.3E	0.24E	0.21E	0.16D	0.12F	0.11F
	0.36E	0.29E	0.26E	0.2D
	0.35E	0.24E	0.21E	0.16D
	0.2 - 0.4	0.32E	0.24E	0.21E	0.16D	0.12F	0.1F	69.9D	26.1A
	0.3E	0.24E	0.21E	0.16D	0.12F	0.11F
	0.36E	0.29E	0.26E	0.2D
	0.35E	0.24E	0.21E	0.16D
	0.3 - 0.5
	0.5 - 0.7
	0.7 - 1	0.004B
	0.7 - 0.9	0.43E	0.27E	0.22E	0.17D	0.13F	0.12F	352.9D	82.6A
	0.41E	0.28E	0.23E	0.18D	0.13F	0.12F
	0.39E	0.26E	0.22E	0.16D
	0.4E	0.27E	0.22E	0.17D
	0.7 - 0.9	0.43E	0.27E	0.22E	0.17D	0.13F	0.12F	352.9D	82.6A
	0.41E	0.28E	0.23E	0.18D	0.13F	0.12F
	0.39E	0.26E	0.22E	0.16D
	0.4E	0.27E	0.22E	0.17D
	1 - 1.4

	Project Name:	Improving Soil Survey Field Measurement and Interpretation. LWRRDC Project No. 90/R16
	Project Code:	Morphology	Site ID:	CP315	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	P10_GRAV	Gravel (%)
	P10_S_0.20	0.20 micron (cumulative %) - Sedigraph
	P10_S_1000	1000 micron (cumulative %) - Sedigraph
	P10_S_125	125 micron (cumulative %) - Sedigraph
	P10_S_2	2 micron (cumulative %) - Sedigraph
	P10_S_20	20 micron (cumulative %) - Sedigraph
	P10_S_2000	2000 micron (cumulative %) - Sedigraph
	P10_S_250	250 micron (cumlative %) - Sedigraph
	P10_S_31.2	31.2 micron (cumulative %) - Sedigraph
	P10_S_500	500 micron (cumulative %) - Sedigraph
	P10_S_63	63 micron (cumulative %) - Sedigraph
	P3A1	Bulk density - g/cm3
	P3B2VL_15	15 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B2VL_5	5 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B3VLb001	0.01 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLb003	0.03 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLb005	0.05 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLb01	0.1 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLb05	0.5 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLbSAT	Saturated Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P4_50_McK	Unsaturated Hydraulic Conductivity - 50mm potential (CSIRO Div of Soil, DR 125, McKenzie and 
	Jacquier, 1996)
	P4_sat_McK	Saturated Hydraulic Conductivity (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 1996)
	P5_LS_MOD	Modified linear shrinkage (McKenzie, Jacquier and Ringrose-Voase, AJSR, 1994, 32, 931-8)