Project Name:	Improving Soil Survey Field Measurement and Interpretation. LWRRDC Project No. 90/R16
	Project Code:	Morphology	Site ID:	CP334	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	N.J. McKenzie	Locality:
	Date Desc.:	06/12/93	Elevation:	5 metres
	Map Ref.:	Sheet No. : 9435-1-N   1:25000	Rainfall:	No Data
	Northing/Long.:	6566700 AMG zone: 56	Runoff:	Slow
	Easting/Lat.:	494400  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Soil pit, 1.5 m deep,Slightly porous, Silt 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Covered plain
	3%
	Morph. Type:	Flat	Relief:	3 metres
	Elem. Type:	Levee	Slope Category:	Very gently sloped
	Slope:	1.5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Grey Kandosol     	Principal Profile Form:	Um6.14
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:	Low Strata - Sod grass, <0.25m, Closed or dense. *Species includes - None recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.05 m	Very dark greyish brown (10YR3/2-Moist); ; Silty clay loam; Moderate grade of structure, 5-10 
	mm, Cast; Rough-ped fabric; Moist; Field pH 6 (pH meter); Abundant, medium (2-5mm) roots; 
	Clear, Smooth change to - 
	A12	0.05 - 0.15 m	Very dark greyish brown (10YR3/2-Moist); ; Silty clay loam; Moderate grade of structure, 5-10 
	mm, Cast; Rough-ped fabric; Moderately moist; Field pH 6 (pH meter); Many, fine (1-2mm) roots; 
	Diffuse, Smooth change to - 
	A3	0.15 - 0.32 m	Very dark greyish brown (10YR3/2-Moist); , 10YR42, 10-20% , 5-15mm, Faint; Silty clay loam; 
	Weak grade of structure, 10-20 mm, Polyhedral; Rough-ped fabric; Moderately moist; Field pH 6 
	(pH meter); Many, fine (1-2mm) roots; Gradual, Smooth change to - 
	B2	0.32 - 0.61 m	Dark greyish brown (10YR4/2-Moist); ; Silty clay loam; Weak grade of structure, 20-50 mm, 
	Polyhedral; Weak grade of structure, 20-50 mm, Polyhedral; Rough-ped fabric; Moderately 
	moist; Field pH 6 (pH meter); Common, fine (1-2mm) roots; Clear, Smooth change to - 
	B31	0.61 - 0.9 m	Brown (10YR4/3-Moist); , 10YR51, 20-50% , 5-15mm, Faint; Light clay; Weak grade of 
	structure, 20-50 mm, Polyhedral; Rough-ped fabric; Moderately moist; Field pH 6 (pH meter); 
	Few, fine (1-2mm) roots; Diffuse, Smooth change to - 
	B32	0.9 - 1.3 m	Brown (10YR4/3-Moist); , 10YR51, 20-50% , 15-30mm, Distinct; Light clay; Weak grade of 
	structure, 20-50 mm, Polyhedral; Rough-ped fabric; Moderately moist; Field pH 6 (pH meter); 
	Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Substrate Genetic Type AL (Alluvium) and strength E (Earth).  Abundant worms throughout.
	Site Notes
	Austral Eden, Kempsey.  Thick Kikuya pasture. (Morph 33)

	Project Name:	Improving Soil Survey Field Measurement and Interpretation. LWRRDC Project No. 90/R16
	Project Code:	Morphology	Site ID:	CP334	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	Cmol (+)/kg 
	0 - 0.05	5.5A	0.36A	7B	3.4	1.6	0.07	15.1A	0.46
	0.05 - 0.15	5.78A	0.1A	5.9B	2.4	0.68	0.06	11.3A	0.53
	0.1 - 0.3
	0.1 - 0.3
	0.15 - 0.32	5.94A	0.05A	5.5B	2.1	0.34	0.19	10A	1.90
	0.32 - 0.61	6.19A	0.04A	8.7B	2.9	0.24	0.22	12.2A	1.80
	0.4 - 0.6
	0.4 - 0.6
	0.61 - 0.9	6.5A	0.03A	8.9B	3.2	0.15	0.16	11.4A	1.40
	0.65 - 0.85
	0.65 - 0.85
	0.9 - 1.3	6.27A	0.03A	5.5B	2.8	0.13	0.25	11.4A	2.19
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	4.03B	0
	0.05 - 0.15	2.21B	1.08	0
	0.1 - 0.3	1.28
	1.30
	1.29
	1.22
	0.1 - 0.3	1.28
	1.30
	1.29
	1.22
	0.15 - 0.32	1.37B	0
	0.32 - 0.61	1.14B	1.38	0
	0.4 - 0.6	1.23
	1.18
	1.29
	1.25
	0.4 - 0.6	1.23
	1.18
	1.29
	1.25
	0.61 - 0.9	0.63B	1.38	0
	0.65 - 0.85	1.32
	1.36
	1.40
	1.37
	0.65 - 0.85	1.32
	1.36
	1.40
	1.37
	0.9 - 1.3	0.42B	1.38	0
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	 m	 dS/m	%
	Project Name:	Improving Soil Survey Field Measurement and Interpretation. LWRRDC Project No. 90/R16
	Project Code:	Morphology	Site ID:	CP334	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	0.05 - 0.15	0.025B
	0.1 - 0.3	0.47E	0.41E	0.39E	0.35D	0.21F	0.15F	2927D	68.1A
	0.44E	0.39E	0.37E	0.34D	0.21F	0.16F
	0.46E	0.41E	0.39E	0.33D
	0.45E	0.4E	0.38E	0.33D
	0.1 - 0.3	0.47E	0.41E	0.39E	0.35D	0.21F	0.15F	2927D	68.1A
	0.44E	0.39E	0.37E	0.34D	0.21F	0.16F
	0.46E	0.41E	0.39E	0.33D
	0.45E	0.4E	0.38E	0.33D
	0.15 - 0.32
	0.32 - 0.61	0.029B
	0.4 - 0.6	0.42E	0.37E	0.35E	0.31D	0.23F	0.15F	4682D	61.7A
	0.39E	0.34E	0.32E	0.29D	0.24F	0.16F
	0.43E	0.38E	0.36E	0.33D
	0.44E	0.38E	0.36E	0.32D
	0.4 - 0.6	0.42E	0.37E	0.35E	0.31D	0.23F	0.15F	4682D	61.7A
	0.39E	0.34E	0.32E	0.29D	0.24F	0.16F
	0.43E	0.38E	0.36E	0.33D
	0.44E	0.38E	0.36E	0.32D
	0.61 - 0.9	0.038B
	0.65 - 0.85	0.42E	0.37E	0.36E	0.33D	0.24F	0.15F	2705D	11.2A
	0.42E	0.37E	0.36E	0.33D	0.25F	0.16F
	0.43E	0.39E	0.38E	0.35D
	0.42E	0.38E	0.36E	0.34D
	0.65 - 0.85	0.42E	0.37E	0.36E	0.33D	0.24F	0.15F	2705D	11.2A
	0.42E	0.37E	0.36E	0.33D	0.25F	0.16F
	0.43E	0.39E	0.38E	0.35D
	0.42E	0.38E	0.36E	0.34D
	0.9 - 1.3

	Project Name:	Improving Soil Survey Field Measurement and Interpretation. LWRRDC Project No. 90/R16
	Project Code:	Morphology	Site ID:	CP334	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	P10_GRAV	Gravel (%)
	P10_S_0.20	0.20 micron (cumulative %) - Sedigraph
	P10_S_0.48	0.48 micron (cumulative %) - Sedigraph
	P10_S_1	1 micron (cumulative %) - Sedigraph
	P10_S_1000	1000 micron (cumulative %) - Sedigraph
	P10_S_125	125 micron (cumulative %) - Sedigraph
	P10_S_15.6	15.6 micron (cumulative %) - Sedigraph
	P10_S_2	2 micron (cumulative %) - Sedigraph
	P10_S_20	20 micron (cumulative %) - Sedigraph
	P10_S_2000	2000 micron (cumulative %) - Sedigraph
	P10_S_250	250 micron (cumlative %) - Sedigraph
	P10_S_3.9	3.9 micron (cumulative %) - Sedigraph
	P10_S_31.2	31.2 micron (cumulative %) - Sedigraph
	P10_S_500	500 micron (cumulative %) - Sedigraph
	P10_S_53	53 micron (cumulative %) - Sedigraph
	P10_S_63	63 micron (cumulative %) - Sedigraph
	P10_S_7.8	7.8 micron (cumulative %) - Sedigraph
	P3A1	Bulk density - g/cm3
	P3B2VL_15	15 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B2VL_5	5 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B3VLb001	0.01 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLb003	0.03 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLb005	0.05 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLb01	0.1 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLb05	0.5 BAR Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P3B3VLbSAT	Saturated Moisture m3/m3 - Volumetric using undisturbed 73mm diameter and 75mm height core on 
	suction plate taken from center of large core (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 
	1996)
	P4_50_McK	Unsaturated Hydraulic Conductivity - 50mm potential (CSIRO Div of Soil, DR 125, McKenzie and 
	Jacquier, 1996)
	P4_sat_McK	Saturated Hydraulic Conductivity (CSIRO Div of Soil, DR 125, McKenzie and Jacquier, 1996)
	P5_LS_MOD	Modified linear shrinkage (McKenzie, Jacquier and Ringrose-Voase, AJSR, 1994, 32, 931-8)