Project Name:	SOIL STRUCTURE & MANAGEMENT             
	Project Code:	SSM	Site ID:	SSM206	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	B. Murphy	Locality:
	Date Desc.:	12/03/92	Elevation:	215 metres
	Map Ref.:	Sheet No. : 8327   1:100000	Rainfall:	No Data
	Northing/Long.:	6085400 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	505900  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	1 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy2.41
	ASC Confidence:	Great Soil Group:	Yellow podzolic 
	Confidence level not specified	soil
	Site Disturbance:	Cultivation. Rainfed, Extensive clearing, for example poisoning, ringbarking, 
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.14 m	Brown (7.5YR5/4-Moist); ; Loam; Weak grade of structure, 20-50 mm, Subangular blocky; 50-
	100 mm, Prismatic; Earthy fabric; Dry; Very weak consistence; Non-plastic; Normal plasticity; 
	Non-sticky; Field pH 5.5 (Raupach); Many, very fine (0-1mm) roots; 
	A21	0.14 - 0.27 m	Yellowish red (5YR5/6-Moist); ; Fine sandy loam; Massive grade of structure; Earthy fabric; 
	Dry; Non-plastic; Normal plasticity; Non-sticky; Field pH 6 (Raupach); Few, very fine (0-1mm) 
	A22	0.27 - 0.36 m	Pink (7.5YR7/4-Moist); Substrate influence, 0-2% , Faint; Fine sandy loam; Massive grade of 
	structure; Earthy fabric; Dry; Non-plastic; Normal plasticity; Non-sticky; Field pH 7 (Raupach); 
	Few, very fine (0-1mm) roots; 
	B21	0.36 - 0.5 m	Reddish yellow (7.5YR6/6-Moist); ; Medium clay; Strong grade of structure, 20-50 mm, 
	Prismatic; 50-100 mm, Angular blocky; Smooth-ped fabric; Dry; Moderately plastic; Normal 
	plasticity; Moderately sticky; Many cutans, >50% of ped faces or walls coated, faint; Field pH 
	6.5 (Raupach); Few, very fine (0-1mm) roots; 
	B22	0.5 - 0.7 m	Strong brown (7.5YR5/6-Moist); ; Medium clay; Strong grade of structure, 20-50 mm, Prismatic; 
	50-100 mm, Angular blocky; Smooth-ped fabric; Dry; Moderately plastic; Normal plasticity; 
	Moderately sticky; Many cutans, >50% of ped faces or walls coated, faint; Field pH 6 
	(Raupach); Few, very fine (0-1mm) roots; 
	B23	0.7 - 1 m	Strong brown (7.5YR5/6-Moist); Substrate influence, 2-10% , Faint; Medium clay; Strong grade 
	of structure, 20-50 mm, Prismatic; 50-100 mm, Angular blocky; Smooth-ped fabric; Dry; 
	Moderately plastic; Normal plasticity; Moderately sticky; Many cutans, >50% of ped faces or 
	walls coated, faint; Field pH 6 (Raupach); Few, very fine (0-1mm) roots; 
	Morphological Notes
	A1	Sand fraction is fine.                                                                                                             
	                                                                     
	Observation Notes
	Site Notes
	FRASER TRANSECT F                     

	Project Name:	SOIL STRUCTURE & MANAGEMENT             
	Project Code:	SSM	Site ID:	SSM206	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	SOIL STRUCTURE & MANAGEMENT             
	Project Code:	SSM	Site ID:	SSM206	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile