Project Name:	SOIL STRUCTURE & MANAGEMENT             
	Project Code:	SSM	Site ID:	SSM217	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	B. Murphy	Locality:
	Date Desc.:	12/03/92	Elevation:	220 metres
	Map Ref.:	Sheet No. : 8327   1:100000	Rainfall:	No Data
	Northing/Long.:	6086600 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	506700  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	No Data
	Slope:	1 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn2.13
	ASC Confidence:	Great Soil Group:	Red earth
	Confidence level not specified
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.1 m	Brown (7.5YR5/4-Moist); Light brown (7.5YR6/4-Dry); ; Fine sandy loam; Weak grade of 
	structure, 10-20 mm, Subangular blocky; Common (1-5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Dry; Very weak consistence; Field pH 5.5 (Raupach); Common, very fine (0-1mm) 
	roots; 
	B21	0.1 - 0.27 m	Yellowish red (5YR4/6-Moist); ; Medium sandy clay loam; Weak grade of structure, 20-50 mm, 
	Subangular blocky; 50-100 mm, Columnar; Common (1-5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Dry; Very firm consistence; Field pH 6 (Raupach); Common, very fine (0-1mm) 
	roots; 
	B22	0.27 - 0.55 m	Yellowish red (5YR5/8-Moist); ; Clay loam; Moderate grade of structure, 20-50 mm, Subangular 
	blocky; 50-100 mm, Columnar; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, 
	Dry; Very firm consistence; Field pH 7 (Raupach); Common, very fine (0-1mm) roots; 
	B23	0.55 - 0.95 m	Reddish yellow (7.5YR6/6-Moist); Substrate influence, 2.5YR36, 2-10% , Distinct; Light clay; 
	Moderate grade of structure, 20-50 mm, Subangular blocky; 50-100 mm, Columnar; Dry; Very 
	weak consistence; Common cutans, 10-50% of ped faces or walls coated, distinct; Few (2 - 10
	 %), Manganiferous, Medium (2 -6 mm), Nodules, strong, segregations;Soil matrix is Slightly 
	calcareous; Field pH 8.5 (Raupach); Few, very fine (0-1mm) roots; 
	Morphological Notes
	B23	Breaks 2-5mm polyhedral.                                                                                                     
	                                                                           
	Observation Notes
	Site Notes
	YATE'S TRANSECT E                     

	Project Name:	SOIL STRUCTURE & MANAGEMENT             
	Project Code:	SSM	Site ID:	SSM217	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	SOIL STRUCTURE & MANAGEMENT             
	Project Code:	SSM	Site ID:	SSM217	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile