Project Name:	SOIL STRUCTURE & MANAGEMENT             
	Project Code:	SSM	Site ID:	SSM224	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	B. Murphy	Locality:
	Date Desc.:	25/03/92	Elevation:	270 metres
	Map Ref.:	Sheet No. : 8430   1:50000	Rainfall:	No Data
	Northing/Long.:	6249700 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	581800  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	QrOs	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Rises
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	No Data
	Slope:	2 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:	Not apparent (wind); No scalding (scald) Partial, 
	Minor (sheet) No wave erosion (wave) No rill 
	erosion (rill) No mass movement (mass) No gully 
	erosion (gully) No stream bank erosion (stbank) 
	No tunnel erosion (tunnel) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dr2.13
	ASC Confidence:	Great Soil Group:	Red-brown earth
	Confidence level not specified
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.1 m	Dark brown (7.5YR3/4-Moist); ; Loam; Weak grade of structure; Earthy fabric; Dry; Very weak 
	consistence; Non-plastic; Normal plasticity; Non-sticky; Field pH 6 (Raupach); 
	A12	0.1 - 0.2 m	Dark reddish brown (5YR3/4-Moist); ; Fine sandy clay loam; Weak grade of structure; Earthy 
	fabric; Dry; Very weak consistence; Non-plastic; Normal plasticity; Non-sticky; Field pH 6.5 
	(Raupach); 
	B21	0.2 - 0.4 m	Reddish brown (5YR4/4-Moist); ; Medium clay; Strong grade of structure; Smooth-ped fabric; 
	Dry; Moderately plastic; Normal plasticity; Moderately sticky; Very few (0 - 2 %), 
	Manganiferous, Medium (2 -6 mm), Veins, weak, segregations;Field pH 7 (Raupach); 
	B22	0.4 - 0.6 m	Yellowish red (5YR4/6-Moist); ; Medium clay; Strong grade of structure; Smooth-ped fabric; 
	Dry; Moderately plastic; Normal plasticity; Moderately sticky; Very few (0 - 2 %), 
	Manganiferous, Medium (2 -6 mm), Veins, weak, segregations;Very few (0 - 2 %), Calcareous, 
	Medium (2 -6 mm), Soft segregations, weak, segregations;Soil matrix is Slightly calcareous; 
	Field pH 8.5 (Raupach); 
	B23	0.6 - 0.7 m	Yellowish red (5YR5/6-Moist); ; Medium clay; Strong grade of structure; Smooth-ped fabric; 
	Dry; Moderately plastic; Normal plasticity; Moderately sticky; Very few (0 - 2 %), 
	Manganiferous, Medium (2 -6 mm), Veins, weak, segregations;Very few (0 - 2 %), Calcareous, 
	Medium (2 -6 mm), Soft segregations, weak, segregations;Soil matrix is Slightly calcareous; 
	Field pH 9 (Raupach); 
	B31	0.7 - 0.9 m	Yellowish red (5YR5/6-Moist); Substrate influence, 2-10% , Faint; Medium clay; Strong grade of
	 structure; Smooth-ped fabric; Dry; Moderately plastic; Normal plasticity; Moderately sticky; Very
	 few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Veins, weak, segregations;Very few (0 - 2 
	%), Calcareous, Medium (2 -6 mm), Soft segregations, weak, segregations;Soil matrix is Slightly
	 calcareous; Field pH 9 (Raupach); 
	Morphological Notes
	A11	Sand fraction is fine.                                                                                                             
	                                                                     
	Observation Notes

	Project Name:	SOIL STRUCTURE & MANAGEMENT             
	Project Code:	SSM	Site ID:	SSM224	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Notes
	PHILLIP'S TRANSECT F                  

	Project Name:	SOIL STRUCTURE & MANAGEMENT             
	Project Code:	SSM	Site ID:	SSM224	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	SOIL STRUCTURE & MANAGEMENT             
	Project Code:	SSM	Site ID:	SSM224	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile