Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD16	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	McKane, Dermot	Locality:
	Date Desc.:	15/07/93	Elevation:	267 metres
	Map Ref.:	Sheet No. : 8327   DGPS	Rainfall:	No Data
	Northing/Long.:	6126350 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	540730  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	5 % 	Aspect:	315 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Red Kandosol Medium Non-gravelly Loamy 	Principal Profile Form:	N/A
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.12 m	Dark reddish brown (5YR3/4-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; 
	Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Very weak consistence; 0-2%, fine 
	gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; Common, very fine (0-1mm)
	 roots; Few, fine (1-2mm) roots; Clear change to - 
	B1	0.12 - 0.41 m	Red (2.5YR4/8-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Common (1-5 per 
	100mm2) Very fine (0.075-1mm) macropores, Weak consistence; 0-2%, fine gravelly, 2-6mm, 
	subangular, dispersed, Quartz, coarse fragments; Few, very fine (0-1mm) roots; Clear change 
	B21	0.41 - 0.65 m	Yellowish red (5YR5/8-Moist); ; Light medium clay; Massive grade of structure; Earthy fabric; 
	Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Weak consistence; 0-2%, fine 
	gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; Few, very fine (0-1mm) 
	roots; Clear change to - 
	B22	0.65 - 0.86 m	Mottles, 2-10% , Faint; Light medium clay; Weak grade of structure, 2-5 mm, Subangular blocky; 
	Smooth-ped fabric; Weak consistence; 2-10%, fine gravelly, 2-6mm, subangular, dispersed, 
	Quartz, coarse fragments; 
	Morphological Notes
	B1	Very sticky.                                                                                                                           
	                                                                 
	Observation Notes
	Site Notes

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD16	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	8.08A	0.186A	14.2J	14.1	1.3	0.05	9I	0.56
	0.12 - 0.41	7.82A	0.088A	2.6J	2.5	1.5	0.06	6.3I	0.95
	0.41 - 0.65	8.18A	0.142A	3J	2.9	4	0.11	11.8I	0.93
	0.65 - 0.86	8.11A	0.103A	4J	3.9	3.6	0.16	12.8I	1.25
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12	2.13C	24.6I	11.3	64.1
	0.12 - 0.41	0.3C	34.7I	9.6	55.7
	0.41 - 0.65	0.44C	54.8I	7.3	37.9
	0.65 - 0.86	0.3C	59.6I	12.6	27.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.12
	0.12 - 0.41
	0.41 - 0.65
	0.65 - 0.86

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD16	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15L1	Base saturation percentage (BSP)
	15N1	Exchangeable sodium percentage (ESP)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded