Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD21	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	McKane, Dermot	Locality:
	Date Desc.:	15/07/93	Elevation:	253 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6125090 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	536910  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	5 % 	Aspect:	315 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Brown Dermosol Medium Non-gravelly Clay-	Principal Profile Form:	N/A
	loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (7.5YR3/4-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Many (>5 
	per 100mm2) Very fine (0.075-1mm) macropores, Weak consistence; 0-2%, fine gravelly, 2-
	6mm, subangular, Quartz, coarse fragments; Field pH 5.5 (pH meter); Common, very fine (0-
	1mm) roots; Gradual, Smooth change to - 
	B1	0.1 - 0.58 m	Yellowish red (5YR4/8-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Common 
	(1-5 per 100mm2) Very fine (0.075-1mm) macropores, Weak consistence; 0-2%, fine gravelly, 
	2-6mm, subangular, Quartz, coarse fragments; 0-2%, fine gravelly, 2-6mm, subangular, coarse 
	fragments; Field pH 6.5 (pH meter); Few, very fine (0-1mm) roots; Gradual, Smooth change to - 
	B21	0.58 - 0.79 m	Yellowish brown (10YR5/8-Moist); ; Light medium clay; Weak grade of structure, 2-5 mm, 
	Subangular blocky; Smooth-ped fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Firm consistence; 0-2%, fine gravelly, 2-6mm, subangular, Quartz, coarse 
	fragments; 0-2%, fine gravelly, 2-6mm, subangular, coarse fragments; Field pH 6.5 (pH meter); 
	Gradual, Smooth change to - 
	B22	0.79 - 1.5 m	Brownish yellow (10YR6/8-Moist); Mottles, 2-10% , Faint; Mottles, 0-2% , Distinct; Medium clay; 
	Moderate grade of structure, 2-5 mm, Subangular blocky; Smooth-ped fabric; Few (<1 per 
	100mm2) Very fine (0.075-1mm) macropores, Firm consistence; 0-2%, fine gravelly, 2-6mm, 
	subangular, Quartz, coarse fragments; 0-2%, fine gravelly, 2-6mm, subangular, coarse 
	fragments; Field pH 6.5 (pH meter); Gradual, Smooth change to - 
	B23	1.5 - 1.6 m	Brownish yellow (10YR6/8-Moist); Mottles, 2-10% , Faint; Mottles, 0-2% , Distinct; Medium clay; 
	Moderate grade of structure, 2-5 mm, Subangular blocky; Smooth-ped fabric; Firm consistence; 
	0-2%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; 0-2%, fine gravelly, 2-6mm, 
	subangular, coarse fragments; Field pH 7 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD21	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.53A	0.044A	3.4J	0.83	1.2	0.05	8.3I	0.60
	0.1 - 0.58	6.77A	0.02A	5J	2.4	0.86	0.07	9.8I	0.71
	0.58 - 0.79	7.44A	0.027A	5.7J	3.9	0.68	0.08	9.8I	0.82
	0.79 - 1.5	8.2A	0.17A	17.6J	8.9	1.5	0.37	19.3I	1.92
	1.5 - 1.6	8.44A	0.042A	12.6J	11.5	1.8	0.6	23.4I	2.56
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.86C	38.6I	13.4	48
	0.1 - 0.58	0.39C	52.3I	9.5	38.2
	0.58 - 0.79	0.35C	61.2I	11	27.8
	0.79 - 1.5	0.16C	68.5I	10.8	20.7
	1.5 - 1.6	0.06C	71.5I	11.6	16.9
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.58
	0.58 - 0.79
	0.79 - 1.5
	1.5 - 1.6

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD21	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15L1	Base saturation percentage (BSP)
	15N1	Exchangeable sodium percentage (ESP)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded