Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD34	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	McKane, Dermot	Locality:
	Date Desc.:	15/07/93	Elevation:	284 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6126174 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	538272  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	4 % 	Aspect:	315 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Brown Dermosol Medium Non-gravelly 	Principal Profile Form:	N/A
	Loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark reddish brown (5YR3/4-Moist); ; Loam; Massive grade of structure; Earthy fabric; Few (<1
	 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Weak consistence; 0-2%, fine gravelly, 
	2-6mm, subangular, dispersed, Quartz, coarse fragments; Common, very fine (0-1mm) roots; 
	Clear change to - 
	B1	0.1 - 0.59 m	Red (2.5YR4/8-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Common (1-5 per 
	100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Medium (2-5mm) 
	macropores, Dry; Firm consistence; 0-2%, fine gravelly, 2-6mm, subangular, dispersed, Quartz,
	 coarse fragments; Few, very fine (0-1mm) roots; Gradual change to - 
	B21	0.59 - 1.5 m	Mottles, 10-20% , Distinct; Mottles, 2-10% , Faint; Light medium clay; Strong grade of structure, 
	2-5 mm, Subangular blocky; Smooth-ped fabric; Dry; Very firm consistence; 2-10%, fine 
	gravelly, 2-6mm, subrounded, dispersed, coarse fragments; Common cutans, 10-50% of ped 
	faces or walls coated; Few (2 - 10 %), Manganiferous, , ; Clear change to - 
	BC	1.5 - 1.66 m	Strong brown (7.5YR5/8-Moist); Mottles, 2-10% , Faint; Mottles, 2-10% , Faint; Light clay; 
	Massive grade of structure; Earthy fabric; Dry; Very firm consistence; 0-2%, fine gravelly, 2-
	6mm, subrounded, dispersed, Quartz, coarse fragments; 
	Morphological Notes
	B1	Moist Munsell should be 10YR 4/8                                                                                        
	                                                                                
	Observation Notes
	Site Notes

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD34	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.37A	0.066A	3.3J	0.82	1	0	9.1I	0.00
	0.1 - 0.59	6.05A	0.036A	4.4J	2.1	0.96	0.86	9.8I	8.78
	0.59 - 1.5	7.13A	0.034A	4.9J	5	0.71	0.37	15.9I	2.33
	1.5 - 1.66	8.29A	0.067A	9.8J	8.4	1.3	0.99	20I	4.95
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	2.02C	39.1I	13.1	47.8
	0.1 - 0.59	0.4C	55.6I	10.1	34.3
	0.59 - 1.5	0.07C	63.9I	10.9	25.2
	1.5 - 1.66	0.06C	60.2I	17	22.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.59
	0.59 - 1.5
	1.5 - 1.66

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD34	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15L1	Base saturation percentage (BSP)
	15N1	Exchangeable sodium percentage (ESP)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded