Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD36	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	McKane, Dermot	Locality:
	Date Desc.:	15/07/93	Elevation:	238 metres
	Map Ref.:	Sheet No. : 8327   DGPS	Rainfall:	No Data
	Northing/Long.:	6123010 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	535550  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	3 % 	Aspect:	90 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Brown Dermosol Medium Non-gravelly 	Principal Profile Form:	N/A
	Loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.11 m	Brown (7.5YR4/4-Moist); ; Loam; Massive grade of structure; Earthy fabric; Common (1-5 per 
	100mm2) Very fine (0.075-1mm) macropores, Dry; Very weak consistence; 0-2%, fine gravelly,
	 2-6mm, subrounded, dispersed, Quartz, coarse fragments; Common, very fine (0-1mm) roots; 
	Few, fine (1-2mm) roots; Clear, Smooth change to - 
	B1	0.11 - 0.42 m	Yellowish red (5YR5/8-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Common 
	(1-5 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Very weak consistence; 0-2%, fine
	 gravelly, 2-6mm, subrounded, reoriented, Quartz, coarse fragments; 0-2%, fine gravelly, 2-
	6mm, subangular, reoriented, coarse fragments; Few, very fine (0-1mm) roots; Clear, Smooth 
	change to - 
	B21	0.42 - 0.83 m	Brownish yellow (10YR6/8-Moist); ; Light medium clay; Weak grade of structure, 5-10 mm, 
	Subangular blocky; Smooth-ped fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) 
	macropores, Dry; Very weak consistence; 0-2%, fine gravelly, 2-6mm, subrounded, reoriented,
	 Quartz, coarse fragments; 0-2%, fine gravelly, 2-6mm, subangular, reoriented, coarse 
	fragments; Few, very fine (0-1mm) roots; Gradual, Smooth change to - 
	B22	0.83 - 1.29 m	Yellowish brown (10YR5/8-Moist); Mottles, 2-10% , Distinct; Mottles, 0-2% , Faint; Medium clay; 
	Moderate grade of structure, 20-50 mm, Subangular blocky; Smooth-ped fabric; Dry; Strong 
	consistence; 0-2%, fine gravelly, 2-6mm, subangular, reoriented, coarse fragments; Common 
	cutans, 10-50% of ped faces or walls coated; Gradual change to - 
	BC	1.29 - 2 m	Yellowish brown (10YR5/8-Moist); Mottles, 2-10% , Distinct; Mottles, 0-2% , Distinct; Light clay; 
	Moderate grade of structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; Dry; Firm 
	consistence; Common cutans, 10-50% of ped faces or walls coated; Very few (0 - 2 %), 
	Ferruginous, , ; Very few (0 - 2 %), Ferromanganiferous, , ; 
	Morphological Notes
	B21	Slightly plastic.                                                                                                                       
	                                                                
	B22	Soapy when wet.                                                                                                                 
	                                                                        
	Observation Notes
	Very friendly horses!                                                                                                                                                                          

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD36	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Notes
	HORSE STUD                            

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD36	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.11	5.25A	0.046A	2.6J	0.7	0.79	0.06	6.4I	0.94
	0.11 - 0.42	6.23A	0.019A	4.2J	2.3	0.62	0.09	8.9I	1.01
	0.42 - 0.83	4.87A	0.035A	3.4J	4.1	0.32	0.46	10.8I	4.26
	0.83 - 1.29	8.59A	0.078A	11.1J	11.9	1.3	3.6	25.8I	13.95
	1.29 - 2	8.67A	0.06A	11.7J	11.7	1.1	3.9	23.4I	16.67
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.11	1.64C	36.9I	13.6	49.5
	0.11 - 0.42	0.35C	56.2I	10.8	33
	0.42 - 0.83	0.22C	60.6I	18.7	20.7
	0.83 - 1.29	0.12C	79.7I	6.4	13.9
	1.29 - 2	0.1C	63.8I	15.9	20.3
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.11
	0.11 - 0.42
	0.42 - 0.83
	0.83 - 1.29
	1.29 - 2

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD36	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15L1	Base saturation percentage (BSP)
	15N1	Exchangeable sodium percentage (ESP)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded