Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD37	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	McKane, Dermot	Locality:
	Date Desc.:	15/07/93	Elevation:	222 metres
	Map Ref.:	Sheet No. : 8327   DGPS	Rainfall:	No Data
	Northing/Long.:	6121990 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	541370  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	2 % 	Aspect:	90 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Brown Dermosol Medium Non-gravelly 	Principal Profile Form:	N/A
	Loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.16 m	Brown (7.5YR4/4-Moist); ; Fine sandy loam; Massive grade of structure; Earthy fabric; Common
	 (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 100mm2) Fine (1-
	2mm) macropores, Dry; Weak consistence; 0-2%, fine gravelly, 2-6mm, subrounded, dispersed,
	 coarse fragments; Few, very fine (0-1mm) roots; Clear, Smooth change to - 
	B1	0.16 - 0.53 m	Yellowish red (5YR4/8-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Common 
	(1-5 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-2mm) 
	macropores, Dry; Weak consistence; 0-2%, fine gravelly, 2-6mm, subrounded, dispersed, 
	coarse fragments; Very few (0 - 2 %), Manganiferous, , ; Few, very fine (0-1mm) roots; Clear, 
	Smooth change to - 
	B21	0.53 - 0.81 m	Strong brown (7.5YR5/8-Moist); Mottles, 2-10% , Faint; Mottles; Light clay; Moderate grade of 
	structure, 2-5 mm, Subangular blocky; Smooth-ped fabric; Common (1-5 per 100mm2) Very fine 
	(0.075-1mm) macropores, Dry; Weak consistence; 0-2%, fine gravelly, 2-6mm, subrounded, 
	dispersed, coarse fragments; Common cutans, 10-50% of ped faces or walls coated; Gradual, 
	Smooth change to - 
	B22	0.81 - 1.7 m	Brownish yellow (10YR6/8-Moist); Mottles, 10-20% , Prominent; Mottles, 2-10% , Distinct; Light 
	medium clay; Moderate grade of structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; 
	Dry; Firm consistence; 0-2%, fine gravelly, 2-6mm, subrounded, dispersed, coarse fragments; 
	0-2%, fine gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments; Common 
	cutans, 10-50% of ped faces or walls coated; Gradual, Smooth change to - 
	B23	1.7 - 2 m	Yellowish brown (10YR5/8-Moist); Mottles, 2-10% , Distinct; Light clay; Dry; Firm consistence; 
	0-2%, fine gravelly, 2-6mm, subrounded, dispersed, coarse fragments; 0-2%, fine gravelly, 2-
	6mm, subrounded, dispersed, Quartz, coarse fragments; 
	Morphological Notes
	Observation Notes
	Site Notes
	NEXT TO RAIL LINE                     

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD37	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.16	3.93A	0.047A	2.4J	0.34	0.62	0.07	5.2I	1.35
	0.16 - 0.53	5.56A	0.029A	3.3J	1.4	0.46	0.09	7.4I	1.22
	0.53 - 0.81	6.27A	0.045A	3.3J	4.7	0.28	0.4	10.3I	3.88
	0.81 - 1.7	8.53A	0.049A	8J	11	0.95	2.2	20.9I	10.53
	1.7 - 2	8.61A	0.058A	11.3J	13.9	1.2	3.4	27.3I	12.45
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.16	1.1C	35I	14.8	50.2
	0.16 - 0.53	0.28C	44.7I	12	43.3
	0.53 - 0.81	0.19C	57.1I	11.7	31.2
	0.81 - 1.7	0.08C	73.6I	9.7	16.7
	1.7 - 2	0.07C	72.2I	10.3	17.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.16
	0.16 - 0.53
	0.53 - 0.81
	0.81 - 1.7
	1.7 - 2

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD37	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15L1	Base saturation percentage (BSP)
	15N1	Exchangeable sodium percentage (ESP)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded