Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD53	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	McKane, Dermot	Locality:
	Date Desc.:	15/07/93	Elevation:	215 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6125510 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	534270  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	2 % 	Aspect:	315 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Brown Chromosol Medium Non-gravelly 	Principal Profile Form:	N/A
	Loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.15 m	Dark reddish brown (5YR3/4-Moist); ; Loam; Massive grade of structure; Earthy fabric; Many 
	(>5 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 100mm2) Fine (1-2mm) 
	macropores, Weak consistence; 0-2%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, 
	coarse fragments; 0-2%, medium gravelly, 6-20mm, subrounded, dispersed, coarse fragments; 
	Common, very fine (0-1mm) roots; Clear change to - 
	B1	0.15 - 0.58 m	Red (2.5YR4/6-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Common (1-5 per 
	100mm2) Very fine (0.075-1mm) macropores, Weak consistence; 0-2%, fine gravelly, 2-6mm, 
	subangular, dispersed, Quartz, coarse fragments; 0-2%, medium gravelly, 6-20mm, 
	subrounded, dispersed, coarse fragments; Few, very fine (0-1mm) roots; Clear change to - 
	B21	0.58 - 0.84 m	Yellowish brown (10YR5/6-Moist); Mottles, 0-2% , Faint; Medium clay; Strong grade of 
	structure, 2-5 mm, Subangular blocky; Smooth-ped fabric; Common (1-5 per 100mm2) Very fine 
	(0.075-1mm) macropores, Firm consistence; 0-2%, fine gravelly, 2-6mm, subangular, dispersed,
	 Quartz, coarse fragments; 0-2%, fine gravelly, 2-6mm, subangular, dispersed, coarse 
	fragments; Common cutans, 10-50% of ped faces or walls coated, faint; Few (2 - 10 %), 
	Manganiferous, Fine (0 - 2 mm), Fragments, weak, segregations;Clear change to - 
	B22	0.84 - 1.51 m	Brownish yellow (10YR6/8-Moist); Mottles, 0-2% , Faint; Light medium clay; Strong grade of 
	structure, 10-20 mm, Platy; 50-100 mm, Lenticular; Smooth-ped fabric; Firm consistence; 2-10%,
	 fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; 2-10%, fine gravelly, 
	2-6mm, subangular, dispersed, coarse fragments; Common cutans, 10-50% of ped faces or 
	walls coated, faint; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), Veins, weak, 
	segregations;Gradual change to - 
	B23	1.51 - 1.85 m	Pale yellow (2.5Y7/3-Moist); Mottles, 10-20% , Distinct; Mottles, 10-20% , Distinct; Light medium 
	clay; Strong grade of structure, 2-5 mm, Subangular blocky; Smooth-ped fabric; Firm 
	consistence; 2-10%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; 2-
	10%, medium gravelly, 6-20mm, subrounded, dispersed, coarse fragments; Few (2 - 10 %), 
	Calcareous, Medium (2 -6 mm), Fragments, weak, segregations;Few (2 - 10 %), 
	Manganiferous, Medium (2 -6 mm), Fragments, weak, segregations;
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD53	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD53	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	5.35A	0.05A	2.8J	0.83	1.1	0.01	7.8I	0.13
	0.15 - 0.58	6.43A	0.025A	4J	2.7	0.72	0.11	9.4I	1.17
	0.58 - 0.84	7.08A	0.041A	5.6J	6.8	1.1	0.66	17.9I	3.69
	0.84 - 1.51	7.6A	0.105A	6.4J	8.9	1.4	1.1	17.7I	6.21
	1.51 - 1.85	8.72A	0.148A	12.8J	12.6	1.6	2.2	25.5I	8.63
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	1.36C	26.3I	14	59.7
	0.15 - 0.58	0.37C	46.9I	10.6	42.5
	0.58 - 0.84	0.18C	65.4I	13.9	20.7
	0.84 - 1.51	0.32C	60.4I	14.8	24.8
	1.51 - 1.85	0.1C	57.1I	21.7	21.2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.58
	0.58 - 0.84
	0.84 - 1.51
	1.51 - 1.85

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD53	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15L1	Base saturation percentage (BSP)
	15N1	Exchangeable sodium percentage (ESP)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded