Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD60	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	McKane, Dermot	Locality:
	Date Desc.:	15/07/93	Elevation:	234 metres
	Map Ref.:	Sheet No. : 8327   DGPS	Rainfall:	No Data
	Northing/Long.:	6124878 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	534894  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	3 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Brown Dermosol Medium Non-gravelly Clay-	Principal Profile Form:	N/A
	loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.13 m	Dark reddish brown (5YR3/3-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; 
	Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 100mm2) Fine (1-
	2mm) macropores, Weak consistence; Many, very fine (0-1mm) roots; 
	A3	0.13 - 0.31 m	Yellowish red (5YR4/8-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Common 
	(1-5 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 100mm2) Fine (1-2mm)
	 macropores, Weak consistence; 2-10%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, 
	coarse fragments; Common, very fine (0-1mm) roots; 
	B1	0.31 - 0.57 m	Yellowish red (5YR5/8-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Common 
	(1-5 per 100mm2) Very fine (0.075-1mm) macropores, Firm consistence; 2-10%, fine gravelly, 
	2-6mm, subangular, dispersed, Quartz, coarse fragments; Few, very fine (0-1mm) roots; 
	B21	0.57 - 1.47 m	Yellowish brown (10YR5/8-Moist); Mottles, 10-20% , Prominent; Mottles, 10-20% , Prominent; 
	Light medium clay; Moderate grade of structure, 2-5 mm, Subangular blocky; Smooth-ped fabric;
	 Firm consistence; 2-10%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse 
	fragments; Few (2 - 10 %), Manganiferous, , ; 
	B22	1.47 - 1.9 m	Yellowish brown (10YR5/6-Moist); Mottles, 20-50% , Distinct; Light medium clay; Strong grade 
	of structure, 2-5 mm, Subangular blocky; Smooth-ped fabric; Firm consistence; 0-2%, fine 
	gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD60	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	5.03A	0.041A	3J	0.78	0.78	0.02	8.2I	0.24
	0.13 - 0.31	6.09A	0.024A	4J	1.8	0.39	0.03	7.9I	0.38
	0.31 - 0.57	6.64A	0.02A	4.9J	3.3	0.24	0.07	10.4I	0.67
	0.57 - 1.47	5.52A	0.129A	5.4J	5.9	0.66	0.12	13.5I	0.89
	1.47 - 1.9	5.52A	0.031A	10.2J	10.6	1	0.42	24.8I	1.69
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13	1.44C	33.8I	17.9	48.3
	0.13 - 0.31	0.45C	46.2I	12.2	41.6
	0.31 - 0.57	0.35C	54.2I	12.4	33.4
	0.57 - 1.47	0.56C	57.9I	15	27.1
	1.47 - 1.9	0.05C	57.4I	18.2	24.4
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.31
	0.31 - 0.57
	0.57 - 1.47
	1.47 - 1.9

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD60	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15L1	Base saturation percentage (BSP)
	15N1	Exchangeable sodium percentage (ESP)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded