Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD65	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	McKane, Dermot	Locality:
	Date Desc.:	15/07/93	Elevation:	258 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6123660 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	541727  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	3 % 	Aspect:	90 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Brown Dermosol Medium Non-gravelly Clay-	Principal Profile Form:	N/A
	loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.16 m	Dark reddish brown (5YR3/4-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; 
	Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 100mm2) Fine (1-
	2mm) macropores, Firm consistence; 0-2%, fine gravelly, 2-6mm, subangular, dispersed, 
	Quartz, coarse fragments; Common, very fine (0-1mm) roots; 
	B1	0.16 - 0.39 m	Yellowish red (5YR4/8-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Many (>5 
	per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 100mm2) Fine (1-2mm) 
	macropores, Very firm consistence; 0-2%, fine gravelly, 2-6mm, subangular, dispersed, Quartz,
	 coarse fragments; Few, very fine (0-1mm) roots; 
	B21	0.39 - 0.72 m	Strong brown (7.5YR5/6-Moist); Mottles, 10-20% , Distinct; Light clay; Moderate grade of 
	structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; Common (1-5 per 100mm2) Very 
	fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-2mm) macropores, Weak 
	consistence; 10-20%, fine gravelly, 2-6mm, subangular, dispersed, coarse fragments; 
	B22	0.72 - 1.43 m	Brownish yellow (10YR6/8-Moist); Mottles, 20-50% , Prominent; Mottles, 10-20% , Distinct; 
	Moderate grade of structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; Few (<1 per 
	100mm2) Very fine (0.075-1mm) macropores, Firm consistence; 10-20%, fine gravelly, 2-6mm, 
	subrounded, dispersed, coarse fragments; Common (10 - 20 %), Manganiferous, Fine (0 - 2 
	mm), Fragments, weak, segregations;Common (10 - 20 %), Manganiferous, Medium (2 -6 mm), 
	Fragments, weak, segregations;
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD65	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.16	5.37A	0.076A	2.5J	0.52	0.67	0.1	6.9I	1.45
	0.16 - 0.39	6.56A	0.035A	3.9J	1.2	0.2	0.21	7.2I	2.92
	0.39 - 0.72	6.98A	0.027A	5J	3.4	0.27	0.32	11.2I	2.86
	0.72 - 1.43	8.04A	0.036A	6.7J	6.6	0.79	1.4	16.3I	8.59
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.16	1.14C	26.5I	15.8	57.7
	0.16 - 0.39	0.32C	37.1I	16.7	46.2
	0.39 - 0.72	0.25C	51.3I	15.1	33.6
	0.72 - 1.43	0.07C	60.8I	12	27.2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.16
	0.16 - 0.39
	0.39 - 0.72
	0.72 - 1.43

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD65	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15L1	Base saturation percentage (BSP)
	15N1	Exchangeable sodium percentage (ESP)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded