Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD67	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	McKane, Dermot	Locality:
	Date Desc.:	15/07/93	Elevation:	248 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6123151 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	539834  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	2 % 	Aspect:	315 degrees
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Yellow Dermosol Medium Non-gravelly 	Principal Profile Form:	N/A
	Loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.12 m	Dark reddish brown (5YR3/4-Moist); ; Loam; Massive grade of structure; Earthy fabric; Common
	 (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 100mm2) Fine (1-
	2mm) macropores, Weak consistence; Few, fine (1-2mm) roots; Many, very fine (0-1mm) roots;
	B1	0.12 - 0.43 m	Yellowish red (5YR5/8-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Common 
	(1-5 per 100mm2) Very fine (0.075-1mm) macropores, Weak consistence; 0-2%, fine gravelly, 
	2-6mm, subangular, dispersed, Quartz, coarse fragments; Few, very fine (0-1mm) roots; 
	B21	0.43 - 0.75 m	Brownish yellow (10YR6/8-Moist); Mottles, 10-20% , Distinct; Light clay; Moderate grade of 
	structure, 2-5 mm, Subangular blocky; Smooth-ped fabric; Common (1-5 per 100mm2) Very fine 
	(0.075-1mm) macropores, Firm consistence; 2-10%, fine gravelly, 2-6mm, subangular, 
	dispersed, Quartz, coarse fragments; Few, very fine (0-1mm) roots; 
	B22	0.75 - 2.37 m	Brownish yellow (10YR6/8-Moist); Mottles, 20-50% , Distinct; Light medium clay; Moderate 
	grade of structure, 2-5 mm, Subangular blocky; Smooth-ped fabric; Few (<1 per 100mm2) Very 
	fine (0.075-1mm) macropores, Firm consistence; 2-10%, fine gravelly, 2-6mm, subangular, 
	dispersed, Quartz, coarse fragments; 2-10%, fine gravelly, 2-6mm, subangular, dispersed, 
	coarse fragments; Common (10 - 20 %), Manganiferous, Fine (0 - 2 mm), Nodules, weak, 
	segregations;Common (10 - 20 %), Manganiferous, Medium (2 -6 mm), Nodules, weak, 
	segregations;
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD67	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	4.43A	0.136A	2.2J	0.66	0.72	0	7.2I	0.00
	0.12 - 0.43	4.97A	0.098A	4J	2.3	0.61	0	9.5I	0.00
	0.43 - 0.75	6.29A	0.033A	4.3J	4.6	0.35	0.03	11.7I	0.26
	0.75 - 2.37	6.67A	0.041A	5.5J	6.1	0.75	0.32	15.2I	2.11
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12	2.08C	32.5I	22.8	44.7
	0.12 - 0.43	0.66C	50.5I	14.8	34.7
	0.43 - 0.75	0.32C	58I	19	23
	0.75 - 2.37	0.14C	66.2I	10.9	22.9
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.12
	0.12 - 0.43
	0.43 - 0.75
	0.75 - 2.37

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD67	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15L1	Base saturation percentage (BSP)
	15N1	Exchangeable sodium percentage (ESP)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded