Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD72	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	McKane, Dermot	Locality:
	Date Desc.:	15/07/93	Elevation:	239 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6123690 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	539070  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	1 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Brown Dermosol Medium Non-gravelly Clay-	Principal Profile Form:	N/A
	loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark reddish brown (5YR3/3-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; 
	Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-
	2mm) macropores, Firm consistence; 0-2%, fine gravelly, 2-6mm, subrounded, dispersed, 
	coarse fragments; Few, very fine (0-1mm) roots; Clear change to - 
	B1	0.1 - 0.37 m	Yellowish red (5YR4/6-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Common 
	(1-5 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-2mm) 
	macropores, Firm consistence; 0-2%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, 
	coarse fragments; 0-2%, fine gravelly, 2-6mm, subangular, dispersed, coarse fragments; Few, 
	very fine (0-1mm) roots; Clear change to - 
	B21	0.37 - 0.83 m	Yellowish brown (10YR5/8-Moist); Mottles, 10-20% , Distinct; Mottles, 2-10% , Faint; Light clay; 
	Strong grade of structure, 2-5 mm, Subangular blocky; Smooth-ped fabric; Firm consistence; 0-
	2%, fine gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments; 0-2%, fine 
	gravelly, 2-6mm, subrounded, dispersed, coarse fragments; Few (2 - 10 %), Manganiferous, 
	Medium (2 -6 mm), Fragments, weak, segregations;Clear change to - 
	B22	0.83 - 1.4 m	Pale brown (10YR6/3-Moist); Mottles, 10-20% , Faint; Mottles, 10-20% , Faint; Light medium 
	clay; Strong grade of structure, 2-5 mm, Subangular blocky; Firm consistence; 0-2%, fine 
	gravelly, 2-6mm, subrounded, dispersed, coarse fragments; Clear change to - 
	BC	1.4 - 2.1 m	Reddish yellow (7.5YR6/6-Moist); Mottles, 10-20% , Faint; Mottles, 10-20% , Faint; Coarse 
	sandy light clay; Moderate grade of structure, <2 mm, Subangular blocky; Firm consistence; 2-
	10%, fine gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments; 2-10%, fine 
	gravelly, 2-6mm, subrounded, dispersed, coarse fragments; Few (2 - 10 %), Manganiferous, 
	Fine (0 - 2 mm), Fragments, weak, segregations;
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD72	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.24A	0.144A	4.3J	0.81	0.57	0	8I	0.00
	0.1 - 0.37	6.33A	0.022A	5.3J	1.5	0	0.27	9.1I	2.97
	0.37 - 0.83	6.6A	0.037A	5.2J	2.2	0.3	0	9.4I	0.00
	0.83 - 1.4	6.04A	0.065A	6.2J	2.5	0	0.41	10.7I	3.83
	1.4 - 2.1	7.67A	0.058A	17.8J	6.6	0.72	0.03	25I	0.12
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.52C	28.7I	18	53.3
	0.1 - 0.37	0.38C	37.5I	19.8	42.7
	0.37 - 0.83	0.24C	41.5I	13.4	45.1
	0.83 - 1.4	0.25C	41.9I	11.3	46.8
	1.4 - 2.1	0.19C	52.7I	10.7	36.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.37
	0.37 - 0.83
	0.83 - 1.4
	1.4 - 2.1

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD72	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15L1	Base saturation percentage (BSP)
	15N1	Exchangeable sodium percentage (ESP)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded