Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD82	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	McKane, Dermot	Locality:
	Date Desc.:	15/07/93	Elevation:	252 metres
	Map Ref.:	Sheet No. : 8327   DGPS	Rainfall:	No Data
	Northing/Long.:	6123375 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	540126  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	2 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Yellow Dermosol Medium Slightly gravelly 	Principal Profile Form:	N/A
	Loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.16 m	Dark reddish brown (5YR3/3-Moist); ; Coarse sandy clay loam; Massive grade of structure; 
	Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 
	100mm2) Fine (1-2mm) macropores, Firm consistence; 2-10%, fine gravelly, 2-6mm, 
	subangular, dispersed, coarse fragments; Many, very fine (0-1mm) roots; Gradual change to - 
	B1	0.16 - 0.53 m	Yellowish red (5YR4/8-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Common 
	(1-5 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-2mm) 
	macropores, Few (<1 per 100mm2) Medium (2-5mm) macropores, Very firm consistence; 0-2%,
	 fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; 0-2%, fine gravelly, 2-
	6mm, subangular, dispersed, coarse fragments; Few, very fine (0-1mm) roots; Gradual change 
	to - 
	B21	0.53 - 0.91 m	Brownish yellow (10YR6/8-Moist); Mottles, 10-20% , Prominent; Mottles, 10-20% , Distinct; Light
	 clay; Weak grade of structure, 2-5 mm, Subangular blocky; Smooth-ped fabric; Common (1-5 
	per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-2mm) 
	macropores, Very firm consistence; 2-10%, fine gravelly, 2-6mm, subangular, dispersed, 
	coarse fragments; Common (10 - 20 %), Manganiferous, , ; Few, very fine (0-1mm) roots; Clear
	B22	0.91 - 1.24 m	Yellowish brown (10YR5/6-Moist); Mottles, 10-20% , Distinct; Mottles, 20-50% , Distinct; Light 
	clay; Moderate grade of structure, 2-5 mm, Subangular blocky; Smooth-ped fabric; Common (1-
	5 per 100mm2) Very fine (0.075-1mm) macropores, 2-10%, fine gravelly, 2-6mm, subangular, 
	dispersed, coarse fragments; Common (10 - 20 %), Manganiferous, , ; Gradual change to - 
	B23	1.24 - 1.99 m	Yellowish brown (10YR5/6-Moist); Mottles, 20-50% , Distinct; Light clay; Moderate grade of 
	structure; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, 20-50%, fine gravelly, 2-
	6mm, subangular, dispersed, coarse fragments; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD82	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.16	4.87A	0.079A	2.2J	0.53	0.78	0.06	7.9I	0.76
	0.16 - 0.53	5.75A	0.032A	4J	1.3	0.55	0.07	8.5I	0.82
	0.53 - 0.91	6.49A	0.056A	5.5J	3.7	0.5	0.19	11.8I	1.61
	0.91 - 1.24	7.17A	0.053A	5.2J	4.2	0.63	0.42	14.1I	2.98
	1.24 - 1.99	7.88A	0.077A	7.6J	6.1	0.87	0.77	15.6I	4.94
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.16	1.6C	30.9I	23.9	45.2
	0.16 - 0.53	0.4C	42.9I	17.9	39.2
	0.53 - 0.91	0.32C	53.8I	17.6	28.6
	0.91 - 1.24	0.2C	55.9I	12.8	31.3
	1.24 - 1.99	0.19C	55.7I	16.9	27.4
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.16
	0.16 - 0.53
	0.53 - 0.91
	0.91 - 1.24
	1.24 - 1.99

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD82	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15L1	Base saturation percentage (BSP)
	15N1	Exchangeable sodium percentage (ESP)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded