Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD83	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	McKane, Dermot	Locality:
	Date Desc.:	15/07/93	Elevation:	243 metres
	Map Ref.:	Sheet No. : 8327   DGPS	Rainfall:	No Data
	Northing/Long.:	6122379 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	541262  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	1 % 	Aspect:	90 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Hypocalcic Black Dermosol Medium Non-gravelly Clay-	Principal Profile Form:	N/A
	loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.13 m	Dark reddish brown (5YR3/2-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; 
	Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 100mm2) Fine (1-
	2mm) macropores, Weak consistence; 0-2%, fine gravelly, 2-6mm, subangular, dispersed, 
	Quartz, coarse fragments; Many, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Gradual 
	B21	0.13 - 0.33 m	Dark brown (7.5YR3/2-Moist); ; Light clay; Weak grade of structure, 10-20 mm, Subangular 
	blocky; Smooth-ped fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, 
	Few (<1 per 100mm2) Fine (1-2mm) macropores, Few (<1 per 100mm2) Medium (2-5mm) 
	macropores, Very firm consistence; 0-2%, fine gravelly, 2-6mm, subangular, dispersed, Quartz,
	 coarse fragments; Few, very fine (0-1mm) roots; Gradual change to - 
	B22	0.33 - 0.65 m	Very dark brown (10YR2/2-Moist); ; Light medium clay; Moderate grade of structure, 10-20 mm,
	 Subangular blocky; Smooth-ped fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Strong consistence; 0-2%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, 
	coarse fragments; Few, very fine (0-1mm) roots; Diffuse change to - 
	B23	0.65 - 1.11 m	Brownish yellow (10YR6/8-Moist); Mottles, 20-50% , Distinct; Mottles, 20-50% , Distinct; Light 
	medium clay; Strong grade of structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; 
	Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Very firm consistence; 0-2%, 
	fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; Few (2 - 10 %), 
	Calcareous, , ; Few, very fine (0-1mm) roots; Gradual change to - 
	B3	1.11 - 2 m	Very pale brown (10YR7/4-Moist); Mottles, 20-50% , Distinct; Mottles, 20-50% , Faint; Light 
	medium clay; Weak grade of structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; 
	Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Very firm consistence; 2-10%, 
	fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; Common (10 - 20 %), 
	Calcareous, , ; Common (10 - 20 %), Manganiferous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes
	DEER FARM                             

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD83	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	5.83A	0.073A	3.7J	0.65	1.3	0	8.5I	0.00
	0.13 - 0.33	6.44A	0.041A	9.7J	2.1	0.92	0.11	15.7I	0.70
	0.33 - 0.65	7.25A	0.034A	15J	4.6	0.75	0.19	20.7I	0.92
	0.65 - 1.11	7.67A	0.032A	14.6J	5.3	1	0.1	21.9I	0.46
	1.11 - 2	8.36A	0.139A	17.2J	5.1	0.64	0.03	13.8I	0.22
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13	1.39C	28.7I	20.5	50.8
	0.13 - 0.33	1.15C	42.4I	21.8	35.8
	0.33 - 0.65	0.76C	45.4I	11.3	43.3
	0.65 - 1.11	0.26C	53.2I	9.5	37.3
	1.11 - 2	0.23C	39.2I	12	48.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.33
	0.33 - 0.65
	0.65 - 1.11
	1.11 - 2

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD83	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15L1	Base saturation percentage (BSP)
	15N1	Exchangeable sodium percentage (ESP)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded