Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	GW27	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Gessler	Locality:
	Date Desc.:	15/07/93	Elevation:	359 metres
	Map Ref.:	DGPS	Rainfall:	No Data
	Northing/Long.:	6081608 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	541207  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	8.5919 % 	Aspect:	125 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.31 m	Black (10YR2/1-Moist); ; Clay loam; 
	A3	0.31 - 0.47 m	Dark brown (10YR3/3-Moist); ; Clay loam; 
	B	0.47 - 1.15 m	Dark brown (7.5YR3/4-Moist); ; Light clay; 2-10%, fine gravelly, 2-6mm, angular, reoriented, 
	Mudstone, coarse fragments; 
	B	1.15 - 2.1 m	Yellowish red (5YR4/6-Moist); ; Light clay; 2-10%, fine gravelly, 2-6mm, angular, reoriented, 
	Mudstone, coarse fragments; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	GW27	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.31	6.02A	0.035A	5J	4.9	0.55	0.07	15.6I	0.45
	0.31 - 0.47	6.31A	0.022A	3J	5.3	0.4	0.04	12.6I	0.32
	0.47 - 1.15	6.21A	0.018A	1.4J	5.1	0.22	0.08	10I	0.80
	1.15 - 2.1	6.27A	0.017A	0.27J	3.6	0.15	0.11	6.2I	1.77
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.31	2.74C	40.9	13I	23.2	22.9
	0.31 - 0.47	1.38C	34.6	13.5I	24.9	26.9
	0.47 - 1.15	0.58C	42.9	14.4I	20.2	22.5
	1.15 - 2.1	0.22C	64.7	14.3I	11.9	9.1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.31
	0.31 - 0.47
	0.47 - 1.15
	1.15 - 2.1

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	GW27	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15L1	Base saturation percentage (BSP)
	15N1	Exchangeable sodium percentage (ESP)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded