Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	GW7	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Gessler	Locality:
	Date Desc.:	15/07/93	Elevation:	423 metres
	Map Ref.:	DGPS	Rainfall:	No Data
	Northing/Long.:	6080470 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	541550  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	10.46 % 	Aspect:	16 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.09 m	Very dark greyish brown (10YR3/2-Moist); ; Loam; 
	A2	0.09 - 0.2 m	Brown (10YR5/3-Moist); ; Loam; 2-10%, medium gravelly, 6-20mm, subrounded tabular, 
	reoriented, Shale, coarse fragments; 
	B	0.2 - 0.54 m	Strong brown (7.5YR5/6-Moist); ; Clay loam; 20-50%, coarse gravelly, 20-60mm, subangular 
	tabular, undisturbed, Shale, coarse fragments; 
	C	0.54 -  m	; 
	Morphological Notes
	C	shaly light coloured material
	Observation Notes
	Site Notes

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	GW7	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.09	4.75A	0.33A	2.7J	0.86	1.9	0.01	11.1I	0.09
	0.09 - 0.2	5.04A	0.073A	0.64J	0.83	0.64	0.01	8.7I	0.11
	0.2 - 0.54	5.69A	0.045A	0.55J	2.8	0.87	0.03	8.8I	0.34
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.09	4.66C	46.4	18.9I	19.1	15.6
	0.09 - 0.2	1.41C	50.9	14.9I	19.6	14.6
	0.2 - 0.54	0.56C	68	4.5I	12.7	14.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.09
	0.09 - 0.2
	0.2 - 0.54

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	GW7	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15L1	Base saturation percentage (BSP)
	15N1	Exchangeable sodium percentage (ESP)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded