Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	LS27	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	McKane, Dermot	Locality:
	Date Desc.:	15/07/93	Elevation:	266 metres
	Map Ref.:	Sheet No. : 8427   DGPS	Rainfall:	No Data
	Northing/Long.:	6102430 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	548631  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Quartz 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	5 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Kurosol Thin Gravelly Loamy Clayey 	Principal Profile Form:	N/A
	Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.07 m	Strong brown (7.5YR4/6-Moist); ; Loam; Massive grade of structure; Earthy fabric; Dry; Very 
	weak consistence; 10-20%, fine gravelly, 2-6mm, subangular, dispersed, coarse fragments; 
	Field pH 5.5 (Raupach); Common, very fine (0-1mm) roots; 
	A2	0.07 - 0.26 m	Brown (7.5YR5/4-Moist); ; Coarse sandy clay loam; Massive grade of structure; Earthy fabric; 
	Dry; Very weak consistence; 50-90%, medium gravelly, 6-20mm, subangular, dispersed, 
	coarse fragments; Field pH 5 (Raupach); Common, very fine (0-1mm) roots; 
	B21	0.26 - 0.55 m	Red (2.5YR4/8-Moist); ; Light medium clay; Moderate grade of structure, 2-5 mm, Angular 
	blocky; Smooth-ped fabric; Dry; Firm consistence; Field pH 4.5 (Raupach); Few, very fine (0-
	1mm) roots; 
	C	0.55 - 0.8 m	Red (2.5YR4/8-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Dry; Very weak 
	consistence; 20-50%, medium gravelly, 6-20mm, subangular, dispersed, coarse fragments; 
	Field pH 4.5 (Raupach); 
	Morphological Notes
	A1	Hydrophobic.                                                                                                                         
	                                                                   
	A2	Hydrophobic (not as bad as layer 1).                                                                                   
	                                                                                 
	Observation Notes
	Site Notes
	A. WAKEHAM, NABILLA                   

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	LS27	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.07	4.96A	0.124A	1.1J	0.53	1.3	0	5.6I	0.00
	0.07 - 0.26	4.83A	0.1A	0.59J	0.39	0.64	0	3.3I	0.00
	0.26 - 0.55	5.01A	0.094A	1.4J	3.6	1.2	0	9.8I	0.00
	0.55 - 0.8	4.94A	0.117A	0.54J	4.6	0.74	0	8.8I	0.00
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.07	2.2C	66I	17	17
	0.07 - 0.26	0.58C	73I	3	24
	0.26 - 0.55	0.51C	44I	12	44
	0.55 - 0.8	0.31C	44I	12	44
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.07
	0.07 - 0.26
	0.26 - 0.55
	0.55 - 0.8

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	LS27	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15L1	Base saturation percentage (BSP)
	15N1	Exchangeable sodium percentage (ESP)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded