Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	LS62	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	McKane, Dermot	Locality:
	Date Desc.:	15/07/93	Elevation:	204 metres
	Map Ref.:	Sheet No. : 8427   DGPS	Rainfall:	No Data
	Northing/Long.:	6106260 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	546960  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	4 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Class Undetermined Red Chromosol Thick 	Principal Profile Form:	N/A
	Non-gravelly Clay-loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (7.5YR3/4-Moist); ; Fine sandy clay loam; Massive grade of structure; Earthy 
	fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 
	100mm2) Fine (1-2mm) macropores, Very weak consistence; 0-2%, fine gravelly, 2-6mm, 
	subangular platy, dispersed, Siltstone, coarse fragments; Field pH 6 (Raupach); Common, very 
	A2	0.1 - 0.33 m	Reddish yellow (7.5YR6/6-Moist); Pinkish white (7.5YR8/3-Dry); ; Fine sandy loam; Massive 
	grade of structure; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Few (<1 per 100mm2) Fine (1-2mm) macropores, Weak consistence; 2-10%, fine 
	gravelly, 2-6mm, subangular platy, dispersed, Siltstone, coarse fragments; Field pH 6.5 
	(Raupach); Few, very fine (0-1mm) roots; 
	B21	0.33 - 0.63 m	Yellowish red (5YR4/8-Moist); Mottles, 20-50% , Distinct; Mottles, 10-20% , Distinct; Light 
	medium clay; Moderate grade of structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; 
	Very firm consistence; 0-2%, fine gravelly, 2-6mm, subangular platy, dispersed, Siltstone, 
	coarse fragments; Many cutans, >50% of ped faces or walls coated; Field pH 7 (Raupach); 
	B22	0.63 - 1.33 m	Yellowish brown (10YR5/6-Moist); ; Light medium clay; Weak grade of structure, 5-10 mm, 
	Subangular blocky; Smooth-ped fabric; Very firm consistence; Field pH 7 (Raupach); 
	B3	1.33 - 2.1 m	Strong brown (7.5YR5/6-Moist); ; Light clay; Weak grade of structure, 5-10 mm, Subangular 
	blocky; Smooth-ped fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Firm
	 consistence; 2-10%, fine gravelly, 2-6mm, subrounded, dispersed, Siltstone, coarse 
	fragments; Field pH 8 (Raupach); 
	Morphological Notes
	A1	Hydrophobic.                                                                                                                         
	                                                                   
	Observation Notes
	Site Notes
	D. BYE                                

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	LS62	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.98A	0.089A	0.57J	0.19	0.61	0.03	4.4I	0.68
	0.1 - 0.33	5.81A	0.026A	0.69J	0.24	0.28	0.06	2.1I	2.86
	0.33 - 0.63	7.01A	0.033A	5.6J	6.7	1.1	0.36	15.7I	2.29
	0.63 - 1.33	8.24A	0.065A	4.2J	7.2	0.8	0.85	12.5I	6.80
	1.33 - 2.1	8.5A	0.072A	2.6J	5.3	0.46	1	9.4I	10.64
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.66C	73I	3	24
	0.1 - 0.33	0.22C	82I	4	14
	0.33 - 0.63	0.27C	44I	12	44
	0.63 - 1.33	0.11C	44I	12	44
	1.33 - 2.1	0.15C	50I	12	38
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.33
	0.33 - 0.63
	0.63 - 1.33
	1.33 - 2.1

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	LS62	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15L1	Base saturation percentage (BSP)
	15N1	Exchangeable sodium percentage (ESP)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded