Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	LS7	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	McKane, Dermot	Locality:
	Date Desc.:	15/07/93	Elevation:	229 metres
	Map Ref.:	Sheet No. : 8327   DGPS	Rainfall:	No Data
	Northing/Long.:	6104100 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	545497  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Siltstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	11 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Palic Paralithic Leptic Tenosol Thin Gravelly Loamy  Very 	Principal Profile Form:	N/A
	shallow
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.05 m	Dark brown (7.5YR3/4-Moist); ; Sandy loam; Weak grade of structure, 2-5 mm, Granular; 
	Smooth-ped fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 
	per 100mm2) Fine (1-2mm) macropores, Dry; Weak consistence; 10-20%, fine gravelly, 2-6mm, 
	subangular platy, dispersed, coarse fragments; Field pH 4.5 (Raupach); Common, very fine (0-
	1mm) roots; 
	A2	0.05 - 0.19 m	Dark brown (7.5YR3/4-Moist); ; Sandy loam; Weak grade of structure, <2 mm, Granular; 
	Smooth-ped fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Weak 
	consistence; 10-20%, fine gravelly, 2-6mm, subangular platy, dispersed, coarse fragments; 
	Field pH 4.5 (Raupach); Few, very fine (0-1mm) roots; 
	C	0.19 - 0.5 m	Yellowish red (5YR4/6-Moist); ; Clay loam, sandy; Weak grade of structure, <2 mm, Granular; 
	Smooth-ped fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Weak 
	consistence; 20-50%, fine gravelly, 2-6mm, subangular platy, dispersed, coarse fragments; 
	Field pH 6 (Raupach); 
	R	0.5 - 0.68 m	Rock 
	Morphological Notes
	A2	Dilatency.                                                                                                                               
	                                                               
	Observation Notes
	Site Notes
	J. DUMARESQ, MONAVALE                 

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	LS7	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.2A	0.276A	6.9J	1.8	2.1	0.24	15.6I	1.54
	0.05 - 0.19	4.87A	0.217A	2.6J	0.59	0.45	0.04	7.9I	0.51
	0.19 - 0.5	5.31A	0.047A	2.4J	0.9	0.43	0.06	7.5I	0.80
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	6.7C	82I	4	14
	0.05 - 0.19	2.22C	82I	4	14
	0.19 - 0.5	2.19C	60I	11	29
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.19
	0.19 - 0.5

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	LS7	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15L1	Base saturation percentage (BSP)
	15N1	Exchangeable sodium percentage (ESP)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded