Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	LS73	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	McKane, Dermot	Locality:
	Date Desc.:	15/07/93	Elevation:	234 metres
	Map Ref.:	Sheet No. : 8327   DGPS	Rainfall:	No Data
	Northing/Long.:	6101757 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	542701  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	3 % 	Aspect:	90 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Class Undetermined Brown Dermosol 	Principal Profile Form:	N/A
	Medium Non-gravelly Clay-loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.13 m	Brown (7.5YR5/3-Moist); ; Fine sandy loam; Massive grade of structure; Earthy fabric; Common
	 (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Very weak consistence; Few (2 - 10 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules, strong, segregations;Field pH 6 (Raupach); 
	A2	0.13 - 0.42 m	Very pale brown (10YR7/3-Moist); ; Fine sandy clay loam; Massive grade of structure; Earthy 
	fabric; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Weak consistence; 0-2%, 
	fine gravelly, 2-6mm, subrounded, dispersed, coarse fragments; Field pH 6.5 (Raupach); 
	B21	0.42 - 0.82 m	Brownish yellow (10YR6/6-Moist); Mottles, 10-20% , Faint; Light clay; Moderate grade of 
	structure, 2-5 mm, Subangular blocky; Smooth-ped fabric; Dry; Firm consistence; 2-10%, fine 
	gravelly, 2-6mm, subrounded, dispersed, coarse fragments; Few (2 - 10 %), 
	Ferromanganiferous, Fine (0 - 2 mm), Nodules, strong, segregations;Field pH 7 (Raupach); 
	B22	0.82 - 1.2 m	Brownish yellow (10YR6/6-Moist); Mottles, 20-50% , Distinct; Light clay; Strong grade of 
	structure, 5-10 mm, Prismatic; Smooth-ped fabric; Dry; Firm consistence; Many (20 - 50 %), 
	Ferromanganiferous, Fine (0 - 2 mm), Nodules, strong, segregations;Many (20 - 50 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules, strong, segregations;Field pH 7 (Raupach); 
	B23	1.2 - 1.6 m	Brownish yellow (10YR6/8-Moist); Mottles, 10-20% , Distinct; Light medium clay; Weak grade of
	 structure, 2-5 mm, Subangular blocky; Smooth-ped fabric; Dry; Strong consistence; Field pH 
	7.5 (Raupach); 
	B3	1.6 - 3 m	Brownish yellow (10YR6/8-Moist); Mottles, 20-50% , Distinct; Light medium clay; Moderate 
	grade of structure, 2-5 mm, Subangular blocky; Smooth-ped fabric; Dry; Strong consistence; 0-
	2%, fine gravelly, 2-6mm, subrounded, dispersed, coarse fragments; Field pH 7.5 (Raupach); 
	Morphological Notes
	A1	Hydrophobic.                                                                                                                         
	                                                                   
	Observation Notes
	Site Notes
	S. CLARK, SAMARA                      

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	LS73	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	4.98A	0.048A	0.34J	0.11	0.21	0.05	4I	1.25
	0.13 - 0.42	5.7A	0.065A	0.5J	0.11	0.12	0.16	1.5I	10.67
	0.42 - 0.82	6.71A	0.025A	1.7J	2.8	0.32	0.27	6.9I	3.91
	0.82 - 1.2	7.31A	0.06A	4.9J	6.4	0.41	1.2	14.4I	8.33
	1.2 - 1.6	8.18A	0.061A	7.6J	10.7	0.53	2.4	21.9I	10.96
	1.6 - 3	8.4A	0.07A	6.3J	9	0.41	2.3	17.9I	12.85
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13	0.84C	82I	4	14
	0.13 - 0.42	0.18C	73I	3	24
	0.42 - 0.82	0.06C	50I	12	38
	0.82 - 1.2	0.14C	50I	12	38
	1.2 - 1.6	0.1C	44I	12	44
	1.6 - 3	0.07C	44I	12	44
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.42
	0.42 - 0.82
	0.82 - 1.2
	1.2 - 1.6
	1.6 - 3

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	LS73	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15L1	Base saturation percentage (BSP)
	15N1	Exchangeable sodium percentage (ESP)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded