Project Name:	CAN
	Project Code:	CAN	Site ID:	C230	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	R.W. Jessup	Locality:	1.6km south-west of Thalgarah Station, Armidale-
	Rockvale Road:
	Date Desc.:	01/01/54	Elevation:	No Data
	Map Ref.:	Sheet No. : 9237   1:100000	Rainfall:	0
	Northing/Long.:	151.833333333333	Runoff:	No Data
	Easting/Lat.:	-30.4166666666667	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Detrital sedimentary rock (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dd2.43
	ASC Confidence:	Great Soil Group:	Solodic soil
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark grey (10YR4/1-Moist); Light brownish grey (10YR6/2-Dry); ; Silty loam; Moderate grade of 
	structure, 2-5 mm, Subangular blocky; Diffuse change to - 
	A2cb	0.1 - 0.17 m	White (10YR8/1-Dry); , 10YR64; Silty loam; Massive grade of structure; Clear change to - 
	B1	0.17 - 0.38 m	Very dark greyish brown (2.5Y3/2-Moist); , 10YR71; , 10YR66; Light clay; Moderate grade of 
	structure, 10-20 mm, Prismatic; 2-10%, medium gravelly, 6-20mm, subangular, dispersed, 
	Detrital sedimentary rock (unidentified), coarse fragments; 
	B2	0.38 - 0.99 m	Strong brown (7.5YR5/8-Moist); , 10YR71; Light clay; Massive grade of structure; 0-2%, medium 
	gravelly, 6-20mm, subangular, dispersed, Detrital sedimentary rock (unidentified), coarse 
	fragments; 
	Morphological Notes
	Observation Notes
	JINGELLA FAMILY:                                                                                                        
	Site Notes
	ARMIDALE

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C230	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.6H	 0.034B	 8.7K	 3.3	 0.52	 0.86	 6.8D
	0.1 - 0.17	7.1H	 0.032B
	0.17 - 0.38	8.3H	 0.074B	 4.4K	 3.7	 0.15	 2.2
	0.38 - 0.99	8.8H	 0.18B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.024F	 0.235B	 0.28B	 6C	 28	 37	 27
	0.1 - 0.17	 5C	 30	 39	 26
	0.17 - 0.38	 0.01C	 0.011F	 0.052B	 0.46B	 5C	 24	 29	 41
	0.38 - 0.99	 0.01C	 3C	 31	 27	 38
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.17
	0.17 - 0.38
	0.38 - 0.99

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C230	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded