Project Name:	CAN
	Project Code:	CAN	Site ID:	C522	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	J. Loveday	Locality:	Tubbo site 7A-AM
	Date Desc.:	01/12/61	Elevation:	 150 metres
	Map Ref.:	Sheet No. : 8128   1:100000	Rainfall:	410
	Northing/Long.:	146.075277777778	Runoff:	Very slow
	Easting/Lat.:	-34.7141666666667	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	<1 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Calcic Brown Chromosol     	Principal Profile Form:	Db2.33
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Irrigated, past or present
	Vegetation:	Low Strata - Forb, <0.25m, Closed or dense. *Species includes - None recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	0 - 0.15 m	Greyish brown (10YR5/2-Dry); ; Loamy sand; Massive grade of structure; Firm consistence; Field
	 pH 5.8 (pH meter); 
	0.15 - 0.2 m	Light brownish grey (10YR6/2-Dry); , 10YR72; Loamy sand; Massive grade of structure; Very firm 
	consistence; 
	0.2 - 0.3 m	Dark brown (10YR3/3-Dry); ; Sandy light clay; 5-10 mm, Angular blocky; 20-50 mm, Prismatic; 
	Very strong consistence; Field pH 7.7 (pH meter); 
	0.3 - 0.46 m	Dark brown (10YR3/3-Dry); , 7.5YR44; Sandy light clay; 20-50 mm, Prismatic; Strong 
	consistence; Very few (0 - 2 %), Calcareous, , ; 
	0.46 - 0.76 m	Brown (7.5YR4/4-Dry); , 10YR33; , 10YR54; Sandy medium clay; , Angular blocky; Few (2 - 10 
	%), Calcareous, , Concretions; 
	0.76 - 1.22 m	Greyish brown (2.5Y5/2-Moist); , 10YR54; Sandy medium clay; Few (2 - 10 %), Calcareous, , 
	Concretions; Few (2 - 10 %), Gypseous, Fine (0 - 2 mm), Crystals; 
	Morphological Notes
	Observation Notes
	Site Notes
	COLEAMBALLY

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C522	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.025	5.5A	 0.12A
	0.025 - 0.1	6A	 0.03A	 5.6K	 1.2	 0.42	 0.09	 3E	 10.3B
	0.1 - 0.2
	0.2 - 0.3	7.7A	 0.09A	 14.3K	 8.5	 1.1	 0.57	 2.3E	 26.8B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.025	 50D	 28	 9	 12
	0.025 - 0.1	 0.72F	 49D	 28	 9	 11
	0.1 - 0.2
	0.2 - 0.3	 25D	 14	 8	 50
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.025
	0.025 - 0.1
	0.1 - 0.2
	0.2 - 0.3

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C522	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6_DC	Organic carbon (%) - Dry combustion
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance