Project Name:	CAN
	Project Code:	CAN	Site ID:	C526	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	J. Loveday	Locality:	Tubbo site 10A-AM
	Date Desc.:	01/12/61	Elevation:	 150 metres
	Map Ref.:	Sheet No. : 8128   1:100000	Rainfall:	410
	Northing/Long.:	146.090555555556	Runoff:	Very slow
	Easting/Lat.:	-34.6877777777778	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	<1 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Calcic Red Chromosol     	Principal Profile Form:	Dr2.23
	ASC Confidence:	Great Soil Group:	Red-brown earth
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Irrigated, past or present
	Vegetation:	Low Strata - Forb, <0.25m, Closed or dense. *Species includes - None recorded
	Surface Coarse Fragments:	2-10%, fine gravelly, 2-6mm, , Quartz
	Profile Morphology
	0 - 0.15 m	Brown (10YR4/3-Moist); , 10YR33, 20-50% ; , 10YR64, 20-50% ; Sandy loam; Weak grade of 
	structure, 2-5 mm, Subangular blocky; Firm consistence; 2-10%, fine gravelly, 2-6mm, 
	dispersed, Quartz, coarse fragments; Field pH 5.9 (pH meter); 
	0.15 - 0.2 m	Brown (10YR4/3-Moist); ; Sandy loam; Weak grade of structure, 2-5 mm, Subangular blocky; 
	Firm consistence; 
	0.2 - 0.25 m	Strong brown (7.5YR5/6-Moist); ; Sandy clay loam; Weak grade of structure, 2-5 mm, Subangular
	 blocky; Common cutans, 10-50% of ped faces or walls coated, distinct; Field pH 7 (pH meter); 
	Common, coarse (>5mm) roots; 
	0.25 - 0.41 m	Dark reddish brown (2.5YR3/4-Moist); , 2.5YR44, 20-50% ; , 20-50% ; Light medium clay; 5-10 
	mm, Angular blocky; 10-20 mm, Prismatic; Few, coarse (>5mm) roots; 
	0.41 - 0.61 m	Reddish brown (5YR4/4-Moist); , 10YR43; Light medium clay; Very few (0 - 2 %), Calcareous, , 
	Concretions; Few, coarse (>5mm) roots; 
	0.61 - 0.91 m	Yellowish brown (10YR5/5-Moist); , 2.5Y44; Silty medium clay; Few (2 - 10 %), Calcareous, , 
	Concretions; 
	0.91 - 1.07 m	Olive brown (2.5Y4/4-Moist); ; Sandy medium clay; Very few (0 - 2 %), Calcareous, , Concretions; 
	1.07 - 1.27 m	Reddish brown (5YR4/4-Moist); , 10YR55, 20-50% ; , 20-50% ; Coarse sand; 
	Morphological Notes
	Observation Notes
	CHARCOAL & BAKED SOIL ESP. 15-30CM:LENSES OF OLIVE BROWN SANDY & SILTY CLAY 107-127CM:SL. BLACK 
	STAINING 61-91CM        
	Site Notes
	COLEAMBALLY

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C526	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.025	5.3A	 0.12A	 6.7K	 1.2	 0.45	 0.03	 6.6E	 15B
	0.025 - 0.1	6A	 0.03A	 7.4K	 1.7	 0.7	 0	 5E	 14.8B
	0.1 - 0.2
	0.2 - 0.3	7A	 0.03A	 13.5K	 4.7	 0.94	 0.04	 3.9E	 23.1B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.025	 1.21F	 34D	 30	 22	 16
	0.025 - 0.1	 0.83F	 34D	 31	 20	 16
	0.1 - 0.2
	0.2 - 0.3	 23D	 24	 16	 36
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.025
	0.025 - 0.1
	0.1 - 0.2
	0.2 - 0.3

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C526	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6_DC	Organic carbon (%) - Dry combustion
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance