Project Name:	CAN
	Project Code:	CAN	Site ID:	CP99	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	J. Loveday	Locality:	Yanco Agricultural Exp. Farm S. of Orange Orchard &
	 gum trees left sideof road
	Date Desc.:	09/10/78	Elevation:	No Data
	Map Ref.:	Sheet No. : 8128   1:100000	Rainfall:	430
	Northing/Long.:	146.416666666667	Runoff:	Slow
	Easting/Lat.:	-34.6166666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Alluvial plain
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Subnatric Red Sodosol     	Principal Profile Form:	Dr2.13
	ASC Confidence:	Great Soil Group:	Red-brown earth
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Irrigated, past or present
	Vegetation:	Low Strata - Forb, <0.25m, Mid-dense. *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.1 m	Brown (7.5YR4/4-Moist); ; Clay loam; Weak grade of structure, 200-500 mm, Angular blocky; Dry;
	 Firm consistence; Field pH 6.6 (pH meter); 
	0.1 - 0.2 m	Brown (7.5YR4/4-Moist); ; Clay loam; Weak grade of structure, 200-500 mm, Angular blocky; 
	Firm consistence; Field pH 6.9 (pH meter); Sharp change to - 
	B2	0.2 - 0.3 m	Dark red (2.5YR3/6-Moist); ; Heavy clay; Weak grade of structure, 200-500 mm, Angular blocky; 
	Wet; Loose consistence; Field pH 7.9 (pH meter); 
	0.3 - 0.4 m	Dark red (2.5YR3/6-Moist); ; Heavy clay; Weak grade of structure, 200-500 mm, Angular blocky; 
	Loose consistence; Field pH 8.4 (pH meter); 
	0.4 - 0.5 m	Dark red (2.5YR3/6-Moist); ; Heavy clay; Weak grade of structure, 200-500 mm, Angular blocky; 
	Loose consistence; Field pH 8.7 (pH meter); Gradual change to - 
	0.5 - 0.6 m	Yellowish red (5YR4/6-Moist); ; Heavy clay; Loose consistence; Very few (0 - 2 %), Calcareous, ,
	 Soft segregations; Field pH 9 (pH meter); 
	0.6 - 0.7 m	Yellowish red (5YR4/6-Moist); ; Heavy clay; Loose consistence; Very few (0 - 2 %), Calcareous, ,
	 Soft segregations; Field pH 9.1 (pH meter); 
	0.7 - 0.8 m	Yellowish red (5YR4/6-Moist); ; Heavy clay; Loose consistence; Few (2 - 10 %), Calcareous, , 
	Soft segregations; Field pH 9.2 (pH meter); 
	0.8 - 0.9 m	Yellowish red (5YR4/6-Moist); ; Heavy clay; Loose consistence; Few (2 - 10 %), Calcareous, , 
	Soft segregations; Field pH 9.4 (pH meter); 
	0.9 - 1 m	Yellowish red (5YR4/6-Moist); ; Heavy clay; Loose consistence; Common (10 - 20 %), 
	Calcareous, , Soft segregations; Field pH 9.3 (pH meter); 
	1 - 1.1 m	Yellowish red (5YR4/6-Moist); ; Light clay; Weak consistence; Common (10 - 20 %), 
	Calcareous, , Concretions; Field pH 9.4 (pH meter); 
	1.1 - 1.2 m	Yellowish red (5YR5/8-Moist); ; Light clay; Weak consistence; Common (10 - 20 %), 
	Calcareous, , Concretions; Field pH 9.5 (pH meter); 

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP99	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	1.2 - 1.3 m	Yellowish red (5YR5/8-Moist); ; Light clay; Weak consistence; Common (10 - 20 %), 
	Calcareous, , Concretions; Field pH 9.5 (pH meter); 
	1.3 - 1.4 m	Yellowish red (5YR5/8-Moist); ; Light clay; Weak consistence; Common (10 - 20 %), 
	Calcareous, , Concretions; Field pH 9.5 (pH meter); 
	1.4 - 1.5 m	Yellowish red (5YR5/8-Moist); , 2-10% ; , 2-10% ; Light clay; Weak consistence; Few (2 - 10 %), 
	Calcareous, , Concretions; Field pH 9.4 (pH meter); 
	1.5 - 1.6 m	Yellowish red (5YR5/8-Moist); , 10-20% ; , 10-20% ; Light clay; Weak consistence; Few (2 - 10 
	%), Calcareous, , Concretions; Field pH 9.3 (pH meter); 
	1.6 - 1.7 m	Light olive brown (2.5Y5/4-Moist); , 5YR58, 20-50% ; , 20-50% ; Light clay; Weak consistence; 
	Field pH 9.1 (pH meter); 
	1.7 - 1.8 m	Light olive brown (2.5Y5/4-Moist); , 5YR58, 20-50% ; , 20-50% ; Light clay; Weak consistence; 
	Field pH 9 (pH meter); 
	1.8 - 1.9 m	Light olive brown (2.5Y5/4-Moist); , 5YR58, 20-50% ; , 20-50% ; Light clay; Weak consistence; 
	Field pH 9.1 (pH meter); 
	1.9 - 2 m	Light olive brown (2.5Y5/4-Moist); , 5YR58, 20-50% ; , 20-50% ; Light clay; Weak consistence; 
	Field pH 9 (pH meter); 
	Morphological Notes
	Observation Notes
	ALLUVIUM                                                                                                                
	Site Notes
	YANCO

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP99	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.6A	 0.04A	 4.3K	 2.8	 0.55	 0.3	 8B	 16J	1.88
	0.1 - 0.2	6.9A	 0.05A	 4K	 3	 0.55	 0.56	 6.9B	 15J	3.73
	0.2 - 0.3	7.9A	 0.06A	 8.4K	 8.6	 0.64	 1.5	 7.9B	 27J	5.56
	0.3 - 0.4	8.4A	 0.7A	 9.2K	 10.9	 0.59	 2.1	 7.7B	 30.5J	6.89
	0.4 - 0.5	8.7A	 0.8A	 8.8K	 12.2	 0.62	 2.6	 6B	 30.2J	8.61
	0.5 - 0.6	9A	 0.16A	 7.8K	 13	 0.63	 3	 5.3B	 29.7J	10.10
	0.6 - 0.7	9.1A	 0.29A	 7.3K	 13.3	 0.63	 3.2	 4B	 28.4J	11.27
	0.7 - 0.8	9.2A	 0.31A	 6.5K	 12.3	 0.64	 3.3	 4.4B	 27.1J	12.18
	0.8 - 0.9	9.4A	 0.33A	 5.9K	 13.2	 0.7	 4.1	 3B	 26.9J	15.24
	0.9 - 1	9.3A	 0.33A	 5.7K	 12.7	 0.66	 3.9	 2.6B	 25.6J	15.23
	1 - 1.1	9.4A	 0.33A
	1.1 - 1.2	9.5A	 0.33A	 5.2K	 11.5	 0.67	 4.3	 2.2B	 23.9J	17.99
	1.2 - 1.3	9.5A	 0.32A
	1.3 - 1.4	9.5A	 0.32A
	1.4 - 1.5	9.4A	 0.27A	 5K	 11.7	 0.67	 4.8	 2.3B	 24.5J	19.59
	1.5 - 1.6	9.3A	 0.16A
	1.6 - 1.7	9.1A	 0.15A	 4.4K	 10	 0.63	 4.7	 2.6B	 22.3J	21.08
	1.7 - 1.8	9A	 0.15A
	1.8 - 1.9	9.1A	 0.14A
	1.9 - 2	9A	 0.14A	 4K	 8.8	 0.53	 4.2	 2.2B	 19.7J	21.32
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.2D	 0	 14D	 42	 16	 26
	0.1 - 0.2	 0.82D	 0	 14D	 42	 15	 28
	0.2 - 0.3	 0.05A	 0.64D	 0	 6D	 23	 10	 59
	0.3 - 0.4	 0.07A	 0.61D	 0	 5D	 18	 9	 66
	0.4 - 0.5	 0.06A	 0.43D	 0	 5D	 19	 10	 66
	0.5 - 0.6	 0.26A	 0.3D	 0	 5D	 20	 10	 64
	0.6 - 0.7	 2.41A	 0.21D	 2	 5D	 20	 13	 60
	0.7 - 0.8	 6.32A	 0.18D	 2	 4D	 21	 15	 56
	0.8 - 0.9	 3.54A	 0.12D	 2	 4D	 21	 17	 55
	0.9 - 1	 4.97A	 0.11D	 7	 4D	 23	 18	 50
	1 - 1.1
	1.1 - 1.2	 3.62A	 5	 5D	 27	 19	 45
	1.2 - 1.3
	1.3 - 1.4
	1.4 - 1.5	 0.52A	 0	 3D	 25	 27	 43
	1.5 - 1.6
	1.6 - 1.7	 0.12A	 0	 2D	 24	 32	 42
	1.7 - 1.8
	1.8 - 1.9
	1.9 - 2	 0.06A	 0	 2D	 28	 31	 39
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP99	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1
	1 - 1.1
	1.1 - 1.2
	1.2 - 1.3
	1.3 - 1.4
	1.4 - 1.5
	1.5 - 1.6
	1.6 - 1.7
	1.7 - 1.8
	1.8 - 1.9
	1.9 - 2

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP99	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G_C_AL1	Exchangeable aluminium - meq per 100g of soil - Aluminium By difference of C and A or B
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance