Project Name:	GH
	Project Code:	GH	Site ID:	CP3	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	J. Loveday	Locality:	Ben. Exp. 1
	Date Desc.:	01/10/68	Elevation:	 120 metres
	Map Ref.:	Sheet No. : 8029   1:100000	Rainfall:	400
	Northing/Long.:	145.866666666667	Runoff:	Very slow
	Easting/Lat.:	-34.3833333333333	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Slightly porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	<1 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Firm, Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Episodic-Endocalcareous Epipedal Grey Vertosol     	Principal Profile Form:	Ug5.5
	ASC Confidence:	Great Soil Group:	Grey clay
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:	Low Strata - Sod grass, , . *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Dark greyish brown (2.5Y4/2-Moist); , 10YR54; Medium heavy clay; 50-100 mm, Angular blocky; 
	Medium, (5 - 10) mm crack; Very firm consistence; Field pH 7.6 (pH meter); 
	0.1 - 0.2 m	Dark greyish brown (2.5Y4/2-Moist); , 5Y41; Medium heavy clay; 50-100 mm, Angular blocky; 
	Very firm consistence; 
	0.2 - 0.3 m	Dark greyish brown (2.5Y4/2-Moist); ; Medium heavy clay; 50-100 mm, Angular blocky; Very firm 
	consistence; Field pH 8.3 (pH meter); 
	0.3 - 0.4 m	Dark greyish brown (2.5Y4/2-Moist); ; Medium heavy clay; 50-100 mm, Angular blocky; Very firm 
	consistence; 
	0.4 - 0.5 m	Dark greyish brown (10YR4/2-Moist); ; Medium heavy clay; 50-100 mm, Angular blocky; Very firm 
	consistence; Field pH 8.5 (pH meter); 
	0.5 - 0.6 m	Dark greyish brown (10YR4/2-Moist); , 10YR53; Medium heavy clay; 50-100 mm, Angular blocky; 
	Very firm consistence; 
	0.6 - 0.7 m	Dark greyish brown (10YR4/2-Moist); , 10YR53; Medium heavy clay; 50-100 mm, Angular blocky; 
	Very firm consistence; Field pH 8.1 (pH meter); 
	0.7 - 0.8 m	Brown (10YR5/3-Moist); ; Medium heavy clay; 50-100 mm, Angular blocky; Very firm 
	consistence; Few (2 - 10 %), Calcareous, , Soft segregations; 
	0.8 - 0.9 m	Brown (10YR5/3-Moist); , 2.5Y53; Medium heavy clay; 50-100 mm, Angular blocky; Very firm 
	consistence; Few (2 - 10 %), Gypseous, , ; Field pH 7.3 (pH meter); 
	0.9 - 1 m	Greyish brown (2.5Y5/3-Moist); , 10YR21; Medium heavy clay; 50-100 mm, Angular blocky; Weak
	 consistence; Many (20 - 50 %), Gypseous, , ; 
	Morphological Notes
	Observation Notes
	ALLUVIUM                                                                                                                
	Site Notes
	BEHEREMBAH

	Project Name:	GH
	Project Code:	GH	Site ID:	CP3	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)

	Project Name:	GH
	Project Code:	GH	Site ID:	CP3	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7.6A	 0.12A	 10.3K	 9.7	 1.1	 1.6	4D	 27J	5.93
	7.4A	0.06A	10K	10.3	1.1	1.3	26.7J	4.87
	0 - 0.1	7.6A	 0.12A	 10.3K	 9.7	 1.1	 1.6	4D	 27J	5.93
	7.4A	0.06A	10K	10.3	1.1	1.3	26.7J	4.87
	0.2 - 0.3	8.3A	 0.13A	 11.9K	 11.7	 0.78	 3.7	 30.8J	12.01
	0.4 - 0.5	8.5A	 0.39A
	0.6 - 0.7	8.1A	 0.87A
	0.8 - 0.9	7.3A	 2.29A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.87D	 19A	 6D	 32	 14	 48
	0.88D	20.1A	6D	33	11	50
	0 - 0.1	 0.87D	 19A	 6D	 32	 14	 48
	0.88D	20.1A	6D	33	11	50
	0.2 - 0.3	 0.05A	 5A
	0.4 - 0.5	 2A
	0.6 - 0.7	 2A
	0.8 - 0.9	 4A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0 - 0.1
	0.2 - 0.3
	0.4 - 0.5
	0.6 - 0.7
	0.8 - 0.9

	Project Name:	GH
	Project Code:	GH	Site ID:	CP3	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance