Project Name:	GH
	Project Code:	GH	Site ID:	CP4	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	J. Loveday	Locality:	.35 mile down and across road from Willbriggie 
	siding wheat storage
	Date Desc.:	02/10/68	Elevation:	 120 metres
	Map Ref.:	Sheet No. : 8029   1:100000	Rainfall:	400
	Northing/Long.:	146	Runoff:	Very slow
	Easting/Lat.:	-34.4666666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Slightly porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	<1 % 	Aspect:	125 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Hypercalcic Subnatric Red Sodosol     	Principal Profile Form:	Dr2.33
	ASC Confidence:	Great Soil Group:	Red-brown earth
	All necessary analytical data are available.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.06 m	Brown (7.5YR4/3-Moist); ; Clay loam; 20-50 mm, Angular blocky; Weak consistence; Field pH 
	6.8 (pH meter); Sharp change to - 
	0.06 - 0.1 m	Dark reddish brown (5YR3/4-Moist); ; Medium clay; 10-20 mm, Prismatic; Weak consistence; 
	Field pH 7.1 (pH meter); 
	0.1 - 0.2 m	Dark reddish brown (5YR3/4-Moist); ; Medium clay; 20-50 mm, Prismatic; Weak consistence; 
	0.2 - 0.3 m	Reddish brown (5YR4/3-Moist); ; Medium clay; 20-50 mm, Angular blocky; Weak consistence; 
	Few (2 - 10 %), Calcareous, , Soft segregations; Field pH 8.2 (pH meter); 
	0.3 - 0.4 m	Reddish brown (5YR4/3-Moist); ; Medium clay; 20-50 mm, Angular blocky; Weak consistence; 
	Few (2 - 10 %), Calcareous, , Soft segregations; Field pH 8.3 (pH meter); 
	0.4 - 0.5 m	Reddish brown (5YR4/4-Moist); ; Medium clay; Massive grade of structure; Weak consistence; 
	Few (2 - 10 %), Calcareous, , Soft segregations; Field pH 8.4 (pH meter); 
	0.5 - 0.6 m	Brown (7.5YR5/4-Moist); ; Medium clay; Massive grade of structure; Weak consistence; Many (20
	 - 50 %), Calcareous, , Soft segregations; 
	0.6 - 0.7 m	Brown (10YR5/3-Moist); , 7.5YR56; Light clay; , Angular blocky; Weak consistence; Few (2 - 10 
	%), Calcareous, , Soft segregations; Field pH 8.1 (pH meter); 
	0.7 - 0.8 m	Brown (10YR5/3-Moist); , 10YR42; , 7.5YR56; Light clay; , Angular blocky; Weak consistence; 
	Few (2 - 10 %), Calcareous, , Soft segregations; 
	0.8 - 0.9 m	Brown (10YR5/3-Moist); , 10YR42; , 7.5YR56; Light clay; , Angular blocky; Very weak 
	consistence; Few (2 - 10 %), Calcareous, , Soft segregations; Very few (0 - 2 %), Gypseous, , ; 
	Field pH 7.8 (pH meter); 
	Morphological Notes
	Observation Notes
	PARNA AND ALLUVIUM LAYERS RE NUMBERED 21/10/92                                                                          
	Site Notes
	WILLBRIGGIE

	Project Name:	GH
	Project Code:	GH	Site ID:	CP4	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)

	Project Name:	GH
	Project Code:	GH	Site ID:	CP4	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	6.8A	 0.06A	 3.7K	 2.9	 0.8	 0.54	 12.2J	4.43
	0 - 0.1	7.1A	0.06A	5.6K	6.2	1.1	1.3	4D	18.2J	7.14
	0.06 - 0.1	7.1A	 0.06A	 8.3K	 7.7	 1.2	 2.2	 29.1J	7.56
	0.2 - 0.3	8.2A	 0.35A	 11.8K	 14.1	 1.2	 4.8	 35.8J	13.41
	0.3 - 0.4	8.3A	 0.76A	 10K	 18	 1.3	 6.3	 36J	17.50
	0.4 - 0.5	8.4A	 1.39A
	0.6 - 0.7	8.1A	 1.85A
	0.8 - 0.9	7.8A	 2.64A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06	 0.81D	 6A	 16D	 49	 17	 18
	0 - 0.1	0.85D	5.1A	13D	41	12	34
	0.06 - 0.1	 0.77D	 3A	 9D	 29	 10	 53
	0.2 - 0.3	 0.06A	 2A
	0.3 - 0.4	 0.13A
	0.4 - 0.5	 3A
	0.6 - 0.7	 3A
	0.8 - 0.9	 3A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0 - 0.1
	0.06 - 0.1
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.6 - 0.7
	0.8 - 0.9

	Project Name:	GH
	Project Code:	GH	Site ID:	CP4	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance