Project Name:	GH
	Project Code:	GH	Site ID:	CP7	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	J. Loveday	Locality:	Slightly W. of end of irrigation Warrawidgee 
	Date Desc.:	03/10/68	Elevation:	 120 metres
	Map Ref.:	Sheet No. : 7929   1:100000	Rainfall:	400
	Northing/Long.:	145.25	Runoff:	Very slow
	Easting/Lat.:	-34.2833333333334	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Slightly porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	<1 % 	Aspect:	225 degrees
	Surface Soil Condition (dry):	Cracking, Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Mesonatric Grey Sodosol     	Principal Profile Form:	Db1.33
	ASC Confidence:	Great Soil Group:	Red-brown earth
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.03 m	Brown (7.5YR4/3-Moist); , 10YR52; Fine sandy loam; Massive grade of structure; Fine, (0 - 5) 
	mm crack; Weak consistence; Field pH 6.2 (pH meter); Sharp change to - 
	0.03 - 0.1 m	Brown (7.5YR4/2-Moist); ; Medium heavy clay; 20-50 mm, Angular blocky; Very firm consistence;
	 Field pH 6.9 (pH meter); 
	0.1 - 0.2 m	Brown (7.5YR4/2-Moist); ; Medium heavy clay; 20-50 mm, Angular blocky; Very firm consistence;
	 
	0.2 - 0.3 m	Brown (7.5YR4/2-Moist); ; Medium heavy clay; Massive grade of structure; Very firm consistence;
	 Field pH 8.2 (pH meter); 
	0.3 - 0.4 m	Brown (7.5YR4/2-Moist); ; Medium heavy clay; Massive grade of structure; Very firm consistence;
	 Few (2 - 10 %), Calcareous, , Concretions; Field pH 8.4 (pH meter); 
	0.4 - 0.5 m	Brown (10YR4/3-Moist); ; Medium heavy clay; Massive grade of structure; Very firm consistence; 
	Few (2 - 10 %), Calcareous, , Concretions; Field pH 8.1 (pH meter); 
	0.5 - 0.6 m	Brown (10YR5/3-Moist); ; Medium heavy clay; Massive grade of structure; Very firm consistence; 
	Few (2 - 10 %), Calcareous, , Soft segregations; 
	0.6 - 0.7 m	Brown (10YR5/3-Moist); , 10YR21; Medium heavy clay; 10-20 mm, Angular blocky; Very firm 
	consistence; Few (2 - 10 %), Calcareous, , Soft segregations; Field pH 7.5 (pH meter); 
	0.7 - 0.8 m	Brown (10YR5/3-Moist); , 10YR21; Medium clay; 10-20 mm, Angular blocky; Very firm 
	consistence; Few (2 - 10 %), Calcareous, , Soft segregations; Few (2 - 10 %), Gypseous, , ; 
	0.8 - 0.9 m	Greyish brown (2.5Y5/2-Moist); , 10YR21; Light medium clay; 10-20 mm, Angular blocky; Very 
	firm consistence; Few (2 - 10 %), Calcareous, , Soft segregations; Few (2 - 10 %), Gypseous, , ; 
	Field pH 7.2 (pH meter); 
	Morphological Notes
	Observation Notes
	ALLUVIUM  LAYERS RE NUMBERED 21/10/92                                                                                   
	Site Notes
	WARRAWIDGEE

	Project Name:	GH
	Project Code:	GH	Site ID:	CP7	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)

	Project Name:	GH
	Project Code:	GH	Site ID:	CP7	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	6.2A	 0.15A	 2.4K	 3.4	 1.1	 0.65	 13.8J	4.71
	0 - 0.1	6.9A	0.15A	6.1K	8.9	1.1	1.9	4.3D	22.3J	8.52
	0.03 - 0.1	6.9A	 0.12A	 6.6K	 9.4	 1.1	 2.4	 25.4J	9.45
	0.2 - 0.3	8.2A	 0.69A	 9.4K	 12.2	 0.68	 5.9	 28.7J	20.56
	0.3 - 0.4	8.4A	 1A	 8K	 14	 0.76	 7.2	 29J	24.83
	0.4 - 0.5	8.1A	 1.47A
	0.6 - 0.7	7.5A	 2.23A
	0.8 - 0.9	7.2A	 3A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03	 1.3D	 18A	 17D	 41	 17	 25
	0 - 0.1	0.9D	10.6A	12D	32	12	44
	0.03 - 0.1	 0.79D	 5A	 6D	 33	 14	 46
	0.2 - 0.3	 0.05A	 2A
	0.3 - 0.4	 0.03A
	0.4 - 0.5	 5A
	0.6 - 0.7	 10A
	0.8 - 0.9	 17A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0 - 0.1
	0.03 - 0.1
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.6 - 0.7
	0.8 - 0.9

	Project Name:	GH
	Project Code:	GH	Site ID:	CP7	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance