Project Name:	Handbook of Australian Soils
	Project Code:	HAS	Site ID:	A1011	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	151.18333333	Runoff:	No Data
	Easting/Lat.:	-29.716666667	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	; 
	0.1 - 0.2 m	; 
	0.2 - 0.46 m	; 
	0.46 - 0.61 m	; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Handbook of Australian Soils
	Project Code:	HAS	Site ID:	A1011	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.1J	 0.073A	 12B	 5.9	 1.5	 0.08	 30J	0.27
	6.8A
	0.1 - 0.2	5.7J	 0.046A	 7.6B	 4.9	 0.95	 0.09	 28J	0.32
	6.7A
	0.2 - 0.46	5.3J	 0.324A
	5.7A
	0.46 - 0.61	5.2J	 0.184A	 4B	 6.5	 0.23	 0.47
	5.7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 2.56A	 16A	 0.06A	 0.17B	 0.37A	 18	 30C	 13	 14	 39
	0.1 - 0.2	 1.16A	 5A	 0.04A	 0.082B	 0.28A	 9	 26C	 10	 11	 51
	0.2 - 0.46	 0.581A	 3A	 0.03A	 0.037B	 0.26A	 8	 22C	 9	 10	 57
	0.46 - 0.61	 0.349A	 0.02A	 0.021B	 0.34A	 2	 24C	 9	 12	 52
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.46
	0.46 - 0.61

	Project Name:	Handbook of Australian Soils
	Project Code:	HAS	Site ID:	A1011	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	17A1	Total potassium - X-ray fluorescence
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B_C_2.5	pH of soil - pH of 1:2.5 Soil/0.1M CaCl2 suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A1	Total phosphorus - X-ray fluorescence
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	MIN_NR_K2O	Kaolin minerals
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Hm	Hematite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction