Project Name:	MUR
	Project Code:	MUR	Site ID:	C108	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	H.M. Churchwood	Locality:	90m from west bndry,20m Sof Thule Rd, Portion 13 
	Hundred of Whymoul
	Date Desc.:	14/10/53	Elevation:	 76 metres
	Map Ref.:	Sheet No. : 7826   1:100000	Rainfall:	355
	Northing/Long.:	144.5	Runoff:	Rapid
	Easting/Lat.:	-35.5	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Red-brown earth
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.12 m	Yellowish brown (10YR5/4-Moist); ; Loam; Weak grade of structure, 20-50 mm, Subangular 
	blocky; Moderately moist; Strong consistence; 0-2%, fine gravelly, 2-6mm, angular, Quartz, 
	coarse fragments; 
	B11	0.13 - 0.17 m	Dark red (10R3/6-Moist); ; Medium clay; Moderate grade of structure, 50-100 mm, Prismatic; 
	Moderate grade of structure, 20-50 mm, Angular blocky; Moderately moist; Weak consistence; 
	B12	0.17 - 0.27 m	Red (2.5YR5/6-Moist); ; Medium clay; Moderate grade of structure, 100-200 mm, Prismatic; 
	Moderate grade of structure, 20-50 mm, Angular blocky; Moderately moist; Weak consistence; 
	B21	0.33 - 0.48 m	Yellowish brown (10YR5/6-Moist); , 10YR76; Medium clay (Light); Moderate grade of structure, 
	20-50 mm, Angular blocky; Moderately moist; Weak consistence; Common (10 - 20 %), 
	Calcareous, , Concretions; 
	D11	0.53 - 0.63 m	Pale yellow (2.5Y7/4-Moist); , 2.5YR58; , 5Y72; Sandy light medium clay; Weak grade of 
	structure, 10-20 mm, Subangular blocky; Moderately moist; Weak consistence; Very few (0 - 2 
	%), Calcareous, , Soft segregations; 
	D12	0.73 - 0.83 m	Pale yellow (2.5Y7/4-Moist); , 2.5Y46; Sandy light medium clay; Weak grade of structure, 5-10 
	mm, Subangular blocky; Moist; Weak consistence; 
	D13	0.88 - 1.04 m	Pale yellow (2.5Y7/4-Moist); , 2.5YR66; , 5Y72; Sandy light medium clay; Weak grade of 
	structure, 5-10 mm, Angular blocky; Moist; Weak consistence; 
	D21	1.21 - 1.42 m	White (5Y8/2-Moist); , 5Y72; , 7.5YR68; Sandy light medium clay; Moderately moist; Weak 
	consistence; 0-2%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; Very few (0 - 2 %), 
	Calcareous, , Soft segregations; 
	D22	1.52 - 1.72 m	White (5Y8/2-Moist); , 10YR78; , 5YR36; Light clay; Moderately moist; Weak consistence; 0-2%,
	 fine gravelly, 2-6mm, angular, Quartz, coarse fragments; Very few (0 - 2 %), Ferruginous, , 
	Concretions; 
	D23	1.82 - 2.03 m	Light grey (5Y7/2-Moist); , 10YR68; , 2.5YR68; Medium clay (Light); Moderately moist; Weak 
	consistence; 0-2%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; Few (2 - 10 %), 
	Ferruginous, , Concretions; 

	Project Name:	MUR
	Project Code:	MUR	Site ID:	C108	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	D24	2.1 - 2.43 m	Pale yellow (5Y7/3-Moist); , 10YR68; Sandy light medium clay; Moderately moist; Weak 
	consistence; 0-2%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; 
	D25	2.64 - 3.04 m	Yellow (5Y7/8-Moist); , 10YR78; Sandy light medium clay (Light); Moderately moist; Weak 
	consistence; 0-2%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; 
	Morphological Notes
	Observation Notes
	WOMBOOTA LOAM:                                                                                                          
	Site Notes
	WAKOOL

	Project Name:	MUR
	Project Code:	MUR	Site ID:	C108	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	MUR
	Project Code:	MUR	Site ID:	C108	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile