Project Name:	WAG
	Project Code:	WAG	Site ID:	C48	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Site Information
	Desc. By:	Beattie, John	Locality:	.8km w of site 8 on ridge 40m w of lane,15km w of 
	Henty on Pleasant Hills Rd.
	Date Desc.:	11/01/57	Elevation:	 274 metres
	Map Ref.:	Sheet No. : 8327   1:100000	Rainfall:	570
	Northing/Long.:	147	Runoff:	Rapid
	Easting/Lat.:	-35.25	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Shale 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	No Data	Relief:	61 metres
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:	Low Strata - , , . *Species includes - None recorded
	Tall Strata - , , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.05 m	Brown (7.5YR4/3-Moist); ; Loam; Massive grade of structure; Dry; Firm consistence; 10-20%, 
	coarse gravelly, 20-60mm, coarse fragments; 
	A12	0.05 - 0.12 m	Brown (7.5YR5/4-Moist); ; Loam; Massive grade of structure; 20-50%, coarse gravelly, 20-60mm, 
	coarse fragments; 
	A2	0.2 - 0.3 m	Light brown (7.5YR6/4-Moist); ; Loam; Massive grade of structure; 20-50%, coarse gravelly, 20-
	60mm, coarse fragments; 
	B11	0.36 - 0.46 m	Red (2.5YR4/6-Moist); , 2.5YR58; Medium clay; Weak grade of structure, 5-10 mm, Angular 
	blocky; Moist; Firm consistence; 10-20%, coarse gravelly, 20-60mm, coarse fragments; 
	B12	0.58 - 0.68 m	Dark red (10R3/6-Moist); , 2.5YR58; Fine sandy medium clay; Weak grade of structure, 10-20 
	mm, Angular blocky; Moist; Weak consistence; 10-20%, coarse gravelly, 20-60mm, coarse 
	fragments; 
	BC	0.73 - 0.78 m	Yellowish red (5YR3/6-Moist); , 7.5YR58; , 7.5YR68; Fine sandy light clay; Massive grade of 
	structure; 10-20%, coarse gravelly, 20-60mm, coarse fragments; 
	Morphological Notes
	Observation Notes
	MUNDAWADDRY STRONG LOAM; SEE ORIGINAL FOR MORE DETAIL:                                                                  
	Site Notes
	WAGGA

	Project Name:	WAG
	Project Code:	WAG	Site ID:	C48	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAG
	Project Code:	WAG	Site ID:	C48	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NSW)
	Laboratory Analyses Completed for this profile