Project Name:	CAN
	Project Code:	CAN	Site ID:	C124	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	B.E. Butler	Locality:	Parish Wychitella 24:N.E. corner:Lunette on 
	Woolshed Swamp
	Date Desc.:	24/09/55	Elevation:	No Data
	Map Ref.:	Sheet No. : 7625   1:100000	Rainfall:	425
	Northing/Long.:	143.716666666667	Runoff:	Slow
	Easting/Lat.:	-36.1883333333333	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Playa plain
	1-3%
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Lunette	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Epipedal Brown Vertosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Brown clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Sod grass, , . *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.13 m	Greyish brown (2.5Y5/3-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Moist; Weak consistence; Field pH 9.6 (pH meter); Gradual change to - 
	B1	0.13 - 0.36 m	Greyish brown (2.5Y5/3-Moist); ; Light medium clay; <2 mm, Subangular blocky; Moderate grade 
	of structure, 100-200 mm, Prismatic; Moist; Weak consistence; Field pH 9.1 (pH meter); Gradual
	 change to - 
	B2	0.48 - 0.66 m	Light brownish grey (2.5Y6/3-Moist); ; Light medium clay; Moderate grade of structure, 20-50 
	mm, Angular blocky; Moist; Weak consistence; Field pH 9.6 (pH meter); Gradual change to - 
	C	1.07 - 1.17 m	Pale yellow (2.5Y7/3-Moist); ; Light clay; Dry; Very firm consistence; Few (2 - 10 %), Calcareous,
	 , Soft segregations; Field pH 9.2 (pH meter); 
	Morphological Notes
	Observation Notes
	VERY YOUNG PARNA                                                                                                        
	Site Notes
	GLADSTONE COUN

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C124	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	9.6A	 0.33A
	0.13 - 0.36	9.1A	 0.14A
	0.48 - 0.66	9.6A	 0.122A
	1.07 - 1.17	9.2A	 1.32A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13
	0.13 - 0.36
	0.48 - 0.66
	1.07 - 1.17
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.36
	0.48 - 0.66
	1.07 - 1.17

	Project Name:	CAN
	Project Code:	CAN	Site ID:	C124	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour