Project Name:	Lowan, Vic.
	Project Code:	LO1	Site ID:	A933	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	G. Blackburn	Locality:
	Date Desc.:	11/06/64	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	141.58333333	Runoff:	Rapid
	Easting/Lat.:	-36.38333333	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	Ridge	Relief:	3 metres
	Elem. Type:	Lunette	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Surface crust, Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Vertic Calcic Brown Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Brown clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Tall Strata - Tree, , . *Species includes - Eucalyptus species, Casuarina leuhmannii
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.04 m	; Clay loam, fine sandy; Weak grade of structure, 2-5 mm, Angular blocky; Firm consistence; 
	Clear change to - 
	0.04 - 0.12 m	; Medium clay; 10-20 mm, Angular blocky; Very firm consistence; 
	0.12 - 0.26 m	; Medium clay; , Angular blocky; Firm consistence; 
	0.26 - 0.35 m	; Medium clay; Weak consistence; Diffuse change to - 
	0.35 - 0.55 m	; Medium clay; Weak consistence; Very few (0 - 2 %), Calcareous, , Soft segregations; 
	0.55 - 0.68 m	; Medium clay; Weak consistence; Common (10 - 20 %), Calcareous, , Soft segregations; 
	0.68 - 0.9 m	; Medium clay; Weak consistence; 
	0.9 - 1.2 m	; Medium clay; Common (10 - 20 %), Calcareous, , Soft segregations; 
	1.3 - 1.4 m	; Medium clay; 
	Morphological Notes
	Observation Notes
	SOMEWHAT SURFACE SEALED: 12-26CM WEAK CLAY SKINS: 26-35CM CLAY SKIN DISAPPEARING:                                  
	     
	Site Notes
	LOWAN

	Project Name:	Lowan, Vic.
	Project Code:	LO1	Site ID:	A933	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	7.1H	 0.043C
	0.04 - 0.12	7.6H	 0.09C
	0.12 - 0.26	7.9H	 0.18C
	0.26 - 0.35	8.3H	 0.44C
	0.35 - 0.55	8.8H	 1C
	0.55 - 0.68	8.8H	 1.5C
	0.68 - 0.9	8.8H	 1.5C
	0.9 - 1.2	8.9H	 1.4C
	1.3 - 1.4	8.8H	 1.3C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	 0.01C	 14C	 48	 11	 22
	0.04 - 0.12	 0.01C	 5C	 21	 8	 66
	0.12 - 0.26	 0.02C
	0.26 - 0.35	 0.03C	 2C	 9	 4	 85
	0.35 - 0.55	 1.3C
	0.55 - 0.68	 2.2C
	0.68 - 0.9	 4.1C	 1C	 7	 3	 85
	0.9 - 1.2	 4.5C
	1.3 - 1.4	 1C
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0.04 - 0.12
	0.12 - 0.26
	0.26 - 0.35
	0.35 - 0.55
	0.55 - 0.68
	0.68 - 0.9
	0.9 - 1.2
	1.3 - 1.4

	Project Name:	Lowan, Vic.
	Project Code:	LO1	Site ID:	A933	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded