Project Name:	NSF
	Project Code:	NSF	Site ID:	VP22	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Site Information
	Desc. By:	Locality:
	Date Desc.:	//	Elevation:	 52 metres
	Map Ref.:	Rainfall:	686
	Northing/Long.:	147.683333333333	Runoff:	No Data
	Easting/Lat.:	-37.93	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	N/A
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy5.42
	ASC Confidence:	Great Soil Group:	Solodic soil
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.2 m	Dark reddish brown (5YR3/2-Moist); ; Loamy sand; Single grain grade of structure; 
	A2cb	0.2 - 0.35 m	Very pale brown (10YR7/3-Moist); ; Loamy sand; Single grain grade of structure; 
	B1	0.35 - 0.5 m	Brownish yellow (10YR6/8-Moist); , 2.5Y62; Sandy medium clay; Moderate grade of structure; 
	B22	0.5 - 0.7 m	Yellowish brown (10YR5/8-Moist); , 2.5Y64; Medium clay; Moderate grade of structure; 
	B23	0.7 - 0.8 m	Yellowish brown (10YR5/8-Moist); , 5Y51; Medium clay; Moderate grade of structure; Few (2 - 10 
	%), Manganiferous, Medium (2 -6 mm), Nodules; 
	0.8 - 1.1 m	; 
	Morphological Notes
	Observation Notes
	V70/P24                                                                                                                 
	Site Notes
	BENGWORTH

	Project Name:	NSF
	Project Code:	NSF	Site ID:	VP22	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.5I	 0.11D	 2.1K	 0.52	 0.16	 0.28
	0.1 - 0.2	5.4I	 0.05D	 0.65K	 0.12	 0.01	 0.12
	0.2 - 0.3	5.9I	 0.06D	 0.7K	 0.67	 0.04	 0.67
	0.3 - 0.4	6.3I	 0.09D	 1.1K	 2.4	 0.08	 2.4
	0.4 - 0.5	6.5I	 0.16D	 2.1K	 7	 0.18	 7
	0.5 - 0.6	6.9I	 0.22D	 1.2K	 6.8	 0.17	 6.8
	0.6 - 0.7	7.1I	 0.27D	 0.89K	 7	 0.16	 7
	0.7 - 0.8	7.1I	 0.3D	 0.75K	 7	 0.14	 7
	0.8 - 0.9	7.4I	 0.37D	 0.82K	 7.4	 0.16	 7.4
	0.9 - 1	7.1I	 0.37D	 0.94K	 7.7	 0.18	 7.7
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.9A	 18A
	0.1 - 0.2	 0.39A	 6.7A
	0.2 - 0.3	 0.19A	 3.5A
	0.3 - 0.4	 0.23A	 1.5A
	0.4 - 0.5	 0.32A	 0.5A
	0.5 - 0.6	 0.25A	 0.5A
	0.6 - 0.7	 0.2A	 0.5A
	0.7 - 0.8	 0.26A	 0.4A
	0.8 - 0.9	 0.13A	 0.4A
	0.9 - 1	 0.14A	 0.4A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1

	Project Name:	NSF
	Project Code:	NSF	Site ID:	VP22	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (VIC)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	3_C_B	Electrical conductivity or soluble salts - Total soluble salts %
	4A_C_2.5	pH of soil - pH of 1:2.5 soil/water suspension
	5_C_B	Water soluble Chloride - Method recorded as B
	6A1	Organic carbon - Walkley and Black
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable